<?xml version="1.0"?>
<!DOCTYPE lmms-project>
<lmms-project version="1.0" creator="LMMS" creatorversion="1.2.0-rc2.80" type="instrumenttracksettings">
  <head/>
  <instrumenttracksettings muted="0" type="0" name="Dream" solo="0">
    <instrumenttrack pan="0" fxch="0" usemasterpitch="1" pitchrange="1" pitch="0" basenote="81" vol="31.9334">
      <instrument name="xpressive">
        <xpressive W3="randv(srate*t)" PAN1="0.07" PAN2="-0.05" W3sample="[encoded data, 21848 characters]" RELTRANS="50" version="0.1" A1="-0.28" A2="-0.45" O1="W1(integrate(f))*0.5" A3="0.0125002" O2="W2(integrate(f)*(1+A1/64)+W3(t/(t+1+A2)+A1)*t)-0.47(last(101+30*W1(0.2+t))+last(121+50*randv(1)+60*W1((1-t)^2)))sinew(integrate(f)/64)" interpolateW1="0" interpolateW2="0" W1sample="[encoded data, 21848 characters]" interpolateW3="0" smoothW1="56.6067" smoothW2="54.4192" smoothW3="70" W1="" W2="" W2sample="[encoded data, 21848 characters]"/>
      </instrument>
      <eldata fres="0.5" ftype="0" fcut="2921" fwet="1">
        <elvol lspd_denominator="4" sustain="0.621" pdel="0" userwavefile="" dec="0.354" lamt="0" latt="0" rel="0.466" amt="1" x100="0" att="0.012" lpdel="0" hold="0.238" lspd_syncmode="0" lshp="0" lspd="0.1" ctlenvamt="0" lspd_numerator="4"/>
        <elcut lspd_denominator="4" sustain="0.5" pdel="0" userwavefile="" dec="0.5" lamt="0" latt="0" rel="0.1" amt="0" x100="0" att="0" lpdel="0" hold="0.5" lspd_syncmode="0" lshp="0" lspd="0.1" ctlenvamt="0" lspd_numerator="4"/>
        <elres lspd_denominator="4" sustain="0.5" pdel="0" userwavefile="" dec="0.5" lamt="0" latt="0" rel="0.1" amt="0" x100="0" att="0" lpdel="0" hold="0.5" lspd_syncmode="0" lshp="0" lspd="0.1" ctlenvamt="0" lspd_numerator="4"/>
      </eldata>
      <chordcreator chord="0" chordrange="2" chord-enabled="0"/>
      <arpeggiator arptime="250" arprange="3" arpskip="0" arptime_denominator="4" arptime_syncmode="0" arpmode="2" arpcycle="0" arp-enabled="0" arp="3" arptime_numerator="4" arpdir="4" arpmiss="0" arpgate="77.4135"/>
      <midiport inputcontroller="0" fixedoutputvelocity="-1" inputchannel="0" outputcontroller="0" writable="0" outputchannel="1" fixedinputvelocity="-1" fixedoutputnote="-1" outputprogram="1" basevelocity="63" readable="0"/>
      <fxchain numofeffects="1" enabled="1">
        <effect autoquit_syncmode="0" autoquit_numerator="4" autoquit_denominator="4" autoquit="1" gate="0" name="ladspaeffect" wet="1" on="1">
          <ladspacontrols ports="4">
            <port02 data="0.711953"/>
            <port03 data="0.610435"/>
            <port04 data="0.276112"/>
            <port05 data="0.31"/>
          </ladspacontrols>
          <key>
            <attribute value="caps" name="file"/>
            <attribute value="Plate2x2" name="plugin"/>
          </key>
        </effect>
      </fxchain>
    </instrumenttrack>
  </instrumenttracksettings>
</lmms-project>
