<?xml version="1.0"?>
<!DOCTYPE lmms-project>
<lmms-project version="1.0" creator="LMMS" creatorversion="1.0.93" type="instrumenttracksettings">
  <head/>
  <instrumenttracksettings muted="0" type="0" name="Drone Arp" solo="0">
    <instrumenttrack pan="0" fxch="1" pitchrange="1" pitch="0" basenote="69" vol="100">
      <instrument name="lb302">
        <lb302 db24="1" vcf_res="0.37" vcf_dec="0.11" dead="0" vcf_cut="0.585" vcf_mod="0.33" dist="0.24" slide_dec="0.6" slide="0" shape="11"/>
      </instrument>
      <eldata fres="0.01" ftype="0" fcut="1681" fwet="0">
        <elvol lspd_denominator="4" sustain="0.5" pdel="0" userwavefile="" dec="0.5" lamt="0" syncmode="0" latt="0" rel="0.1" amt="1" x100="0" att="0" lpdel="0" hold="0.07" lshp="0" lspd="0.1" ctlenvamt="0" lspd_numerator="4"/>
        <elcut lspd_denominator="4" sustain="0.5" pdel="0" userwavefile="" dec="0.5" lamt="0" syncmode="0" latt="0" rel="0.1" amt="0" x100="0" att="0" lpdel="0" hold="0.5" lshp="0" lspd="0.1" ctlenvamt="0" lspd_numerator="4"/>
        <elres lspd_denominator="4" sustain="0.5" pdel="0" userwavefile="" dec="0.5" lamt="0" syncmode="0" latt="0" rel="0.1" amt="0" x100="0" att="0" lpdel="0" hold="0.5" lshp="0" lspd="0.1" ctlenvamt="0" lspd_numerator="4"/>
      </eldata>
      <chordcreator chord="0" chordrange="1" chord-enabled="0"/>
      <arpeggiator arptime="117" arprange="2" arptime_denominator="4" syncmode="6" arpmode="1" arp-enabled="1" arp="0" arptime_numerator="4" arpdir="2" arpgate="20"/>
      <midiport inputcontroller="0" inports="" fixedoutputvelocity="-1" inputchannel="0" outputcontroller="0" writable="0" outputchannel="1" fixedinputvelocity="-1" fixedoutputnote="-1" outputprogram="1" basevelocity="127" readable="0"/>
      <fxchain numofeffects="0" enabled="0"/>
    </instrumenttrack>
  </instrumenttracksettings>
</lmms-project>
