Description: Enable Coffee Lake support

Little change is needed here because the graphics core is the same as
Kaby Lake.  Includes all PCI IDs currently supported by the kernel driver
in the drm-intel tree (Coffee Lake S, H and U devices in GT 1, 2 and 3
configurations).

Origin: upstream 7e181af2ea4d37f67406f2563c0e13fa1fdbb14b
Author: Mark Thompson

--- a/backend/src/backend/gen_program.cpp
+++ b/backend/src/backend/gen_program.cpp
@@ -209,6 +209,8 @@ namespace gbe {
       ctx = GBE_NEW(BxtContext, unit, name, deviceID, relaxMath);
     } else if (IS_KABYLAKE(deviceID)) {
       ctx = GBE_NEW(KblContext, unit, name, deviceID, relaxMath);
+    } else if (IS_COFFEELAKE(deviceID)) {
+      ctx = GBE_NEW(KblContext, unit, name, deviceID, relaxMath);
     } else if (IS_GEMINILAKE(deviceID)) {
       ctx = GBE_NEW(GlkContext, unit, name, deviceID, relaxMath);
     }
@@ -328,6 +330,7 @@ namespace gbe {
                                       (IS_SKYLAKE(deviceID) && MATCH_SKL_HEADER(binary)) || \
                                       (IS_BROXTON(deviceID) && MATCH_BXT_HEADER(binary)) || \
                                       (IS_KABYLAKE(deviceID) && MATCH_KBL_HEADER(binary)) || \
+                                      (IS_COFFEELAKE(deviceID) && MATCH_KBL_HEADER(binary)) || \
                                       (IS_GEMINILAKE(deviceID) && MATCH_GLK_HEADER(binary)) \
                                       )
 
@@ -436,6 +439,8 @@ namespace gbe {
         FILL_BXT_HEADER(*binary);
       }else if(IS_KABYLAKE(prog->deviceID)){
         FILL_KBL_HEADER(*binary);
+      }else if(IS_COFFEELAKE(prog->deviceID)){
+        FILL_KBL_HEADER(*binary);
       }else if(IS_GEMINILAKE(prog->deviceID)){
         FILL_GLK_HEADER(*binary);
       }else {
--- a/src/cl_device_data.h
+++ b/src/cl_device_data.h
@@ -372,7 +372,59 @@
   (devid == PCI_CHIP_GLK_3x6 ||   \
    devid == PCI_CHIP_GLK_2x6)
 
-#define IS_GEN9(devid)     (IS_SKYLAKE(devid) || IS_BROXTON(devid) || IS_KABYLAKE(devid) || IS_GEMINILAKE(devid))
+#define PCI_CHIP_COFFEELAKE_S_GT1_1  0x3E90
+#define PCI_CHIP_COFFEELAKE_S_GT1_2  0x3E93
+#define PCI_CHIP_COFFEELAKE_S_GT1_3  0x3E99
+
+#define PCI_CHIP_COFFEELAKE_U_GT1_1  0x3EA1
+#define PCI_CHIP_COFFEELAKE_U_GT1_2  0x3EA4
+
+#define PCI_CHIP_COFFEELAKE_S_GT2_1  0x3E91
+#define PCI_CHIP_COFFEELAKE_S_GT2_2  0x3E92
+#define PCI_CHIP_COFFEELAKE_S_GT2_3  0x3E96
+#define PCI_CHIP_COFFEELAKE_S_GT2_4  0x3E9A
+
+#define PCI_CHIP_COFFEELAKE_H_GT2_1  0x3E94
+#define PCI_CHIP_COFFEELAKE_H_GT2_2  0x3E9B
+
+#define PCI_CHIP_COFFEELAKE_U_GT2_1  0x3EA0
+#define PCI_CHIP_COFFEELAKE_U_GT2_2  0x3EA3
+#define PCI_CHIP_COFFEELAKE_U_GT2_3  0x3EA9
+
+#define PCI_CHIP_COFFEELAKE_U_GT3_1  0x3EA2
+#define PCI_CHIP_COFFEELAKE_U_GT3_2  0x3EA5
+#define PCI_CHIP_COFFEELAKE_U_GT3_3  0x3EA6
+#define PCI_CHIP_COFFEELAKE_U_GT3_4  0x3EA7
+#define PCI_CHIP_COFFEELAKE_U_GT3_5  0x3EA8
+
+#define IS_CFL_GT1(devid) \
+    (devid == PCI_CHIP_COFFEELAKE_S_GT1_1 || \
+     devid == PCI_CHIP_COFFEELAKE_S_GT1_2 || \
+     devid == PCI_CHIP_COFFEELAKE_S_GT1_3 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT1_1 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT1_2)
+
+#define IS_CFL_GT2(devid) \
+    (devid == PCI_CHIP_COFFEELAKE_S_GT2_1 || \
+     devid == PCI_CHIP_COFFEELAKE_S_GT2_2 || \
+     devid == PCI_CHIP_COFFEELAKE_S_GT2_3 || \
+     devid == PCI_CHIP_COFFEELAKE_S_GT2_4 || \
+     devid == PCI_CHIP_COFFEELAKE_H_GT2_1 || \
+     devid == PCI_CHIP_COFFEELAKE_H_GT2_2 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT2_1 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT2_2 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT2_3)
+
+#define IS_CFL_GT3(devid) \
+    (devid == PCI_CHIP_COFFEELAKE_U_GT3_1 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT3_2 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT3_3 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT3_4 || \
+     devid == PCI_CHIP_COFFEELAKE_U_GT3_5)
+
+#define IS_COFFEELAKE(devid) (IS_CFL_GT1(devid) || IS_CFL_GT2(devid) || IS_CFL_GT3(devid))
+
+#define IS_GEN9(devid)     (IS_SKYLAKE(devid) || IS_BROXTON(devid) || IS_KABYLAKE(devid) || IS_GEMINILAKE(devid) || IS_COFFEELAKE(devid))
 
 #define MAX_OCLVERSION(devid) (IS_GEN9(devid) ? 200 : 120)
 
--- a/src/cl_device_id.c
+++ b/src/cl_device_id.c
@@ -274,6 +274,36 @@ static struct _cl_device_id intel_glk12eu_device = {
 #include "cl_gen9_device.h"
 };
 
+static struct _cl_device_id intel_cfl_gt1_device = {
+  .max_compute_unit = 12,
+  .max_thread_per_unit = 7,
+  .sub_slice_count = 2,
+  .max_work_item_sizes = {512, 512, 512},
+  .max_work_group_size = 256,
+  .max_clock_frequency = 1000,
+#include "cl_gen9_device.h"
+};
+
+static struct _cl_device_id intel_cfl_gt2_device = {
+  .max_compute_unit = 24,
+  .max_thread_per_unit = 7,
+  .sub_slice_count = 3,
+  .max_work_item_sizes = {512, 512, 512},
+  .max_work_group_size = 256,
+  .max_clock_frequency = 1000,
+#include "cl_gen9_device.h"
+};
+
+static struct _cl_device_id intel_cfl_gt3_device = {
+  .max_compute_unit = 48,
+  .max_thread_per_unit = 7,
+  .sub_slice_count = 6,
+  .max_work_item_sizes = {512, 512, 512},
+  .max_work_group_size = 256,
+  .max_clock_frequency = 1000,
+#include "cl_gen9_device.h"
+};
+
 LOCAL cl_device_id
 cl_get_gt_device(cl_device_type device_type)
 {
@@ -785,6 +815,64 @@ glk12eu_break:
       cl_intel_platform_enable_extension(ret, cl_khr_fp16_ext_id);
       break;
 
+    case PCI_CHIP_COFFEELAKE_S_GT1_1:
+    case PCI_CHIP_COFFEELAKE_S_GT1_2:
+    case PCI_CHIP_COFFEELAKE_S_GT1_3:
+      DECL_INFO_STRING(cfl_gt1_break, intel_cfl_gt1_device, name, "Intel(R) UHD Graphics Coffee Lake Desktop GT1");
+    case PCI_CHIP_COFFEELAKE_U_GT1_1:
+    case PCI_CHIP_COFFEELAKE_U_GT1_2:
+      DECL_INFO_STRING(cfl_gt1_break, intel_cfl_gt1_device, name, "Intel(R) UHD Graphics Coffee Lake Mobile GT1");
+cfl_gt1_break:
+      intel_cfl_gt1_device.device_id = device_id;
+      intel_cfl_gt1_device.platform = cl_get_platform_default();
+      ret = &intel_cfl_gt1_device;
+      cl_intel_platform_get_default_extension(ret);
+#ifdef ENABLE_FP64
+      cl_intel_platform_enable_extension(ret, cl_khr_fp64_ext_id);
+#endif
+      cl_intel_platform_enable_extension(ret, cl_khr_fp16_ext_id);
+      break;
+
+    case PCI_CHIP_COFFEELAKE_S_GT2_1:
+    case PCI_CHIP_COFFEELAKE_S_GT2_2:
+    case PCI_CHIP_COFFEELAKE_S_GT2_3:
+    case PCI_CHIP_COFFEELAKE_S_GT2_4:
+      DECL_INFO_STRING(cfl_gt2_break, intel_cfl_gt2_device, name, "Intel(R) UHD Graphics Coffee Lake Desktop GT2");
+    case PCI_CHIP_COFFEELAKE_H_GT2_1:
+    case PCI_CHIP_COFFEELAKE_H_GT2_2:
+      DECL_INFO_STRING(cfl_gt2_break, intel_cfl_gt2_device, name, "Intel(R) UHD Graphics Coffee Lake Halo GT2");
+    case PCI_CHIP_COFFEELAKE_U_GT2_1:
+    case PCI_CHIP_COFFEELAKE_U_GT2_2:
+    case PCI_CHIP_COFFEELAKE_U_GT2_3:
+      DECL_INFO_STRING(cfl_gt2_break, intel_cfl_gt2_device, name, "Intel(R) UHD Graphics Coffee Lake Mobile GT2");
+cfl_gt2_break:
+      intel_cfl_gt2_device.device_id = device_id;
+      intel_cfl_gt2_device.platform = cl_get_platform_default();
+      ret = &intel_cfl_gt2_device;
+      cl_intel_platform_get_default_extension(ret);
+#ifdef ENABLE_FP64
+      cl_intel_platform_enable_extension(ret, cl_khr_fp64_ext_id);
+#endif
+      cl_intel_platform_enable_extension(ret, cl_khr_fp16_ext_id);
+      break;
+
+    case PCI_CHIP_COFFEELAKE_U_GT3_1:
+    case PCI_CHIP_COFFEELAKE_U_GT3_2:
+    case PCI_CHIP_COFFEELAKE_U_GT3_3:
+    case PCI_CHIP_COFFEELAKE_U_GT3_4:
+    case PCI_CHIP_COFFEELAKE_U_GT3_5:
+      DECL_INFO_STRING(cfl_gt3_break, intel_cfl_gt3_device, name, "Intel(R) UHD Graphics Coffee Lake Mobile GT3");
+cfl_gt3_break:
+      intel_cfl_gt3_device.device_id = device_id;
+      intel_cfl_gt3_device.platform = cl_get_platform_default();
+      ret = &intel_cfl_gt3_device;
+      cl_intel_platform_get_default_extension(ret);
+#ifdef ENABLE_FP64
+      cl_intel_platform_enable_extension(ret, cl_khr_fp64_ext_id);
+#endif
+      cl_intel_platform_enable_extension(ret, cl_khr_fp16_ext_id);
+      break;
+
     case PCI_CHIP_SANDYBRIDGE_BRIDGE:
     case PCI_CHIP_SANDYBRIDGE_GT1:
     case PCI_CHIP_SANDYBRIDGE_GT2:
@@ -992,7 +1080,10 @@ LOCAL cl_bool is_gen_device(cl_device_id device) {
          device == &intel_kbl_gt3_device ||
          device == &intel_kbl_gt4_device ||
          device == &intel_glk18eu_device ||
-         device == &intel_glk12eu_device;
+         device == &intel_glk12eu_device ||
+         device == &intel_cfl_gt1_device ||
+         device == &intel_cfl_gt2_device ||
+         device == &intel_cfl_gt3_device;
 }
 
 LOCAL cl_int
@@ -1420,7 +1511,9 @@ cl_device_get_version(cl_device_id device, cl_int *ver)
         || device == &intel_bxt18eu_device || device == &intel_bxt12eu_device || device == &intel_kbl_gt1_device
         || device == &intel_kbl_gt2_device || device == &intel_kbl_gt3_device
         || device == &intel_kbl_gt4_device || device == &intel_kbl_gt15_device
-        || device == &intel_glk18eu_device || device == &intel_glk12eu_device) {
+        || device == &intel_glk18eu_device || device == &intel_glk12eu_device
+        || device == &intel_cfl_gt1_device || device == &intel_cfl_gt1_device
+        || device == &intel_cfl_gt3_device) {
     *ver = 9;
   } else
     return CL_INVALID_VALUE;
