From e79b0006c45c9b0b22f3ea54ff6e256b34c1f208 Mon Sep 17 00:00:00 2001
From: Megha Dey <megha.dey@intel.com>
Date: Wed, 14 Jun 2017 09:51:56 +0530
Subject: [PATCH] ALSA: hda - Add Coffelake PCI ID

Coffelake is another Intel part, so need to add PCI ID for it.

Signed-off-by: Megha Dey <megha.dey@intel.com>
Signed-off-by: Subhransu S. Prusty <subhransu.s.prusty@intel.com>
Acked-by: Vinod Koul <vinod.koul@intel.com>
Cc: <stable@vger.kernel.org>
Signed-off-by: Takashi Iwai <tiwai@suse.de>
---
 sound/pci/hda/hda_intel.c | 6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

diff --git a/sound/pci/hda/hda_intel.c b/sound/pci/hda/hda_intel.c
index 1770f085c2a6..e3c696c46a21 100644
--- a/sound/pci/hda/hda_intel.c
+++ b/sound/pci/hda/hda_intel.c
@@ -371,9 +371,10 @@ enum {
 #define IS_KBL_H(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0xa2f0)
 #define IS_BXT(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0x5a98)
 #define IS_GLK(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0x3198)
+#define IS_CFL(pci) ((pci)->vendor == 0x8086 && (pci)->device == 0xa348)
 #define IS_SKL_PLUS(pci) (IS_SKL(pci) || IS_SKL_LP(pci) || IS_BXT(pci)) || \
 			IS_KBL(pci) || IS_KBL_LP(pci) || IS_KBL_H(pci)	|| \
-			IS_GLK(pci)
+			IS_GLK(pci) || IS_CFL(pci)
 
 static char *driver_short_names[] = {
 	[AZX_DRIVER_ICH] = "HDA Intel",
@@ -2378,6 +2379,9 @@ static const struct pci_device_id azx_ids[] = {
 	/* Kabylake-H */
 	{ PCI_DEVICE(0x8086, 0xa2f0),
 	  .driver_data = AZX_DRIVER_PCH | AZX_DCAPS_INTEL_SKYLAKE },
+	/* Coffelake */
+	{ PCI_DEVICE(0x8086, 0xa348),
+	  .driver_data = AZX_DRIVER_PCH | AZX_DCAPS_INTEL_SKYLAKE},
 	/* Broxton-P(Apollolake) */
 	{ PCI_DEVICE(0x8086, 0x5a98),
 	  .driver_data = AZX_DRIVER_PCH | AZX_DCAPS_INTEL_BROXTON },
-- 
2.13.1

