#
# Local PCMCIA Configuration File
#
#----------------------------------------------------------------------
#
# System resources available for PCMCIA cards
#
# NOTE: these settings have no effect on resources assigned to a
# CardBus bridge device itself; this file only affects resources
# assigned to cards.  Also, interrupt settings here will only affect
# ISA bus interrupts assigned to 16-bit cards.  PCI interrupts
# generally can't be reconfigured.
#
# With the kernel PCMCIA subsystem, these settings also have no effect
# at all on resources used for 32-bit CardBus cards.  Those are set by
# the PCI hotplug subsystem.
#

# These are the official ports to use from pcmcia-cs:
#include port 0x100-0x4ff, port 0x800-0x8ff, port 0xc00-0xcff
# However, ports 0x810-0x81f hurt on some DELL machines and
# ports 0x3b0-0x3df hurt on some FSC machines, so we use this port
# list instead:

# v3.00 BK changed this line, recommendation from pakt...
#include port 0x100-0x3af, port 0x3e0-0x4ff, port 0x800-0x80f, port 0x820-0x8ff, port 0xc00-0xcff
include port 0x100-0x3af, port 0x3e0-0x4ff, port 0x820-0x8ff, port 0xc00-0xcff

include memory 0xc0000-0xfffff
include memory 0xa0000000-0xa0ffffff, memory 0x60000000-0x60ffffff

# High port numbers do not always work...
# include port 0x1000-0x17ff

# Extra port range for IBM Token Ring
include port 0xa00-0xaff

# Resources we should not use, even if they appear to be available

# First built-in serial port
exclude irq 4
# Second built-in serial port
#exclude irq 3
# First built-in parallel port
exclude irq 7

#----------------------------------------------------------------------

# Examples of options for loadable modules

# To fix sluggish network with IBM ethernet adapter...
#module "pcnet_cs" opts "mem_speed=600"

# Options for IBM Token Ring adapters
#module "ibmtr_cs" opts "mmiobase=0xd0000 srambase=0xd4000"

# Options for Raylink/WebGear driver: uncomment only one line...
# These are the default settings for use with the WebGear Windows driver:
#module "ray_cs" opts "essid=NETWORK_NAME hop_dwell=128 beacon_period=256 translate=0"
# Generic ad-hoc network
#module "ray_cs" opts "essid=ADHOC_ESSID hop_dwell=128 beacon_period=256 translate=1"
# Infrastructure network for older cards
#module "ray_cs" opts "net_type=1 essid=ESSID1"
# Infrastructure network for WebGear
#module "ray_cs" opts "net_type=1 essid=ESSID1 translate=1 hop_dwell=128 beacon_period=256"

# Options for WaveLAN/IEEE driver (AccessPoint mode)...
#module "wvlan_cs" opts "station_name=MY_PC"
# Options for WaveLAN/IEEE driver (ad-hoc mode)...
#module "wvlan_cs" opts "port_type=3 channel=1 station_name=MY_PC"

# Options for Xircom Netwave driver...
#module "netwave_cs" opts "domain=0x100 scramble_key=0x0"

