
 drivers/net/wireless/realtek/rtw88/Kconfig     |   47 +++++++++
 drivers/net/wireless/realtek/rtw88/Makefile    |   15 +++
 drivers/net/wireless/realtek/rtw88/coex.c      |    3 
 drivers/net/wireless/realtek/rtw88/debug.c     |   15 +++
 drivers/net/wireless/realtek/rtw88/fw.c        |   31 +++---
 drivers/net/wireless/realtek/rtw88/fw.h        |   11 ++
 drivers/net/wireless/realtek/rtw88/hci.h       |    9 -
 drivers/net/wireless/realtek/rtw88/mac.c       |   21 ++++
 drivers/net/wireless/realtek/rtw88/mac80211.c  |    2 
 drivers/net/wireless/realtek/rtw88/main.c      |   12 +-
 drivers/net/wireless/realtek/rtw88/main.h      |   12 +-
 drivers/net/wireless/realtek/rtw88/phy.c       |    6 -
 drivers/net/wireless/realtek/rtw88/ps.c        |    2 
 drivers/net/wireless/realtek/rtw88/reg.h       |    1 
 drivers/net/wireless/realtek/rtw88/rtw8723d.c  |   28 +++++
 drivers/net/wireless/realtek/rtw88/rtw8723d.h  |   13 ++
 drivers/net/wireless/realtek/rtw88/rtw8723du.c |   36 +++++++
 drivers/net/wireless/realtek/rtw88/rtw8821c.c  |   18 +++
 drivers/net/wireless/realtek/rtw88/rtw8821c.h  |   21 ++++
 drivers/net/wireless/realtek/rtw88/rtw8821cu.c |   50 ++++++++++
 drivers/net/wireless/realtek/rtw88/rtw8822b.c  |   19 +++
 drivers/net/wireless/realtek/rtw88/rtw8822bu.c |   90 ++++++++++++++++++
 drivers/net/wireless/realtek/rtw88/rtw8822c.c  |   24 ++++
 drivers/net/wireless/realtek/rtw88/rtw8822cu.c |   44 ++++++++
 drivers/net/wireless/realtek/rtw88/tx.h        |   31 ++++++
 drivers/net/wireless/realtek/rtw88/usb.c       |  911 +++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
 drivers/net/wireless/realtek/rtw88/usb.h       |  107 +++++++++++++++++++++
 drivers/net/wireless/realtek/rtw88/util.c      |  103 ++++++++++++++++++++
 drivers/net/wireless/realtek/rtw88/util.h      |   12 +-
 29 files changed, 1650 insertions(+), 44 deletions(-)

diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/coex.c linux-6.2/drivers/net/wireless/realtek/rtw88/coex.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/coex.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/coex.c	2022-12-24 00:49:25.771376835 +0200
@@ -633,7 +633,7 @@ static struct sk_buff *rtw_coex_info_req
 	struct rtw_coex *coex = &rtwdev->coex;
 	struct sk_buff *skb_resp = NULL;
 
-	mutex_lock(&coex->mutex);
+	lockdep_assert_held(&rtwdev->mutex);
 
 	rtw_fw_query_bt_mp_info(rtwdev, req);
 
@@ -650,7 +650,6 @@ static struct sk_buff *rtw_coex_info_req
 	}
 
 out:
-	mutex_unlock(&coex->mutex);
 	return skb_resp;
 }
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/debug.c linux-6.2/drivers/net/wireless/realtek/rtw88/debug.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/debug.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/debug.c	2022-12-24 00:49:25.771376835 +0200
@@ -144,7 +144,9 @@ static int rtw_debugfs_get_rf_read(struc
 	addr = debugfs_priv->rf_addr;
 	mask = debugfs_priv->rf_mask;
 
+	mutex_lock(&rtwdev->mutex);
 	val = rtw_read_rf(rtwdev, path, addr, mask);
+	mutex_unlock(&rtwdev->mutex);
 
 	seq_printf(m, "rf_read path:%d addr:0x%08x mask:0x%08x val=0x%08x\n",
 		   path, addr, mask, val);
@@ -390,7 +392,9 @@ static ssize_t rtw_debugfs_set_h2c(struc
 		return -EINVAL;
 	}
 
+	mutex_lock(&rtwdev->mutex);
 	rtw_fw_h2c_cmd_dbg(rtwdev, param);
+	mutex_unlock(&rtwdev->mutex);
 
 	return count;
 }
@@ -414,7 +418,9 @@ static ssize_t rtw_debugfs_set_rf_write(
 		return count;
 	}
 
+	mutex_lock(&rtwdev->mutex);
 	rtw_write_rf(rtwdev, path, addr, mask, val);
+	mutex_unlock(&rtwdev->mutex);
 	rtw_dbg(rtwdev, RTW_DBG_DEBUGFS,
 		"write_rf path:%d addr:0x%08x mask:0x%08x, val:0x%08x\n",
 		path, addr, mask, val);
@@ -519,6 +525,8 @@ static int rtw_debug_get_rf_dump(struct
 	u32 addr, offset, data;
 	u8 path;
 
+	mutex_lock(&rtwdev->mutex);
+
 	for (path = 0; path < rtwdev->hal.rf_path_num; path++) {
 		seq_printf(m, "RF path:%d\n", path);
 		for (addr = 0; addr < 0x100; addr += 4) {
@@ -533,6 +541,8 @@ static int rtw_debug_get_rf_dump(struct
 		seq_puts(m, "\n");
 	}
 
+	mutex_unlock(&rtwdev->mutex);
+
 	return 0;
 }
 
@@ -831,7 +841,9 @@ static int rtw_debugfs_get_coex_info(str
 	struct rtw_debugfs_priv *debugfs_priv = m->private;
 	struct rtw_dev *rtwdev = debugfs_priv->rtwdev;
 
+	mutex_lock(&rtwdev->mutex);
 	rtw_coex_display_coex_info(rtwdev, m);
+	mutex_unlock(&rtwdev->mutex);
 
 	return 0;
 }
@@ -1026,6 +1038,8 @@ static void dump_gapk_status(struct rtw_
 		   dm_info->dm_flags & BIT(RTW_DM_CAP_TXGAPK) ? '-' : '+',
 		   rtw_dm_cap_strs[RTW_DM_CAP_TXGAPK]);
 
+	mutex_lock(&rtwdev->mutex);
+
 	for (path = 0; path < rtwdev->hal.rf_path_num; path++) {
 		val = rtw_read_rf(rtwdev, path, RF_GAINTX, RFREG_MASK);
 		seq_printf(m, "path %d:\n0x%x = 0x%x\n", path, RF_GAINTX, val);
@@ -1035,6 +1049,7 @@ static void dump_gapk_status(struct rtw_
 				   txgapk->rf3f_fs[path][i], i);
 		seq_puts(m, "\n");
 	}
+	mutex_unlock(&rtwdev->mutex);
 }
 
 static int rtw_debugfs_get_dm_cap(struct seq_file *m, void *v)
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/fw.c linux-6.2/drivers/net/wireless/realtek/rtw88/fw.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/fw.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/fw.c	2022-12-24 00:49:25.771376835 +0200
@@ -311,10 +311,10 @@ EXPORT_SYMBOL(rtw_fw_c2h_cmd_isr);
 static void rtw_fw_send_h2c_command(struct rtw_dev *rtwdev,
 				    u8 *h2c)
 {
+	struct rtw_h2c_cmd *h2c_cmd = (struct rtw_h2c_cmd *)h2c;
 	u8 box;
 	u8 box_state;
 	u32 box_reg, box_ex_reg;
-	int idx;
 	int ret;
 
 	rtw_dbg(rtwdev, RTW_DBG_FW,
@@ -322,7 +322,7 @@ static void rtw_fw_send_h2c_command(stru
 		h2c[3], h2c[2], h2c[1], h2c[0],
 		h2c[7], h2c[6], h2c[5], h2c[4]);
 
-	spin_lock(&rtwdev->h2c.lock);
+	lockdep_assert_held(&rtwdev->mutex);
 
 	box = rtwdev->h2c.last_box_num;
 	switch (box) {
@@ -344,7 +344,7 @@ static void rtw_fw_send_h2c_command(stru
 		break;
 	default:
 		WARN(1, "invalid h2c mail box number\n");
-		goto out;
+		return;
 	}
 
 	ret = read_poll_timeout_atomic(rtw_read8, box_state,
@@ -353,19 +353,14 @@ static void rtw_fw_send_h2c_command(stru
 
 	if (ret) {
 		rtw_err(rtwdev, "failed to send h2c command\n");
-		goto out;
+		return;
 	}
 
-	for (idx = 0; idx < 4; idx++)
-		rtw_write8(rtwdev, box_reg + idx, h2c[idx]);
-	for (idx = 0; idx < 4; idx++)
-		rtw_write8(rtwdev, box_ex_reg + idx, h2c[idx + 4]);
+	rtw_write32(rtwdev, box_ex_reg, le32_to_cpu(h2c_cmd->msg_ext));
+	rtw_write32(rtwdev, box_reg, le32_to_cpu(h2c_cmd->msg));
 
 	if (++rtwdev->h2c.last_box_num >= 4)
 		rtwdev->h2c.last_box_num = 0;
-
-out:
-	spin_unlock(&rtwdev->h2c.lock);
 }
 
 void rtw_fw_h2c_cmd_dbg(struct rtw_dev *rtwdev, u8 *h2c)
@@ -377,15 +372,13 @@ static void rtw_fw_send_h2c_packet(struc
 {
 	int ret;
 
-	spin_lock(&rtwdev->h2c.lock);
+	lockdep_assert_held(&rtwdev->mutex);
 
 	FW_OFFLOAD_H2C_SET_SEQ_NUM(h2c_pkt, rtwdev->h2c.seq);
 	ret = rtw_hci_write_data_h2c(rtwdev, h2c_pkt, H2C_PKT_SIZE);
 	if (ret)
 		rtw_err(rtwdev, "failed to send h2c packet\n");
 	rtwdev->h2c.seq++;
-
-	spin_unlock(&rtwdev->h2c.lock);
 }
 
 void
@@ -823,6 +816,16 @@ void rtw_fw_set_nlo_info(struct rtw_dev
 
 	rtw_fw_send_h2c_command(rtwdev, h2c_pkt);
 }
+
+void rtw_fw_set_recover_bt_device(struct rtw_dev *rtwdev)
+{
+	u8 h2c_pkt[H2C_PKT_SIZE] = {0};
+
+	SET_H2C_CMD_ID_CLASS(h2c_pkt, H2C_CMD_RECOVER_BT_DEV);
+	SET_RECOVER_BT_DEV_EN(h2c_pkt, 1);
+
+	rtw_fw_send_h2c_command(rtwdev, h2c_pkt);
+}
 
 void rtw_fw_set_pg_info(struct rtw_dev *rtwdev)
 {
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/fw.h linux-6.2/drivers/net/wireless/realtek/rtw88/fw.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/fw.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/fw.h	2022-12-24 00:49:25.771376835 +0200
@@ -81,6 +81,11 @@ struct rtw_c2h_adaptivity {
 	u8 option;
 } __packed;
 
+struct rtw_h2c_cmd {
+	__le32 msg;
+	__le32 msg_ext;
+} __packed;
+
 enum rtw_rsvd_packet_type {
 	RSVD_BEACON,
 	RSVD_DUMMY,
@@ -550,6 +555,8 @@ static inline void rtw_h2c_pkt_set_heade
 #define H2C_CMD_AOAC_GLOBAL_INFO	0x82
 #define H2C_CMD_NLO_INFO		0x8C
 
+#define H2C_CMD_RECOVER_BT_DEV		0xD1
+
 #define SET_H2C_CMD_ID_CLASS(h2c_pkt, value)				       \
 	le32p_replace_bits((__le32 *)(h2c_pkt) + 0x00, value, GENMASK(7, 0))
 
@@ -749,6 +756,9 @@ static inline void rtw_h2c_pkt_set_heade
 #define SET_NLO_LOC_NLO_INFO(h2c_pkt, value)                                   \
 	le32p_replace_bits((__le32 *)(h2c_pkt) + 0x00, value, GENMASK(23, 16))
 
+#define SET_RECOVER_BT_DEV_EN(h2c_pkt, value)				       \
+	le32p_replace_bits((__le32 *)(h2c_pkt) + 0x00, value, BIT(8))
+
 #define GET_FW_DUMP_LEN(_header)					\
 	le32_get_bits(*((__le32 *)(_header) + 0x00), GENMASK(15, 0))
 #define GET_FW_DUMP_SEQ(_header)					\
@@ -838,6 +848,7 @@ void rtw_fw_set_aoac_global_info_cmd(str
 				     u8 group_key_enc);
 
 void rtw_fw_set_nlo_info(struct rtw_dev *rtwdev, bool enable);
+void rtw_fw_set_recover_bt_device(struct rtw_dev *rtwdev);
 void rtw_fw_update_pkt_probe_req(struct rtw_dev *rtwdev,
 				 struct cfg80211_ssid *ssid);
 void rtw_fw_channel_switch(struct rtw_dev *rtwdev, bool enable);
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/hci.h linux-6.2/drivers/net/wireless/realtek/rtw88/hci.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/hci.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/hci.h	2022-12-24 00:49:25.771376835 +0200
@@ -166,12 +166,11 @@ static inline u32
 rtw_read_rf(struct rtw_dev *rtwdev, enum rtw_rf_path rf_path,
 	    u32 addr, u32 mask)
 {
-	unsigned long flags;
 	u32 val;
 
-	spin_lock_irqsave(&rtwdev->rf_lock, flags);
+	lockdep_assert_held(&rtwdev->mutex);
+
 	val = rtwdev->chip->ops->read_rf(rtwdev, rf_path, addr, mask);
-	spin_unlock_irqrestore(&rtwdev->rf_lock, flags);
 
 	return val;
 }
@@ -180,11 +179,9 @@ static inline void
 rtw_write_rf(struct rtw_dev *rtwdev, enum rtw_rf_path rf_path,
 	     u32 addr, u32 mask, u32 data)
 {
-	unsigned long flags;
+	lockdep_assert_held(&rtwdev->mutex);
 
-	spin_lock_irqsave(&rtwdev->rf_lock, flags);
 	rtwdev->chip->ops->write_rf(rtwdev, rf_path, addr, mask, data);
-	spin_unlock_irqrestore(&rtwdev->rf_lock, flags);
 }
 
 static inline u32
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/Kconfig linux-6.2/drivers/net/wireless/realtek/rtw88/Kconfig
--- linux-6.1/drivers/net/wireless/realtek/rtw88/Kconfig	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/Kconfig	2022-12-24 00:49:25.770376835 +0200
@@ -16,6 +16,9 @@ config RTW88_CORE
 config RTW88_PCI
 	tristate
 
+config RTW88_USB
+	tristate
+
 config RTW88_8822B
 	tristate
 
@@ -39,6 +42,17 @@ config RTW88_8822BE
 
 	  802.11ac PCIe wireless network adapter
 
+config RTW88_8822BU
+	tristate "Realtek 8822BU USB wireless network adapter"
+	depends on USB
+	select RTW88_CORE
+	select RTW88_USB
+	select RTW88_8822B
+	help
+	  Select this option will enable support for 8822BU chipset
+
+	  802.11ac USB wireless network adapter
+
 config RTW88_8822CE
 	tristate "Realtek 8822CE PCI wireless network adapter"
 	depends on PCI
@@ -50,6 +64,17 @@ config RTW88_8822CE
 
 	  802.11ac PCIe wireless network adapter
 
+config RTW88_8822CU
+	tristate "Realtek 8822CU USB wireless network adapter"
+	depends on USB
+	select RTW88_CORE
+	select RTW88_USB
+	select RTW88_8822C
+	help
+	  Select this option will enable support for 8822CU chipset
+
+	  802.11ac USB wireless network adapter
+
 config RTW88_8723DE
 	tristate "Realtek 8723DE PCI wireless network adapter"
 	depends on PCI
@@ -61,6 +86,17 @@ config RTW88_8723DE
 
 	  802.11n PCIe wireless network adapter
 
+config RTW88_8723DU
+	tristate "Realtek 8723DU USB wireless network adapter"
+	depends on USB
+	select RTW88_CORE
+	select RTW88_USB
+	select RTW88_8723D
+	help
+	  Select this option will enable support for 8723DU chipset
+
+	  802.11n USB wireless network adapter
+
 config RTW88_8821CE
 	tristate "Realtek 8821CE PCI wireless network adapter"
 	depends on PCI
@@ -72,6 +108,17 @@ config RTW88_8821CE
 
 	  802.11ac PCIe wireless network adapter
 
+config RTW88_8821CU
+	tristate "Realtek 8821CU USB wireless network adapter"
+	depends on USB
+	select RTW88_CORE
+	select RTW88_USB
+	select RTW88_8821C
+	help
+	  Select this option will enable support for 8821CU chipset
+
+	  802.11ac USB wireless network adapter
+
 config RTW88_DEBUG
 	bool "Realtek rtw88 debug support"
 	depends on RTW88_CORE
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/mac80211.c linux-6.2/drivers/net/wireless/realtek/rtw88/mac80211.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/mac80211.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/mac80211.c	2022-12-24 00:49:25.772376835 +0200
@@ -487,8 +487,8 @@ static int rtw_ops_sta_remove(struct iee
 {
 	struct rtw_dev *rtwdev = hw->priv;
 
-	rtw_fw_beacon_filter_config(rtwdev, false, vif);
 	mutex_lock(&rtwdev->mutex);
+	rtw_fw_beacon_filter_config(rtwdev, false, vif);
 	rtw_sta_remove(rtwdev, sta, true);
 	mutex_unlock(&rtwdev->mutex);
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/mac.c linux-6.2/drivers/net/wireless/realtek/rtw88/mac.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/mac.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/mac.c	2022-12-24 00:49:25.772376835 +0200
@@ -906,7 +906,8 @@ out:
 	return ret;
 }
 
-int rtw_download_firmware(struct rtw_dev *rtwdev, struct rtw_fw_state *fw)
+static
+int _rtw_download_firmware(struct rtw_dev *rtwdev, struct rtw_fw_state *fw)
 {
 	if (rtw_chip_wcpu_11n(rtwdev))
 		return __rtw_download_firmware_legacy(rtwdev, fw);
@@ -914,6 +915,21 @@ int rtw_download_firmware(struct rtw_dev
 	return __rtw_download_firmware(rtwdev, fw);
 }
 
+int rtw_download_firmware(struct rtw_dev *rtwdev, struct rtw_fw_state *fw)
+{
+	int ret;
+
+	ret = _rtw_download_firmware(rtwdev, fw);
+	if (ret)
+		return ret;
+
+	if (rtw_hci_type(rtwdev) == RTW_HCI_TYPE_PCIE &&
+	    rtwdev->chip->id == RTW_CHIP_TYPE_8821C)
+		rtw_fw_set_recover_bt_device(rtwdev);
+
+	return 0;
+}
+
 static u32 get_priority_queues(struct rtw_dev *rtwdev, u32 queues)
 {
 	const struct rtw_rqpn *rqpn = rtwdev->fifo.rqpn;
@@ -1032,6 +1048,9 @@ static int txdma_queue_mapping(struct rt
 	if (rtw_chip_wcpu_11ac(rtwdev))
 		rtw_write32(rtwdev, REG_H2CQ_CSR, BIT_H2CQ_FULL);
 
+	if (rtw_hci_type(rtwdev) == RTW_HCI_TYPE_USB)
+		rtw_write8_set(rtwdev, REG_TXDMA_PQ_MAP, BIT_RXDMA_ARBBW_EN);
+
 	return 0;
 }
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/main.c linux-6.2/drivers/net/wireless/realtek/rtw88/main.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/main.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/main.c	2022-12-24 00:49:25.772376835 +0200
@@ -1731,7 +1731,8 @@ static void rtw_load_firmware_cb(const s
 	update_firmware_info(rtwdev, fw);
 	complete_all(&fw->completion);
 
-	rtw_info(rtwdev, "Firmware version %u.%u.%u, H2C version %u\n",
+	rtw_info(rtwdev, "%sFirmware version %u.%u.%u, H2C version %u\n",
+		 fw->type == RTW_WOWLAN_FW ? "WOW " : "",
 		 fw->version, fw->sub_version, fw->sub_index, fw->h2c_version);
 }
 
@@ -1757,6 +1758,7 @@ static int rtw_load_firmware(struct rtw_
 		return -ENOENT;
 	}
 
+	fw->type = type;
 	fw->rtwdev = rtwdev;
 	init_completion(&fw->completion);
 
@@ -1781,6 +1783,10 @@ static int rtw_chip_parameter_setup(stru
 		rtwdev->hci.rpwm_addr = 0x03d9;
 		rtwdev->hci.cpwm_addr = 0x03da;
 		break;
+	case RTW_HCI_TYPE_USB:
+		rtwdev->hci.rpwm_addr = 0xfe58;
+		rtwdev->hci.cpwm_addr = 0xfe57;
+		break;
 	default:
 		rtw_err(rtwdev, "unsupported hci type\n");
 		return -EINVAL;
@@ -2065,13 +2071,10 @@ int rtw_core_init(struct rtw_dev *rtwdev
 	skb_queue_head_init(&rtwdev->coex.queue);
 	skb_queue_head_init(&rtwdev->tx_report.queue);
 
-	spin_lock_init(&rtwdev->rf_lock);
-	spin_lock_init(&rtwdev->h2c.lock);
 	spin_lock_init(&rtwdev->txq_lock);
 	spin_lock_init(&rtwdev->tx_report.q_lock);
 
 	mutex_init(&rtwdev->mutex);
-	mutex_init(&rtwdev->coex.mutex);
 	mutex_init(&rtwdev->hal.tx_power_mutex);
 
 	init_waitqueue_head(&rtwdev->coex.wait);
@@ -2143,7 +2146,6 @@ void rtw_core_deinit(struct rtw_dev *rtw
 	}
 
 	mutex_destroy(&rtwdev->mutex);
-	mutex_destroy(&rtwdev->coex.mutex);
 	mutex_destroy(&rtwdev->hal.tx_power_mutex);
 }
 EXPORT_SYMBOL(rtw_core_deinit);
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/main.h linux-6.2/drivers/net/wireless/realtek/rtw88/main.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/main.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/main.h	2022-12-24 00:49:25.773376835 +0200
@@ -871,6 +871,10 @@ struct rtw_chip_ops {
 			       bool is_tx2_path);
 	void (*config_txrx_mode)(struct rtw_dev *rtwdev, u8 tx_path,
 				 u8 rx_path, bool is_tx2_path);
+	/* for USB/SDIO only */
+	void (*fill_txdesc_checksum)(struct rtw_dev *rtwdev,
+				     struct rtw_tx_pkt_info *pkt_info,
+				     u8 *txdesc);
 
 	/* for coex */
 	void (*coex_set_init)(struct rtw_dev *rtwdev);
@@ -1501,8 +1505,6 @@ struct rtw_coex_stat {
 };
 
 struct rtw_coex {
-	/* protects coex info request section */
-	struct mutex mutex;
 	struct sk_buff_head queue;
 	wait_queue_head_t wait;
 
@@ -1851,6 +1853,7 @@ struct rtw_fw_state {
 	u16 h2c_version;
 	u32 feature;
 	u32 feature_ext;
+	enum rtw_fw_type type;
 };
 
 enum rtw_sar_sources {
@@ -1994,9 +1997,6 @@ struct rtw_dev {
 	/* ensures exclusive access from mac80211 callbacks */
 	struct mutex mutex;
 
-	/* read/write rf register */
-	spinlock_t rf_lock;
-
 	/* watch dog every 2 sec */
 	struct delayed_work watch_dog_work;
 	u32 watch_dog_cnt;
@@ -2022,8 +2022,6 @@ struct rtw_dev {
 	struct {
 		/* incicate the mail box to use with fw */
 		u8 last_box_num;
-		/* protect to send h2c to fw */
-		spinlock_t lock;
 		u32 seq;
 	} h2c;
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/Makefile linux-6.2/drivers/net/wireless/realtek/rtw88/Makefile
--- linux-6.1/drivers/net/wireless/realtek/rtw88/Makefile	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/Makefile	2022-12-24 00:49:25.770376835 +0200
@@ -26,23 +26,38 @@ rtw88_8822b-objs		:= rtw8822b.o rtw8822b
 obj-$(CONFIG_RTW88_8822BE)	+= rtw88_8822be.o
 rtw88_8822be-objs		:= rtw8822be.o
 
+obj-$(CONFIG_RTW88_8822BU)	+= rtw88_8822bu.o
+rtw88_8822bu-objs		:= rtw8822bu.o
+
 obj-$(CONFIG_RTW88_8822C)	+= rtw88_8822c.o
 rtw88_8822c-objs		:= rtw8822c.o rtw8822c_table.o
 
 obj-$(CONFIG_RTW88_8822CE)	+= rtw88_8822ce.o
 rtw88_8822ce-objs		:= rtw8822ce.o
 
+obj-$(CONFIG_RTW88_8822CU)	+= rtw88_8822cu.o
+rtw88_8822cu-objs		:= rtw8822cu.o
+
 obj-$(CONFIG_RTW88_8723D)	+= rtw88_8723d.o
 rtw88_8723d-objs		:= rtw8723d.o rtw8723d_table.o
 
 obj-$(CONFIG_RTW88_8723DE)	+= rtw88_8723de.o
 rtw88_8723de-objs		:= rtw8723de.o
 
+obj-$(CONFIG_RTW88_8723DU)	+= rtw88_8723du.o
+rtw88_8723du-objs		:= rtw8723du.o
+
 obj-$(CONFIG_RTW88_8821C)	+= rtw88_8821c.o
 rtw88_8821c-objs		:= rtw8821c.o rtw8821c_table.o
 
 obj-$(CONFIG_RTW88_8821CE)	+= rtw88_8821ce.o
 rtw88_8821ce-objs		:= rtw8821ce.o
 
+obj-$(CONFIG_RTW88_8821CU)	+= rtw88_8821cu.o
+rtw88_8821cu-objs		:= rtw8821cu.o
+
 obj-$(CONFIG_RTW88_PCI)		+= rtw88_pci.o
 rtw88_pci-objs			:= pci.o
+
+obj-$(CONFIG_RTW88_USB)		+= rtw88_usb.o
+rtw88_usb-objs			:= usb.o
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/phy.c linux-6.2/drivers/net/wireless/realtek/rtw88/phy.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/phy.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/phy.c	2022-12-24 00:49:25.773376835 +0200
@@ -300,7 +300,7 @@ static void rtw_phy_stat_rssi(struct rtw
 
 	data.rtwdev = rtwdev;
 	data.min_rssi = U8_MAX;
-	rtw_iterate_stas_atomic(rtwdev, rtw_phy_stat_rssi_iter, &data);
+	rtw_iterate_stas(rtwdev, rtw_phy_stat_rssi_iter, &data);
 
 	dm_info->pre_min_rssi = dm_info->min_rssi;
 	dm_info->min_rssi = data.min_rssi;
@@ -544,7 +544,7 @@ static void rtw_phy_ra_info_update(struc
 	if (rtwdev->watch_dog_cnt & 0x3)
 		return;
 
-	rtw_iterate_stas_atomic(rtwdev, rtw_phy_ra_info_update_iter, rtwdev);
+	rtw_iterate_stas(rtwdev, rtw_phy_ra_info_update_iter, rtwdev);
 }
 
 static u32 rtw_phy_get_rrsr_mask(struct rtw_dev *rtwdev, u8 rate_idx)
@@ -597,7 +597,7 @@ static void rtw_phy_rrsr_update(struct r
 	struct rtw_dm_info *dm_info = &rtwdev->dm_info;
 
 	dm_info->rrsr_mask_min = RRSR_RATE_ORDER_MAX;
-	rtw_iterate_stas_atomic(rtwdev, rtw_phy_rrsr_mask_min_iter, rtwdev);
+	rtw_iterate_stas(rtwdev, rtw_phy_rrsr_mask_min_iter, rtwdev);
 	rtw_write32(rtwdev, REG_RRSR, dm_info->rrsr_val_init & dm_info->rrsr_mask_min);
 }
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/ps.c linux-6.2/drivers/net/wireless/realtek/rtw88/ps.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/ps.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/ps.c	2022-12-24 00:49:25.773376835 +0200
@@ -61,7 +61,7 @@ int rtw_leave_ips(struct rtw_dev *rtwdev
 		return ret;
 	}
 
-	rtw_iterate_vifs_atomic(rtwdev, rtw_restore_port_cfg_iter, rtwdev);
+	rtw_iterate_vifs(rtwdev, rtw_restore_port_cfg_iter, rtwdev);
 
 	rtw_coex_ips_notify(rtwdev, COEX_IPS_LEAVE);
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/reg.h linux-6.2/drivers/net/wireless/realtek/rtw88/reg.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/reg.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/reg.h	2022-12-24 00:49:25.773376835 +0200
@@ -184,6 +184,7 @@
 #define BIT_TXDMA_VIQ_MAP(x)                                                   \
 	(((x) & BIT_MASK_TXDMA_VIQ_MAP) << BIT_SHIFT_TXDMA_VIQ_MAP)
 #define REG_TXDMA_PQ_MAP	0x010C
+#define BIT_RXDMA_ARBBW_EN	BIT(0)
 #define BIT_SHIFT_TXDMA_BEQ_MAP	8
 #define BIT_MASK_TXDMA_BEQ_MAP	0x3
 #define BIT_TXDMA_BEQ_MAP(x)                                                   \
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8723d.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8723d.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8723d.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8723d.c	2022-12-24 00:49:25.773376835 +0200
@@ -210,6 +210,12 @@ static void rtw8723de_efuse_parsing(stru
 	ether_addr_copy(efuse->addr, map->e.mac_addr);
 }
 
+static void rtw8723du_efuse_parsing(struct rtw_efuse *efuse,
+				    struct rtw8723d_efuse *map)
+{
+	ether_addr_copy(efuse->addr, map->u.mac_addr);
+}
+
 static int rtw8723d_read_efuse(struct rtw_dev *rtwdev, u8 *log_map)
 {
 	struct rtw_efuse *efuse = &rtwdev->efuse;
@@ -239,6 +245,9 @@ static int rtw8723d_read_efuse(struct rt
 	case RTW_HCI_TYPE_PCIE:
 		rtw8723de_efuse_parsing(efuse, map);
 		break;
+	case RTW_HCI_TYPE_USB:
+		rtw8723du_efuse_parsing(efuse, map);
+		break;
 	default:
 		/* unsupported now */
 		return -ENOTSUPP;
@@ -1945,6 +1954,24 @@ static void rtw8723d_pwr_track(struct rt
 	dm_info->pwr_trk_triggered = false;
 }
 
+static void rtw8723d_fill_txdesc_checksum(struct rtw_dev *rtwdev,
+					  struct rtw_tx_pkt_info *pkt_info,
+					  u8 *txdesc)
+{
+	size_t words = 32 / 2; /* calculate the first 32 bytes (16 words) */
+	__le16 chksum = 0;
+	__le16 *data = (__le16 *)(txdesc);
+
+	SET_TX_DESC_TXDESC_CHECKSUM(txdesc, 0x0000);
+
+	while (words--)
+		chksum ^= *data++;
+
+	chksum = ~chksum;
+
+	SET_TX_DESC_TXDESC_CHECKSUM(txdesc, __le16_to_cpu(chksum));
+}
+
 static struct rtw_chip_ops rtw8723d_ops = {
 	.phy_set_param		= rtw8723d_phy_set_param,
 	.read_efuse		= rtw8723d_read_efuse,
@@ -1965,6 +1992,7 @@ static struct rtw_chip_ops rtw8723d_ops
 	.config_bfee		= NULL,
 	.set_gid_table		= NULL,
 	.cfg_csi_rate		= NULL,
+	.fill_txdesc_checksum	= rtw8723d_fill_txdesc_checksum,
 
 	.coex_set_init		= rtw8723d_coex_cfg_init,
 	.coex_set_ant_switch	= NULL,
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8723d.h linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8723d.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8723d.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8723d.h	2022-12-24 00:49:25.773376835 +0200
@@ -41,6 +41,14 @@ struct rtw8723de_efuse {
 	u8 sub_device_id[2];
 };
 
+struct rtw8723du_efuse {
+	u8 res4[48];                    /* 0xd0 */
+	u8 vender_id[2];                /* 0x100 */
+	u8 product_id[2];               /* 0x102 */
+	u8 usb_option;                  /* 0x104 */
+	u8 mac_addr[ETH_ALEN];          /* 0x107 */
+};
+
 struct rtw8723d_efuse {
 	__le16 rtl_id;
 	u8 rsvd[2];
@@ -69,7 +77,10 @@ struct rtw8723d_efuse {
 	u8 rfe_option;
 	u8 country_code[2];
 	u8 res[3];
-	struct rtw8723de_efuse e;
+	union {
+		struct rtw8723de_efuse e;
+		struct rtw8723du_efuse u;
+	};
 };
 
 extern const struct rtw_chip_info rtw8723d_hw_spec;
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8723du.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8723du.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8723du.c	1970-01-01 02:00:00.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8723du.c	2022-12-24 00:49:25.773376835 +0200
@@ -0,0 +1,36 @@
+// SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#include <linux/module.h>
+#include <linux/usb.h>
+#include "main.h"
+#include "rtw8723d.h"
+#include "usb.h"
+
+static const struct usb_device_id rtw_8723du_id_table[] = {
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xd723, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8723d_hw_spec) }, /* 8723DU 1*1 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x7392, 0xd611, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8723d_hw_spec) }, /* Edimax EW-7611ULB V2 */
+	{ },
+};
+MODULE_DEVICE_TABLE(usb, rtw_8723du_id_table);
+
+static int rtw8723du_probe(struct usb_interface *intf,
+			   const struct usb_device_id *id)
+{
+	return rtw_usb_probe(intf, id);
+}
+
+static struct usb_driver rtw_8723du_driver = {
+	.name = "rtw_8723du",
+	.id_table = rtw_8723du_id_table,
+	.probe = rtw8723du_probe,
+	.disconnect = rtw_usb_disconnect,
+};
+module_usb_driver(rtw_8723du_driver);
+
+MODULE_AUTHOR("Hans Ulli Kroll <linux@ulli-kroll.de>");
+MODULE_DESCRIPTION("Realtek 802.11n wireless 8723du driver");
+MODULE_LICENSE("Dual BSD/GPL");
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8821c.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8821c.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8821c.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8821c.c	2022-12-24 00:49:25.774376835 +0200
@@ -26,6 +26,12 @@ static void rtw8821ce_efuse_parsing(stru
 	ether_addr_copy(efuse->addr, map->e.mac_addr);
 }
 
+static void rtw8821cu_efuse_parsing(struct rtw_efuse *efuse,
+				    struct rtw8821c_efuse *map)
+{
+	ether_addr_copy(efuse->addr, map->u.mac_addr);
+}
+
 enum rtw8821ce_rf_set {
 	SWITCH_TO_BTG,
 	SWITCH_TO_WLG,
@@ -68,6 +74,9 @@ static int rtw8821c_read_efuse(struct rt
 	case RTW_HCI_TYPE_PCIE:
 		rtw8821ce_efuse_parsing(efuse, map);
 		break;
+	case RTW_HCI_TYPE_USB:
+		rtw8821cu_efuse_parsing(efuse, map);
+		break;
 	default:
 		/* unsupported now */
 		return -ENOTSUPP;
@@ -1148,6 +1157,13 @@ static void rtw8821c_phy_cck_pd_set(stru
 			 dm_info->cck_pd_default + new_lvl * 2);
 }
 
+static void rtw8821c_fill_txdesc_checksum(struct rtw_dev *rtwdev,
+					  struct rtw_tx_pkt_info *pkt_info,
+					  u8 *txdesc)
+{
+	fill_txdesc_checksum_common(txdesc, 16);
+}
+
 static struct rtw_pwr_seq_cmd trans_carddis_to_cardemu_8821c[] = {
 	{0x0086,
 	 RTW_PWR_CUT_ALL_MSK,
@@ -1521,6 +1537,7 @@ static const struct rtw_rfe_def rtw8821c
 	[2] = RTW_DEF_RFE_EXT(8821c, 0, 0, 2),
 	[4] = RTW_DEF_RFE_EXT(8821c, 0, 0, 2),
 	[6] = RTW_DEF_RFE(8821c, 0, 0),
+	[34] = RTW_DEF_RFE(8821c, 0, 0),
 };
 
 static struct rtw_hw_reg rtw8821c_dig[] = {
@@ -1595,6 +1612,7 @@ static struct rtw_chip_ops rtw8821c_ops
 	.config_bfee		= rtw8821c_bf_config_bfee,
 	.set_gid_table		= rtw_bf_set_gid_table,
 	.cfg_csi_rate		= rtw_bf_cfg_csi_rate,
+	.fill_txdesc_checksum	= rtw8821c_fill_txdesc_checksum,
 
 	.coex_set_init		= rtw8821c_coex_cfg_init,
 	.coex_set_ant_switch	= rtw8821c_coex_cfg_ant_switch,
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8821c.h linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8821c.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8821c.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8821c.h	2022-12-24 00:49:25.774376835 +0200
@@ -9,6 +9,26 @@
 
 #define RCR_VHT_ACK		BIT(26)
 
+struct rtw8821cu_efuse {
+	u8 res4[4];			/* 0xd0 */
+	u8 usb_optional_function;
+	u8 res5[0x1e];
+	u8 res6[2];
+	u8 serial[0x0b];		/* 0xf5 */
+	u8 vid;				/* 0x100 */
+	u8 res7;
+	u8 pid;
+	u8 res8[4];
+	u8 mac_addr[ETH_ALEN];		/* 0x107 */
+	u8 res9[2];
+	u8 vendor_name[0x07];
+	u8 res10[2];
+	u8 device_name[0x14];
+	u8 res11[0xcf];
+	u8 package_type;		/* 0x1fb */
+	u8 res12[0x4];
+};
+
 struct rtw8821ce_efuse {
 	u8 mac_addr[ETH_ALEN];		/* 0xd0 */
 	u8 vender_id[2];
@@ -73,6 +93,7 @@ struct rtw8821c_efuse {
 	u8 res[3];
 	union {
 		struct rtw8821ce_efuse e;
+		struct rtw8821cu_efuse u;
 	};
 };
 
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8821cu.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8821cu.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8821cu.c	1970-01-01 02:00:00.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8821cu.c	2022-12-24 00:49:25.774376835 +0200
@@ -0,0 +1,50 @@
+// SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#include <linux/module.h>
+#include <linux/usb.h>
+#include "main.h"
+#include "rtw8821c.h"
+#include "usb.h"
+
+static const struct usb_device_id rtw_8821cu_id_table[] = {
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xb82b, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8821CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xb820, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8821CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc821, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8821CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc820, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8821CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc82a, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8821CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc82b, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8821CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc811, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8811CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0x8811, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* 8811CU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0x2006, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8821c_hw_spec) }, /* TOTOLINK A650UA v3 */
+	{},
+};
+MODULE_DEVICE_TABLE(usb, rtw_8821cu_id_table);
+
+static int rtw_8821cu_probe(struct usb_interface *intf,
+			    const struct usb_device_id *id)
+{
+	return rtw_usb_probe(intf, id);
+}
+
+static struct usb_driver rtw_8821cu_driver = {
+	.name = "rtw_8821cu",
+	.id_table = rtw_8821cu_id_table,
+	.probe = rtw_8821cu_probe,
+	.disconnect = rtw_usb_disconnect,
+};
+module_usb_driver(rtw_8821cu_driver);
+
+MODULE_AUTHOR("Hans Ulli Kroll <linux@ulli-kroll.de>");
+MODULE_DESCRIPTION("Realtek 802.11ac wireless 8821cu driver");
+MODULE_LICENSE("Dual BSD/GPL");
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822b.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822b.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822b.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822b.c	2022-12-24 00:49:25.774376835 +0200
@@ -26,6 +26,12 @@ static void rtw8822be_efuse_parsing(stru
 	ether_addr_copy(efuse->addr, map->e.mac_addr);
 }
 
+static void rtw8822bu_efuse_parsing(struct rtw_efuse *efuse,
+				    struct rtw8822b_efuse *map)
+{
+	ether_addr_copy(efuse->addr, map->u.mac_addr);
+}
+
 static int rtw8822b_read_efuse(struct rtw_dev *rtwdev, u8 *log_map)
 {
 	struct rtw_efuse *efuse = &rtwdev->efuse;
@@ -56,6 +62,9 @@ static int rtw8822b_read_efuse(struct rt
 	case RTW_HCI_TYPE_PCIE:
 		rtw8822be_efuse_parsing(efuse, map);
 		break;
+	case RTW_HCI_TYPE_USB:
+		rtw8822bu_efuse_parsing(efuse, map);
+		break;
 	default:
 		/* unsupported now */
 		return -ENOTSUPP;
@@ -1588,6 +1597,15 @@ static void rtw8822b_adaptivity(struct r
 	rtw_phy_set_edcca_th(rtwdev, l2h, h2l);
 }
 
+static void rtw8822b_fill_txdesc_checksum(struct rtw_dev *rtwdev,
+					  struct rtw_tx_pkt_info *pkt_info,
+					  u8 *txdesc)
+{
+	size_t words = 32 / 2; /* calculate the first 32 bytes (16 words) */
+
+	fill_txdesc_checksum_common(txdesc, words);
+}
+
 static const struct rtw_pwr_seq_cmd trans_carddis_to_cardemu_8822b[] = {
 	{0x0086,
 	 RTW_PWR_CUT_ALL_MSK,
@@ -2163,6 +2181,7 @@ static struct rtw_chip_ops rtw8822b_ops
 	.cfg_csi_rate		= rtw_bf_cfg_csi_rate,
 	.adaptivity_init	= rtw8822b_adaptivity_init,
 	.adaptivity		= rtw8822b_adaptivity,
+	.fill_txdesc_checksum	= rtw8822b_fill_txdesc_checksum,
 
 	.coex_set_init		= rtw8822b_coex_cfg_init,
 	.coex_set_ant_switch	= rtw8822b_coex_cfg_ant_switch,
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822bu.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822bu.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822bu.c	1970-01-01 02:00:00.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822bu.c	2022-12-24 00:49:25.774376835 +0200
@@ -0,0 +1,90 @@
+// SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#include <linux/module.h>
+#include <linux/usb.h>
+#include "main.h"
+#include "rtw8822b.h"
+#include "usb.h"
+
+static const struct usb_device_id rtw_8822bu_id_table[] = {
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xb812, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xb82c, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0x2102, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* CCNC */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x7392, 0xb822, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Edimax EW-7822ULC */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x7392, 0xc822, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Edimax EW-7822UTC */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x7392, 0xd822, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Edimax */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x7392, 0xe822, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Edimax */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x7392, 0xf822, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Edimax EW-7822UAD */
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xb81a, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Default ID */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0b05, 0x1841, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* ASUS AC1300 USB-AC55 B1 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0b05, 0x184c, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* ASUS U2 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0B05, 0x19aa, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* ASUS - USB-AC58 rev A1 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0B05, 0x1870, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* ASUS */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0B05, 0x1874, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* ASUS */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x331e, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Dlink - DWA-181 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x331c, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Dlink - DWA-182 - D1 */
+	{USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x331f, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec)}, /* Dlink - DWA-183 D Ver */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x13b1, 0x0043, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Linksys WUSB6400M */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x13b1, 0x0045, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Linksys WUSB3600 v2 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x012d, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TP-Link Archer T3U v1 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x0138, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TP-Link Archer T3U Plus v1 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x0115, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TP-Link Archer T4U V3 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x012e, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TP-LINK */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x0116, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TP-LINK */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x0117, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TP-LINK */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0846, 0x9055, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Netgear A6150 */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x0e66, 0x0025, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* Hawking HW12ACU */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x04ca, 0x8602, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* LiteOn */
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x20f4, 0x808a, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822b_hw_spec) }, /* TRENDnet TEW-808UBM */
+	{},
+};
+MODULE_DEVICE_TABLE(usb, rtw_8822bu_id_table);
+
+static int rtw8822bu_probe(struct usb_interface *intf,
+			   const struct usb_device_id *id)
+{
+	return rtw_usb_probe(intf, id);
+}
+
+static struct usb_driver rtw_8822bu_driver = {
+	.name = "rtw_8822bu",
+	.id_table = rtw_8822bu_id_table,
+	.probe = rtw8822bu_probe,
+	.disconnect = rtw_usb_disconnect,
+};
+module_usb_driver(rtw_8822bu_driver);
+
+MODULE_AUTHOR("Realtek Corporation");
+MODULE_DESCRIPTION("Realtek 802.11ac wireless 8822bu driver");
+MODULE_LICENSE("Dual BSD/GPL");
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822c.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822c.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822c.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822c.c	2022-12-24 00:49:25.775376835 +0200
@@ -29,6 +29,12 @@ static void rtw8822ce_efuse_parsing(stru
 	ether_addr_copy(efuse->addr, map->e.mac_addr);
 }
 
+static void rtw8822cu_efuse_parsing(struct rtw_efuse *efuse,
+				    struct rtw8822c_efuse *map)
+{
+	ether_addr_copy(efuse->addr, map->u.mac_addr);
+}
+
 static int rtw8822c_read_efuse(struct rtw_dev *rtwdev, u8 *log_map)
 {
 	struct rtw_efuse *efuse = &rtwdev->efuse;
@@ -58,6 +64,9 @@ static int rtw8822c_read_efuse(struct rt
 	case RTW_HCI_TYPE_PCIE:
 		rtw8822ce_efuse_parsing(efuse, map);
 		break;
+	case RTW_HCI_TYPE_USB:
+		rtw8822cu_efuse_parsing(efuse, map);
+		break;
 	default:
 		/* unsupported now */
 		return -ENOTSUPP;
@@ -4557,6 +4566,18 @@ static void rtw8822c_adaptivity(struct r
 	rtw_phy_set_edcca_th(rtwdev, l2h, h2l);
 }
 
+static void rtw8822c_fill_txdesc_checksum(struct rtw_dev *rtwdev,
+					  struct rtw_tx_pkt_info *pkt_info,
+					  u8 *txdesc)
+{
+	const struct rtw_chip_info *chip = rtwdev->chip;
+	size_t words;
+
+	words = (pkt_info->pkt_offset * 8 + chip->tx_pkt_desc_sz) / 2;
+
+	fill_txdesc_checksum_common(txdesc, words);
+}
+
 static const struct rtw_pwr_seq_cmd trans_carddis_to_cardemu_8822c[] = {
 	{0x0086,
 	 RTW_PWR_CUT_ALL_MSK,
@@ -4895,6 +4916,8 @@ static const struct rtw_rfe_def rtw8822c
 	[0] = RTW_DEF_RFE(8822c, 0, 0),
 	[1] = RTW_DEF_RFE(8822c, 0, 0),
 	[2] = RTW_DEF_RFE(8822c, 0, 0),
+	[3] = RTW_DEF_RFE(8822c, 0, 0),
+	[4] = RTW_DEF_RFE(8822c, 0, 0),
 	[5] = RTW_DEF_RFE(8822c, 0, 5),
 	[6] = RTW_DEF_RFE(8822c, 0, 0),
 };
@@ -4978,6 +5001,7 @@ static struct rtw_chip_ops rtw8822c_ops
 	.cfo_track		= rtw8822c_cfo_track,
 	.config_tx_path		= rtw8822c_config_tx_path,
 	.config_txrx_mode	= rtw8822c_config_trx_mode,
+	.fill_txdesc_checksum	= rtw8822c_fill_txdesc_checksum,
 
 	.coex_set_init		= rtw8822c_coex_cfg_init,
 	.coex_set_ant_switch	= NULL,
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822cu.c linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822cu.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/rtw8822cu.c	1970-01-01 02:00:00.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/rtw8822cu.c	2022-12-24 00:49:25.775376835 +0200
@@ -0,0 +1,44 @@
+// SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#include <linux/module.h>
+#include <linux/usb.h>
+#include "main.h"
+#include "rtw8822c.h"
+#include "usb.h"
+
+static const struct usb_device_id rtw_8822cu_id_table[] = {
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc82c, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc812, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc82e, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xd820, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xd82b, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x13b1, 0x0043, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) }, /* Alpha - Alpha */
+	{},
+};
+MODULE_DEVICE_TABLE(usb, rtw_8822cu_id_table);
+
+static int rtw8822bu_probe(struct usb_interface *intf,
+			   const struct usb_device_id *id)
+{
+	return rtw_usb_probe(intf, id);
+}
+
+static struct usb_driver rtw_8822cu_driver = {
+	.name = "rtw_8822cu",
+	.id_table = rtw_8822cu_id_table,
+	.probe = rtw8822bu_probe,
+	.disconnect = rtw_usb_disconnect,
+};
+module_usb_driver(rtw_8822cu_driver);
+
+MODULE_AUTHOR("Realtek Corporation");
+MODULE_DESCRIPTION("Realtek 802.11ac wireless 8822cu driver");
+MODULE_LICENSE("Dual BSD/GPL");
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/tx.h linux-6.2/drivers/net/wireless/realtek/rtw88/tx.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/tx.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/tx.h	2022-12-24 00:49:25.775376835 +0200
@@ -71,6 +71,14 @@
 	le32p_replace_bits((__le32 *)(txdesc) + 0x03, value, BIT(15))
 #define SET_TX_DESC_BT_NULL(txdesc, value)				       \
 	le32p_replace_bits((__le32 *)(txdesc) + 0x02, value, BIT(23))
+#define SET_TX_DESC_TXDESC_CHECKSUM(txdesc, value)				\
+	le32p_replace_bits((__le32 *)(txdesc) + 0x07, value, GENMASK(15, 0))
+#define SET_TX_DESC_DMA_TXAGG_NUM(txdesc, value)				\
+	le32p_replace_bits((__le32 *)(txdesc) + 0x07, value, GENMASK(31, 24))
+#define GET_TX_DESC_PKT_OFFSET(txdesc)						\
+	le32_get_bits(*((__le32 *)(txdesc) + 0x01), GENMASK(28, 24))
+#define GET_TX_DESC_QSEL(txdesc)						\
+	le32_get_bits(*((__le32 *)(txdesc) + 0x01), GENMASK(12, 8))
 
 enum rtw_tx_desc_queue_select {
 	TX_DESC_QSEL_TID0	= 0,
@@ -123,4 +131,27 @@ rtw_tx_write_data_h2c_get(struct rtw_dev
 			  struct rtw_tx_pkt_info *pkt_info,
 			  u8 *buf, u32 size);
 
+static inline
+void fill_txdesc_checksum_common(u8 *txdesc, size_t words)
+{
+	__le16 chksum = 0;
+	__le16 *data = (__le16 *)(txdesc);
+
+	SET_TX_DESC_TXDESC_CHECKSUM(txdesc, 0x0000);
+
+	while (words--)
+		chksum ^= *data++;
+
+	SET_TX_DESC_TXDESC_CHECKSUM(txdesc, __le16_to_cpu(chksum));
+}
+
+static inline void rtw_tx_fill_txdesc_checksum(struct rtw_dev *rtwdev,
+					       struct rtw_tx_pkt_info *pkt_info,
+					       u8 *txdesc)
+{
+	const struct rtw_chip_info *chip = rtwdev->chip;
+
+	chip->ops->fill_txdesc_checksum(rtwdev, pkt_info, txdesc);
+}
+
 #endif
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/usb.c linux-6.2/drivers/net/wireless/realtek/rtw88/usb.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/usb.c	1970-01-01 02:00:00.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/usb.c	2022-12-24 00:49:25.775376835 +0200
@@ -0,0 +1,911 @@
+// SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#include <linux/module.h>
+#include <linux/usb.h>
+#include <linux/mutex.h>
+#include "main.h"
+#include "debug.h"
+#include "reg.h"
+#include "tx.h"
+#include "rx.h"
+#include "fw.h"
+#include "ps.h"
+#include "usb.h"
+
+#define RTW_USB_MAX_RXQ_LEN	512
+
+struct rtw_usb_txcb {
+	struct rtw_dev *rtwdev;
+	struct sk_buff_head tx_ack_queue;
+};
+
+static void rtw_usb_fill_tx_checksum(struct rtw_usb *rtwusb,
+				     struct sk_buff *skb, int agg_num)
+{
+	struct rtw_dev *rtwdev = rtwusb->rtwdev;
+	struct rtw_tx_pkt_info pkt_info;
+
+	SET_TX_DESC_DMA_TXAGG_NUM(skb->data, agg_num);
+	pkt_info.pkt_offset = GET_TX_DESC_PKT_OFFSET(skb->data);
+	rtw_tx_fill_txdesc_checksum(rtwdev, &pkt_info, skb->data);
+}
+
+static u32 rtw_usb_read(struct rtw_dev *rtwdev, u32 addr, u16 len)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	struct usb_device *udev = rtwusb->udev;
+	__le32 *data;
+	unsigned long flags;
+	int idx, ret;
+	static int count;
+
+	spin_lock_irqsave(&rtwusb->usb_lock, flags);
+
+	idx = rtwusb->usb_data_index;
+	rtwusb->usb_data_index = (idx + 1) & (RTW_USB_MAX_RXTX_COUNT - 1);
+
+	spin_unlock_irqrestore(&rtwusb->usb_lock, flags);
+
+	data = &rtwusb->usb_data[idx];
+
+	ret = usb_control_msg(udev, usb_rcvctrlpipe(udev, 0),
+			      RTW_USB_CMD_REQ, RTW_USB_CMD_READ, addr,
+			      RTW_USB_VENQT_CMD_IDX, data, len, 1000);
+	if (ret < 0 && ret != -ENODEV && count++ < 4)
+		rtw_err(rtwdev, "read register 0x%x failed with %d\n",
+			addr, ret);
+
+	return le32_to_cpu(*data);
+}
+
+static u8 rtw_usb_read8(struct rtw_dev *rtwdev, u32 addr)
+{
+	return (u8)rtw_usb_read(rtwdev, addr, 1);
+}
+
+static u16 rtw_usb_read16(struct rtw_dev *rtwdev, u32 addr)
+{
+	return (u16)rtw_usb_read(rtwdev, addr, 2);
+}
+
+static u32 rtw_usb_read32(struct rtw_dev *rtwdev, u32 addr)
+{
+	return (u32)rtw_usb_read(rtwdev, addr, 4);
+}
+
+static void rtw_usb_write(struct rtw_dev *rtwdev, u32 addr, u32 val, int len)
+{
+	struct rtw_usb *rtwusb = (struct rtw_usb *)rtwdev->priv;
+	struct usb_device *udev = rtwusb->udev;
+	unsigned long flags;
+	__le32 *data;
+	int idx, ret;
+	static int count;
+
+	spin_lock_irqsave(&rtwusb->usb_lock, flags);
+
+	idx = rtwusb->usb_data_index;
+	rtwusb->usb_data_index = (idx + 1) & (RTW_USB_MAX_RXTX_COUNT - 1);
+
+	spin_unlock_irqrestore(&rtwusb->usb_lock, flags);
+
+	data = &rtwusb->usb_data[idx];
+
+	*data = cpu_to_le32(val);
+
+	ret = usb_control_msg(udev, usb_sndctrlpipe(udev, 0),
+			      RTW_USB_CMD_REQ, RTW_USB_CMD_WRITE,
+			      addr, 0, data, len, 30000);
+	if (ret < 0 && ret != -ENODEV && count++ < 4)
+		rtw_err(rtwdev, "write register 0x%x failed with %d\n",
+			addr, ret);
+}
+
+static void rtw_usb_write8(struct rtw_dev *rtwdev, u32 addr, u8 val)
+{
+	rtw_usb_write(rtwdev, addr, val, 1);
+}
+
+static void rtw_usb_write16(struct rtw_dev *rtwdev, u32 addr, u16 val)
+{
+	rtw_usb_write(rtwdev, addr, val, 2);
+}
+
+static void rtw_usb_write32(struct rtw_dev *rtwdev, u32 addr, u32 val)
+{
+	rtw_usb_write(rtwdev, addr, val, 4);
+}
+
+static int rtw_usb_parse(struct rtw_dev *rtwdev,
+			 struct usb_interface *interface)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	struct usb_host_interface *host_interface = &interface->altsetting[0];
+	struct usb_interface_descriptor *interface_desc = &host_interface->desc;
+	struct usb_endpoint_descriptor *endpoint;
+	struct usb_device *usbd = interface_to_usbdev(interface);
+	int num_out_pipes = 0;
+	int i;
+	u8 num;
+
+	for (i = 0; i < interface_desc->bNumEndpoints; i++) {
+		endpoint = &host_interface->endpoint[i].desc;
+		num = usb_endpoint_num(endpoint);
+
+		if (usb_endpoint_dir_in(endpoint) &&
+		    usb_endpoint_xfer_bulk(endpoint)) {
+			if (rtwusb->pipe_in) {
+				rtw_err(rtwdev, "IN pipes overflow\n");
+				return -EINVAL;
+			}
+
+			rtwusb->pipe_in = num;
+		}
+
+		if (usb_endpoint_dir_in(endpoint) &&
+		    usb_endpoint_xfer_int(endpoint)) {
+			if (rtwusb->pipe_interrupt) {
+				rtw_err(rtwdev, "INT pipes overflow\n");
+				return -EINVAL;
+			}
+
+			rtwusb->pipe_interrupt = num;
+		}
+
+		if (usb_endpoint_dir_out(endpoint) &&
+		    usb_endpoint_xfer_bulk(endpoint)) {
+			if (num_out_pipes >= ARRAY_SIZE(rtwusb->out_ep)) {
+				rtw_err(rtwdev, "OUT pipes overflow\n");
+				return -EINVAL;
+			}
+
+			rtwusb->out_ep[num_out_pipes++] = num;
+		}
+	}
+
+	switch (usbd->speed) {
+	case USB_SPEED_LOW:
+	case USB_SPEED_FULL:
+		rtwusb->bulkout_size = RTW_USB_FULL_SPEED_BULK_SIZE;
+		break;
+	case USB_SPEED_HIGH:
+		rtwusb->bulkout_size = RTW_USB_HIGH_SPEED_BULK_SIZE;
+		break;
+	case USB_SPEED_SUPER:
+		rtwusb->bulkout_size = RTW_USB_SUPER_SPEED_BULK_SIZE;
+		break;
+	default:
+		rtw_err(rtwdev, "failed to detect usb speed\n");
+		return -EINVAL;
+	}
+
+	rtwdev->hci.bulkout_num = num_out_pipes;
+
+	switch (num_out_pipes) {
+	case 4:
+	case 3:
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID0] = 2;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID1] = 2;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID2] = 2;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID3] = 2;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID4] = 1;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID5] = 1;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID6] = 0;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID7] = 0;
+		break;
+	case 2:
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID0] = 1;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID1] = 1;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID2] = 1;
+		rtwusb->qsel_to_ep[TX_DESC_QSEL_TID3] = 1;
+		break;
+	case 1:
+		break;
+	default:
+		rtw_err(rtwdev, "failed to get out_pipes(%d)\n", num_out_pipes);
+		return -EINVAL;
+	}
+
+	return 0;
+}
+
+static void rtw_usb_write_port_tx_complete(struct urb *urb)
+{
+	struct rtw_usb_txcb *txcb = urb->context;
+	struct rtw_dev *rtwdev = txcb->rtwdev;
+	struct ieee80211_hw *hw = rtwdev->hw;
+
+	while (true) {
+		struct sk_buff *skb = skb_dequeue(&txcb->tx_ack_queue);
+		struct ieee80211_tx_info *info;
+		struct rtw_usb_tx_data *tx_data;
+
+		if (!skb)
+			break;
+
+		info = IEEE80211_SKB_CB(skb);
+		tx_data = rtw_usb_get_tx_data(skb);
+
+		/* enqueue to wait for tx report */
+		if (info->flags & IEEE80211_TX_CTL_REQ_TX_STATUS) {
+			rtw_tx_report_enqueue(rtwdev, skb, tx_data->sn);
+			continue;
+		}
+
+		/* always ACK for others, then they won't be marked as drop */
+		ieee80211_tx_info_clear_status(info);
+		if (info->flags & IEEE80211_TX_CTL_NO_ACK)
+			info->flags |= IEEE80211_TX_STAT_NOACK_TRANSMITTED;
+		else
+			info->flags |= IEEE80211_TX_STAT_ACK;
+
+		ieee80211_tx_status_irqsafe(hw, skb);
+	}
+
+	kfree(txcb);
+}
+
+static int qsel_to_ep(struct rtw_usb *rtwusb, unsigned int qsel)
+{
+	if (qsel >= ARRAY_SIZE(rtwusb->qsel_to_ep))
+		return 0;
+
+	return rtwusb->qsel_to_ep[qsel];
+}
+
+static int rtw_usb_write_port(struct rtw_dev *rtwdev, u8 qsel, struct sk_buff *skb,
+			      usb_complete_t cb, void *context)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	struct usb_device *usbd = rtwusb->udev;
+	struct urb *urb;
+	unsigned int pipe;
+	int ret;
+	int ep = qsel_to_ep(rtwusb, qsel);
+
+	pipe = usb_sndbulkpipe(usbd, rtwusb->out_ep[ep]);
+	urb = usb_alloc_urb(0, GFP_ATOMIC);
+	if (!urb)
+		return -ENOMEM;
+
+	usb_fill_bulk_urb(urb, usbd, pipe, skb->data, skb->len, cb, context);
+	ret = usb_submit_urb(urb, GFP_ATOMIC);
+
+	usb_free_urb(urb);
+
+	return ret;
+}
+
+static bool rtw_usb_tx_agg_skb(struct rtw_usb *rtwusb, struct sk_buff_head *list)
+{
+	struct rtw_dev *rtwdev = rtwusb->rtwdev;
+	struct rtw_usb_txcb *txcb;
+	struct sk_buff *skb_head;
+	struct sk_buff *skb_iter;
+	int agg_num = 0;
+	unsigned int align_next = 0;
+
+	if (skb_queue_empty(list))
+		return false;
+
+	txcb = kmalloc(sizeof(*txcb), GFP_ATOMIC);
+	if (!txcb)
+		return false;
+
+	txcb->rtwdev = rtwdev;
+	skb_queue_head_init(&txcb->tx_ack_queue);
+
+	skb_iter = skb_dequeue(list);
+
+	if (skb_queue_empty(list)) {
+		skb_head = skb_iter;
+		goto queue;
+	}
+
+	skb_head = dev_alloc_skb(RTW_USB_MAX_XMITBUF_SZ);
+	if (!skb_head) {
+		skb_head = skb_iter;
+		goto queue;
+	}
+
+	while (skb_iter) {
+		unsigned long flags;
+
+		skb_put(skb_head, align_next);
+		skb_put_data(skb_head, skb_iter->data, skb_iter->len);
+
+		align_next = ALIGN(skb_iter->len, 8) - skb_iter->len;
+
+		agg_num++;
+
+		skb_queue_tail(&txcb->tx_ack_queue, skb_iter);
+
+		spin_lock_irqsave(&list->lock, flags);
+
+		skb_iter = skb_peek(list);
+
+		if (skb_iter && skb_iter->len + skb_head->len <= RTW_USB_MAX_XMITBUF_SZ)
+			__skb_unlink(skb_iter, list);
+		else
+			skb_iter = NULL;
+		spin_unlock_irqrestore(&list->lock, flags);
+	}
+
+	if (agg_num > 1)
+		rtw_usb_fill_tx_checksum(rtwusb, skb_head, agg_num);
+
+queue:
+	skb_queue_tail(&txcb->tx_ack_queue, skb_head);
+
+	rtw_usb_write_port(rtwdev, GET_TX_DESC_QSEL(skb_head->data), skb_head,
+			   rtw_usb_write_port_tx_complete, txcb);
+
+	return true;
+}
+
+static void rtw_usb_tx_handler(struct work_struct *work)
+{
+	struct rtw_usb *rtwusb = container_of(work, struct rtw_usb, tx_work);
+	int i, limit;
+
+	for (i = ARRAY_SIZE(rtwusb->tx_queue) - 1; i >= 0; i--) {
+		for (limit = 0; limit < 200; limit++) {
+			struct sk_buff_head *list = &rtwusb->tx_queue[i];
+
+			if (!rtw_usb_tx_agg_skb(rtwusb, list))
+				break;
+		}
+	}
+}
+
+static void rtw_usb_tx_queue_purge(struct rtw_usb *rtwusb)
+{
+	int i;
+
+	for (i = 0; i < ARRAY_SIZE(rtwusb->tx_queue); i++)
+		skb_queue_purge(&rtwusb->tx_queue[i]);
+}
+
+static void rtw_usb_write_port_complete(struct urb *urb)
+{
+	struct sk_buff *skb = urb->context;
+
+	dev_kfree_skb_any(skb);
+}
+
+static int rtw_usb_write_data(struct rtw_dev *rtwdev,
+			      struct rtw_tx_pkt_info *pkt_info,
+			      u8 *buf)
+{
+	const struct rtw_chip_info *chip = rtwdev->chip;
+	struct sk_buff *skb;
+	unsigned int desclen, headsize, size;
+	u8 qsel;
+	int ret = 0;
+
+	size = pkt_info->tx_pkt_size;
+	qsel = pkt_info->qsel;
+	desclen = chip->tx_pkt_desc_sz;
+	headsize = pkt_info->offset ? pkt_info->offset : desclen;
+
+	skb = dev_alloc_skb(headsize + size);
+	if (unlikely(!skb))
+		return -ENOMEM;
+
+	skb_reserve(skb, headsize);
+	skb_put_data(skb, buf, size);
+	skb_push(skb, headsize);
+	memset(skb->data, 0, headsize);
+	rtw_tx_fill_tx_desc(pkt_info, skb);
+	rtw_tx_fill_txdesc_checksum(rtwdev, pkt_info, skb->data);
+
+	ret = rtw_usb_write_port(rtwdev, qsel, skb,
+				 rtw_usb_write_port_complete, skb);
+	if (unlikely(ret))
+		rtw_err(rtwdev, "failed to do USB write, ret=%d\n", ret);
+
+	return ret;
+}
+
+static int rtw_usb_write_data_rsvd_page(struct rtw_dev *rtwdev, u8 *buf,
+					u32 size)
+{
+	const struct rtw_chip_info *chip = rtwdev->chip;
+	struct rtw_usb *rtwusb;
+	struct rtw_tx_pkt_info pkt_info = {0};
+	u32 len, desclen;
+
+	rtwusb = rtw_get_usb_priv(rtwdev);
+
+	pkt_info.tx_pkt_size = size;
+	pkt_info.qsel = TX_DESC_QSEL_BEACON;
+
+	desclen = chip->tx_pkt_desc_sz;
+	len = desclen + size;
+	if (len % rtwusb->bulkout_size == 0) {
+		len += RTW_USB_PACKET_OFFSET_SZ;
+		pkt_info.offset = desclen + RTW_USB_PACKET_OFFSET_SZ;
+		pkt_info.pkt_offset = 1;
+	} else {
+		pkt_info.offset = desclen;
+	}
+
+	return rtw_usb_write_data(rtwdev, &pkt_info, buf);
+}
+
+static int rtw_usb_write_data_h2c(struct rtw_dev *rtwdev, u8 *buf, u32 size)
+{
+	struct rtw_tx_pkt_info pkt_info = {0};
+
+	pkt_info.tx_pkt_size = size;
+	pkt_info.qsel = TX_DESC_QSEL_H2C;
+
+	return rtw_usb_write_data(rtwdev, &pkt_info, buf);
+}
+
+static u8 rtw_usb_tx_queue_mapping_to_qsel(struct sk_buff *skb)
+{
+	struct ieee80211_hdr *hdr = (struct ieee80211_hdr *)skb->data;
+	__le16 fc = hdr->frame_control;
+	u8 qsel;
+
+	if (unlikely(ieee80211_is_mgmt(fc) || ieee80211_is_ctl(fc)))
+		qsel = TX_DESC_QSEL_MGMT;
+	else if (skb_get_queue_mapping(skb) <= IEEE80211_AC_BK)
+		qsel = skb->priority;
+	else
+		qsel = TX_DESC_QSEL_BEACON;
+
+	return qsel;
+}
+
+static int rtw_usb_tx_write(struct rtw_dev *rtwdev,
+			    struct rtw_tx_pkt_info *pkt_info,
+			    struct sk_buff *skb)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	const struct rtw_chip_info *chip = rtwdev->chip;
+	struct rtw_usb_tx_data *tx_data;
+	u8 *pkt_desc;
+	int ep;
+
+	pkt_desc = skb_push(skb, chip->tx_pkt_desc_sz);
+	memset(pkt_desc, 0, chip->tx_pkt_desc_sz);
+	pkt_info->qsel = rtw_usb_tx_queue_mapping_to_qsel(skb);
+	ep = qsel_to_ep(rtwusb, pkt_info->qsel);
+	rtw_tx_fill_tx_desc(pkt_info, skb);
+	rtw_tx_fill_txdesc_checksum(rtwdev, pkt_info, skb->data);
+	tx_data = rtw_usb_get_tx_data(skb);
+	tx_data->sn = pkt_info->sn;
+
+	skb_queue_tail(&rtwusb->tx_queue[ep], skb);
+
+	return 0;
+}
+
+static void rtw_usb_tx_kick_off(struct rtw_dev *rtwdev)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+
+	queue_work(rtwusb->txwq, &rtwusb->tx_work);
+}
+
+static void rtw_usb_rx_handler(struct work_struct *work)
+{
+	struct rtw_usb *rtwusb = container_of(work, struct rtw_usb, rx_work);
+	struct rtw_dev *rtwdev = rtwusb->rtwdev;
+	const struct rtw_chip_info *chip = rtwdev->chip;
+	struct rtw_rx_pkt_stat pkt_stat;
+	struct ieee80211_rx_status rx_status;
+	struct sk_buff *skb;
+	u32 pkt_desc_sz = chip->rx_pkt_desc_sz;
+	u32 pkt_offset;
+	u8 *rx_desc;
+	int limit;
+
+	for (limit = 0; limit < 200; limit++) {
+		skb = skb_dequeue(&rtwusb->rx_queue);
+		if (!skb)
+			break;
+
+		rx_desc = skb->data;
+		chip->ops->query_rx_desc(rtwdev, rx_desc, &pkt_stat,
+					 &rx_status);
+		pkt_offset = pkt_desc_sz + pkt_stat.drv_info_sz +
+			     pkt_stat.shift;
+
+		if (pkt_stat.is_c2h) {
+			skb_put(skb, pkt_stat.pkt_len + pkt_offset);
+			rtw_fw_c2h_cmd_rx_irqsafe(rtwdev, pkt_offset, skb);
+			continue;
+		}
+
+		if (skb_queue_len(&rtwusb->rx_queue) >= RTW_USB_MAX_RXQ_LEN) {
+			rtw_err(rtwdev, "failed to get rx_queue, overflow\n");
+			dev_kfree_skb_any(skb);
+			continue;
+		}
+
+		skb_put(skb, pkt_stat.pkt_len);
+		skb_reserve(skb, pkt_offset);
+		memcpy(skb->cb, &rx_status, sizeof(rx_status));
+		ieee80211_rx_irqsafe(rtwdev->hw, skb);
+	}
+}
+
+static void rtw_usb_read_port_complete(struct urb *urb);
+
+static void rtw_usb_rx_resubmit(struct rtw_usb *rtwusb, struct rx_usb_ctrl_block *rxcb)
+{
+	struct rtw_dev *rtwdev = rtwusb->rtwdev;
+	int error;
+
+	rxcb->rx_skb = alloc_skb(RTW_USB_MAX_RECVBUF_SZ, GFP_ATOMIC);
+	if (!rxcb->rx_skb)
+		return;
+
+	usb_fill_bulk_urb(rxcb->rx_urb, rtwusb->udev,
+			  usb_rcvbulkpipe(rtwusb->udev, rtwusb->pipe_in),
+			  rxcb->rx_skb->data, RTW_USB_MAX_RECVBUF_SZ,
+			  rtw_usb_read_port_complete, rxcb);
+
+	error = usb_submit_urb(rxcb->rx_urb, GFP_ATOMIC);
+	if (error) {
+		kfree_skb(rxcb->rx_skb);
+		if (error != -ENODEV)
+			rtw_err(rtwdev, "Err sending rx data urb %d\n",
+				error);
+	}
+}
+
+static void rtw_usb_read_port_complete(struct urb *urb)
+{
+	struct rx_usb_ctrl_block *rxcb = urb->context;
+	struct rtw_dev *rtwdev = rxcb->rtwdev;
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	struct sk_buff *skb = rxcb->rx_skb;
+
+	if (urb->status == 0) {
+		if (urb->actual_length >= RTW_USB_MAX_RECVBUF_SZ ||
+		    urb->actual_length < 24) {
+			rtw_err(rtwdev, "failed to get urb length:%d\n",
+				urb->actual_length);
+			if (skb)
+				dev_kfree_skb_any(skb);
+		} else {
+			skb_queue_tail(&rtwusb->rx_queue, skb);
+			queue_work(rtwusb->rxwq, &rtwusb->rx_work);
+		}
+		rtw_usb_rx_resubmit(rtwusb, rxcb);
+	} else {
+		switch (urb->status) {
+		case -EINVAL:
+		case -EPIPE:
+		case -ENODEV:
+		case -ESHUTDOWN:
+		case -ENOENT:
+		case -EPROTO:
+		case -EILSEQ:
+		case -ETIME:
+		case -ECOMM:
+		case -EOVERFLOW:
+		case -EINPROGRESS:
+			break;
+		default:
+			rtw_err(rtwdev, "status %d\n", urb->status);
+			break;
+		}
+		if (skb)
+			dev_kfree_skb_any(skb);
+	}
+}
+
+static void rtw_usb_cancel_rx_bufs(struct rtw_usb *rtwusb)
+{
+	struct rx_usb_ctrl_block *rxcb;
+	int i;
+
+	for (i = 0; i < RTW_USB_RXCB_NUM; i++) {
+		rxcb = &rtwusb->rx_cb[i];
+		if (rxcb->rx_urb)
+			usb_kill_urb(rxcb->rx_urb);
+	}
+}
+
+static void rtw_usb_free_rx_bufs(struct rtw_usb *rtwusb)
+{
+	struct rx_usb_ctrl_block *rxcb;
+	int i;
+
+	for (i = 0; i < RTW_USB_RXCB_NUM; i++) {
+		rxcb = &rtwusb->rx_cb[i];
+		if (rxcb->rx_urb) {
+			usb_kill_urb(rxcb->rx_urb);
+			usb_free_urb(rxcb->rx_urb);
+		}
+	}
+}
+
+static int rtw_usb_alloc_rx_bufs(struct rtw_usb *rtwusb)
+{
+	int i;
+
+	for (i = 0; i < RTW_USB_RXCB_NUM; i++) {
+		struct rx_usb_ctrl_block *rxcb = &rtwusb->rx_cb[i];
+
+		rxcb->n = i;
+		rxcb->rtwdev = rtwusb->rtwdev;
+		rxcb->rx_urb = usb_alloc_urb(0, GFP_KERNEL);
+		if (!rxcb->rx_urb)
+			goto err;
+	}
+
+	return 0;
+err:
+	rtw_usb_free_rx_bufs(rtwusb);
+	return -ENOMEM;
+}
+
+static int rtw_usb_setup(struct rtw_dev *rtwdev)
+{
+	/* empty function for rtw_hci_ops */
+	return 0;
+}
+
+static int rtw_usb_start(struct rtw_dev *rtwdev)
+{
+	return 0;
+}
+
+static void rtw_usb_stop(struct rtw_dev *rtwdev)
+{
+}
+
+static void rtw_usb_deep_ps(struct rtw_dev *rtwdev, bool enter)
+{
+	/* empty function for rtw_hci_ops */
+}
+
+static void rtw_usb_link_ps(struct rtw_dev *rtwdev, bool enter)
+{
+	/* empty function for rtw_hci_ops */
+}
+
+static void rtw_usb_interface_cfg(struct rtw_dev *rtwdev)
+{
+	/* empty function for rtw_hci_ops */
+}
+
+static struct rtw_hci_ops rtw_usb_ops = {
+	.tx_write = rtw_usb_tx_write,
+	.tx_kick_off = rtw_usb_tx_kick_off,
+	.setup = rtw_usb_setup,
+	.start = rtw_usb_start,
+	.stop = rtw_usb_stop,
+	.deep_ps = rtw_usb_deep_ps,
+	.link_ps = rtw_usb_link_ps,
+	.interface_cfg = rtw_usb_interface_cfg,
+
+	.write8  = rtw_usb_write8,
+	.write16 = rtw_usb_write16,
+	.write32 = rtw_usb_write32,
+	.read8	= rtw_usb_read8,
+	.read16 = rtw_usb_read16,
+	.read32 = rtw_usb_read32,
+
+	.write_data_rsvd_page = rtw_usb_write_data_rsvd_page,
+	.write_data_h2c = rtw_usb_write_data_h2c,
+};
+
+static int rtw_usb_init_rx(struct rtw_dev *rtwdev)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	int i;
+
+	rtwusb->rxwq = create_singlethread_workqueue("rtw88_usb: rx wq");
+	if (!rtwusb->rxwq) {
+		rtw_err(rtwdev, "failed to create RX work queue\n");
+		return -ENOMEM;
+	}
+
+	skb_queue_head_init(&rtwusb->rx_queue);
+
+	INIT_WORK(&rtwusb->rx_work, rtw_usb_rx_handler);
+
+	for (i = 0; i < RTW_USB_RXCB_NUM; i++) {
+		struct rx_usb_ctrl_block *rxcb = &rtwusb->rx_cb[i];
+
+		rtw_usb_rx_resubmit(rtwusb, rxcb);
+	}
+
+	return 0;
+}
+
+static void rtw_usb_deinit_rx(struct rtw_dev *rtwdev)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+
+	skb_queue_purge(&rtwusb->rx_queue);
+
+	flush_workqueue(rtwusb->rxwq);
+	destroy_workqueue(rtwusb->rxwq);
+}
+
+static int rtw_usb_init_tx(struct rtw_dev *rtwdev)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	int i;
+
+	rtwusb->txwq = create_singlethread_workqueue("rtw88_usb: tx wq");
+	if (!rtwusb->txwq) {
+		rtw_err(rtwdev, "failed to create TX work queue\n");
+		return -ENOMEM;
+	}
+
+	for (i = 0; i < ARRAY_SIZE(rtwusb->tx_queue); i++)
+		skb_queue_head_init(&rtwusb->tx_queue[i]);
+
+	INIT_WORK(&rtwusb->tx_work, rtw_usb_tx_handler);
+
+	return 0;
+}
+
+static void rtw_usb_deinit_tx(struct rtw_dev *rtwdev)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+
+	rtw_usb_tx_queue_purge(rtwusb);
+	flush_workqueue(rtwusb->txwq);
+	destroy_workqueue(rtwusb->txwq);
+}
+
+static int rtw_usb_intf_init(struct rtw_dev *rtwdev,
+			     struct usb_interface *intf)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+	struct usb_device *udev = usb_get_dev(interface_to_usbdev(intf));
+	int ret;
+
+	rtwusb->udev = udev;
+	ret = rtw_usb_parse(rtwdev, intf);
+	if (ret)
+		return ret;
+
+	rtwusb->usb_data = kcalloc(RTW_USB_MAX_RXTX_COUNT, sizeof(u32),
+				   GFP_KERNEL);
+	if (!rtwusb->usb_data)
+		return -ENOMEM;
+
+	usb_set_intfdata(intf, rtwdev->hw);
+
+	SET_IEEE80211_DEV(rtwdev->hw, &intf->dev);
+	spin_lock_init(&rtwusb->usb_lock);
+
+	return 0;
+}
+
+static void rtw_usb_intf_deinit(struct rtw_dev *rtwdev,
+				struct usb_interface *intf)
+{
+	struct rtw_usb *rtwusb = rtw_get_usb_priv(rtwdev);
+
+	usb_put_dev(rtwusb->udev);
+	usb_set_intfdata(intf, NULL);
+}
+
+int rtw_usb_probe(struct usb_interface *intf, const struct usb_device_id *id)
+{
+	struct rtw_dev *rtwdev;
+	struct ieee80211_hw *hw;
+	struct rtw_usb *rtwusb;
+	int drv_data_size;
+	int ret;
+
+	drv_data_size = sizeof(struct rtw_dev) + sizeof(struct rtw_usb);
+	hw = ieee80211_alloc_hw(drv_data_size, &rtw_ops);
+	if (!hw)
+		return -ENOMEM;
+
+	rtwdev = hw->priv;
+	rtwdev->hw = hw;
+	rtwdev->dev = &intf->dev;
+	rtwdev->chip = (struct rtw_chip_info *)id->driver_info;
+	rtwdev->hci.ops = &rtw_usb_ops;
+	rtwdev->hci.type = RTW_HCI_TYPE_USB;
+
+	rtwusb = rtw_get_usb_priv(rtwdev);
+	rtwusb->rtwdev = rtwdev;
+
+	ret = rtw_usb_alloc_rx_bufs(rtwusb);
+	if (ret)
+		return ret;
+
+	ret = rtw_core_init(rtwdev);
+	if (ret)
+		goto err_release_hw;
+
+	ret = rtw_usb_intf_init(rtwdev, intf);
+	if (ret) {
+		rtw_err(rtwdev, "failed to init USB interface\n");
+		goto err_deinit_core;
+	}
+
+	ret = rtw_usb_init_tx(rtwdev);
+	if (ret) {
+		rtw_err(rtwdev, "failed to init USB TX\n");
+		goto err_destroy_usb;
+	}
+
+	ret = rtw_usb_init_rx(rtwdev);
+	if (ret) {
+		rtw_err(rtwdev, "failed to init USB RX\n");
+		goto err_destroy_txwq;
+	}
+
+	ret = rtw_chip_info_setup(rtwdev);
+	if (ret) {
+		rtw_err(rtwdev, "failed to setup chip information\n");
+		goto err_destroy_rxwq;
+	}
+
+	ret = rtw_register_hw(rtwdev, rtwdev->hw);
+	if (ret) {
+		rtw_err(rtwdev, "failed to register hw\n");
+		goto err_destroy_rxwq;
+	}
+
+	return 0;
+
+err_destroy_rxwq:
+	rtw_usb_deinit_rx(rtwdev);
+
+err_destroy_txwq:
+	rtw_usb_deinit_tx(rtwdev);
+
+err_destroy_usb:
+	rtw_usb_intf_deinit(rtwdev, intf);
+
+err_deinit_core:
+	rtw_core_deinit(rtwdev);
+
+err_release_hw:
+	ieee80211_free_hw(hw);
+
+	return ret;
+}
+EXPORT_SYMBOL(rtw_usb_probe);
+
+void rtw_usb_disconnect(struct usb_interface *intf)
+{
+	struct ieee80211_hw *hw = usb_get_intfdata(intf);
+	struct rtw_dev *rtwdev;
+	struct rtw_usb *rtwusb;
+
+	if (!hw)
+		return;
+
+	rtwdev = hw->priv;
+	rtwusb = rtw_get_usb_priv(rtwdev);
+
+	rtw_usb_cancel_rx_bufs(rtwusb);
+
+	rtw_unregister_hw(rtwdev, hw);
+	rtw_usb_deinit_tx(rtwdev);
+	rtw_usb_deinit_rx(rtwdev);
+
+	if (rtwusb->udev->state != USB_STATE_NOTATTACHED)
+		usb_reset_device(rtwusb->udev);
+
+	rtw_usb_free_rx_bufs(rtwusb);
+
+	rtw_usb_intf_deinit(rtwdev, intf);
+	rtw_core_deinit(rtwdev);
+	ieee80211_free_hw(hw);
+}
+EXPORT_SYMBOL(rtw_usb_disconnect);
+
+MODULE_AUTHOR("Realtek Corporation");
+MODULE_DESCRIPTION("Realtek 802.11ac wireless USB driver");
+MODULE_LICENSE("Dual BSD/GPL");
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/usb.h linux-6.2/drivers/net/wireless/realtek/rtw88/usb.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/usb.h	1970-01-01 02:00:00.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/usb.h	2022-12-24 00:49:25.775376835 +0200
@@ -0,0 +1,107 @@
+/* SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause */
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#ifndef __RTW_USB_H_
+#define __RTW_USB_H_
+
+#define FW_8192C_START_ADDRESS		0x1000
+#define FW_8192C_END_ADDRESS		0x5fff
+
+#define RTW_USB_MAX_RXTX_COUNT		128
+#define RTW_USB_VENQT_MAX_BUF_SIZE	254
+#define MAX_USBCTRL_VENDORREQ_TIMES	10
+
+#define RTW_USB_CMD_READ		0xc0
+#define RTW_USB_CMD_WRITE		0x40
+#define RTW_USB_CMD_REQ			0x05
+
+#define RTW_USB_VENQT_CMD_IDX		0x00
+
+#define RTW_USB_SUPER_SPEED_BULK_SIZE	1024
+#define RTW_USB_HIGH_SPEED_BULK_SIZE	512
+#define RTW_USB_FULL_SPEED_BULK_SIZE	64
+
+#define RTW_USB_TX_SEL_HQ		BIT(0)
+#define RTW_USB_TX_SEL_LQ		BIT(1)
+#define RTW_USB_TX_SEL_NQ		BIT(2)
+#define RTW_USB_TX_SEL_EQ		BIT(3)
+
+#define RTW_USB_BULK_IN_ADDR		0x80
+#define RTW_USB_INT_IN_ADDR		0x81
+
+#define RTW_USB_HW_QUEUE_ENTRY		8
+
+#define RTW_USB_PACKET_OFFSET_SZ	8
+#define RTW_USB_MAX_XMITBUF_SZ		(1024 * 20)
+#define RTW_USB_MAX_RECVBUF_SZ		32768
+
+#define RTW_USB_RECVBUFF_ALIGN_SZ	8
+
+#define RTW_USB_RXAGG_SIZE		6
+#define RTW_USB_RXAGG_TIMEOUT		10
+
+#define RTW_USB_RXCB_NUM		4
+
+#define RTW_USB_EP_MAX			4
+
+#define TX_DESC_QSEL_MAX		20
+
+#define RTW_USB_VENDOR_ID_REALTEK	0x0bda
+
+static inline struct rtw_usb *rtw_get_usb_priv(struct rtw_dev *rtwdev)
+{
+	return (struct rtw_usb *)rtwdev->priv;
+}
+
+struct rx_usb_ctrl_block {
+	struct rtw_dev *rtwdev;
+	struct urb *rx_urb;
+	struct sk_buff *rx_skb;
+	int n;
+};
+
+struct rtw_usb_tx_data {
+	u8 sn;
+};
+
+struct rtw_usb {
+	struct rtw_dev *rtwdev;
+	struct usb_device *udev;
+
+	/* protects usb_data_index */
+	spinlock_t usb_lock;
+	__le32 *usb_data;
+	unsigned int usb_data_index;
+
+	u32 bulkout_size;
+	u8 pipe_interrupt;
+	u8 pipe_in;
+	u8 out_ep[RTW_USB_EP_MAX];
+	u8 qsel_to_ep[TX_DESC_QSEL_MAX];
+	u8 usb_txagg_num;
+
+	struct workqueue_struct *txwq, *rxwq;
+
+	struct sk_buff_head tx_queue[RTW_USB_EP_MAX];
+	struct work_struct tx_work;
+
+	struct rx_usb_ctrl_block rx_cb[RTW_USB_RXCB_NUM];
+	struct sk_buff_head rx_queue;
+	struct work_struct rx_work;
+};
+
+static inline struct rtw_usb_tx_data *rtw_usb_get_tx_data(struct sk_buff *skb)
+{
+	struct ieee80211_tx_info *info = IEEE80211_SKB_CB(skb);
+
+	BUILD_BUG_ON(sizeof(struct rtw_usb_tx_data) >
+		     sizeof(info->status.status_driver_data));
+
+	return (struct rtw_usb_tx_data *)info->status.status_driver_data;
+}
+
+int rtw_usb_probe(struct usb_interface *intf, const struct usb_device_id *id);
+void rtw_usb_disconnect(struct usb_interface *intf);
+
+#endif
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/util.c linux-6.2/drivers/net/wireless/realtek/rtw88/util.c
--- linux-6.1/drivers/net/wireless/realtek/rtw88/util.c	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/util.c	2022-12-24 00:49:25.775376835 +0200
@@ -105,3 +105,106 @@ void rtw_desc_to_mcsrate(u16 rate, u8 *m
 		*mcs = rate - DESC_RATEMCS0;
 	}
 }
+
+struct rtw_stas_entry {
+	struct list_head list;
+	struct ieee80211_sta *sta;
+};
+
+struct rtw_iter_stas_data {
+	struct rtw_dev *rtwdev;
+	struct list_head list;
+};
+
+static void rtw_collect_sta_iter(void *data, struct ieee80211_sta *sta)
+{
+	struct rtw_iter_stas_data *iter_stas = data;
+	struct rtw_stas_entry *stas_entry;
+
+	stas_entry = kmalloc(sizeof(*stas_entry), GFP_ATOMIC);
+	if (!stas_entry)
+		return;
+
+	stas_entry->sta = sta;
+	list_add_tail(&stas_entry->list, &iter_stas->list);
+}
+
+void rtw_iterate_stas(struct rtw_dev *rtwdev,
+		      void (*iterator)(void *data,
+				       struct ieee80211_sta *sta),
+		      void *data)
+{
+	struct rtw_iter_stas_data iter_data;
+	struct rtw_stas_entry *sta_entry, *tmp;
+
+	/* &rtwdev->mutex makes sure no stations can be removed between
+	 * collecting the stations and iterating over them.
+	 */
+	lockdep_assert_held(&rtwdev->mutex);
+
+	iter_data.rtwdev = rtwdev;
+	INIT_LIST_HEAD(&iter_data.list);
+
+	ieee80211_iterate_stations_atomic(rtwdev->hw, rtw_collect_sta_iter,
+					  &iter_data);
+
+	list_for_each_entry_safe(sta_entry, tmp, &iter_data.list,
+				 list) {
+		list_del_init(&sta_entry->list);
+		iterator(data, sta_entry->sta);
+		kfree(sta_entry);
+	}
+}
+
+struct rtw_vifs_entry {
+	struct list_head list;
+	struct ieee80211_vif *vif;
+	u8 mac[ETH_ALEN];
+};
+
+struct rtw_iter_vifs_data {
+	struct rtw_dev *rtwdev;
+	struct list_head list;
+};
+
+static void rtw_collect_vif_iter(void *data, u8 *mac, struct ieee80211_vif *vif)
+{
+	struct rtw_iter_vifs_data *iter_stas = data;
+	struct rtw_vifs_entry *vifs_entry;
+
+	vifs_entry = kmalloc(sizeof(*vifs_entry), GFP_ATOMIC);
+	if (!vifs_entry)
+		return;
+
+	vifs_entry->vif = vif;
+	ether_addr_copy(vifs_entry->mac, mac);
+	list_add_tail(&vifs_entry->list, &iter_stas->list);
+}
+
+void rtw_iterate_vifs(struct rtw_dev *rtwdev,
+		      void (*iterator)(void *data, u8 *mac,
+				       struct ieee80211_vif *vif),
+		      void *data)
+{
+	struct rtw_iter_vifs_data iter_data;
+	struct rtw_vifs_entry *vif_entry, *tmp;
+
+	/* &rtwdev->mutex makes sure no interfaces can be removed between
+	 * collecting the interfaces and iterating over them.
+	 */
+	lockdep_assert_held(&rtwdev->mutex);
+
+	iter_data.rtwdev = rtwdev;
+	INIT_LIST_HEAD(&iter_data.list);
+
+	ieee80211_iterate_active_interfaces_atomic(rtwdev->hw,
+						   IEEE80211_IFACE_ITER_NORMAL,
+						   rtw_collect_vif_iter, &iter_data);
+
+	list_for_each_entry_safe(vif_entry, tmp, &iter_data.list,
+				 list) {
+		list_del_init(&vif_entry->list);
+		iterator(data, vif_entry->mac, vif_entry->vif);
+		kfree(vif_entry);
+	}
+}
diff -Nurp linux-6.1/drivers/net/wireless/realtek/rtw88/util.h linux-6.2/drivers/net/wireless/realtek/rtw88/util.h
--- linux-6.1/drivers/net/wireless/realtek/rtw88/util.h	2022-12-12 00:15:18.000000000 +0200
+++ linux-6.2/drivers/net/wireless/realtek/rtw88/util.h	2022-12-24 00:49:25.775376835 +0200
@@ -7,9 +7,6 @@
 
 struct rtw_dev;
 
-#define rtw_iterate_vifs(rtwdev, iterator, data)                               \
-	ieee80211_iterate_active_interfaces(rtwdev->hw,                        \
-			IEEE80211_IFACE_ITER_NORMAL, iterator, data)
 #define rtw_iterate_vifs_atomic(rtwdev, iterator, data)                        \
 	ieee80211_iterate_active_interfaces_atomic(rtwdev->hw,                 \
 			IEEE80211_IFACE_ITER_NORMAL, iterator, data)
@@ -20,6 +17,15 @@ struct rtw_dev;
 #define rtw_iterate_keys_rcu(rtwdev, vif, iterator, data)		       \
 	ieee80211_iter_keys_rcu((rtwdev)->hw, vif, iterator, data)
 
+void rtw_iterate_vifs(struct rtw_dev *rtwdev,
+		      void (*iterator)(void *data, u8 *mac,
+				       struct ieee80211_vif *vif),
+		      void *data);
+void rtw_iterate_stas(struct rtw_dev *rtwdev,
+		      void (*iterator)(void *data,
+				       struct ieee80211_sta *sta),
+				       void *data);
+
 static inline u8 *get_hdr_bssid(struct ieee80211_hdr *hdr)
 {
 	__le16 fc = hdr->frame_control;
