From 482626063d446eac1809e025a79ad0a7d45bc22d Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Wed, 16 Dec 2015 13:24:40 -0800
Subject: [PATCH 1/4] ARM: bcm2835: Split the DT for peripherals from the DT
 for the CPU

The set of peripherals remained constant across bcm2835 (Raspberry Pi
1) and bcm2836 (Raspberry Pi 2), but the CPU was swapped out.  Split
the files so that we can include just peripheral setup in 2836.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm2835.dtsi | 194 +-------------------------------------
 arch/arm/boot/dts/bcm283x.dtsi | 205 +++++++++++++++++++++++++++++++++++++++++
 2 files changed, 206 insertions(+), 193 deletions(-)
 create mode 100644 arch/arm/boot/dts/bcm283x.dtsi

diff --git a/arch/arm/boot/dts/bcm2835.dtsi b/arch/arm/boot/dts/bcm2835.dtsi
index aef64de..b83b326 100644
--- a/arch/arm/boot/dts/bcm2835.dtsi
+++ b/arch/arm/boot/dts/bcm2835.dtsi
@@ -1,206 +1,14 @@
-#include <dt-bindings/pinctrl/bcm2835.h>
-#include <dt-bindings/clock/bcm2835.h>
-#include "skeleton.dtsi"
+#include "bcm283x.dtsi"
 
 / {
 	compatible = "brcm,bcm2835";
-	model = "BCM2835";
-	interrupt-parent = <&intc>;
-
-	chosen {
-		bootargs = "earlyprintk console=ttyAMA0";
-	};
 
 	soc {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <1>;
 		ranges = <0x7e000000 0x20000000 0x02000000>;
 		dma-ranges = <0x40000000 0x00000000 0x20000000>;
 
-		timer@7e003000 {
-			compatible = "brcm,bcm2835-system-timer";
-			reg = <0x7e003000 0x1000>;
-			interrupts = <1 0>, <1 1>, <1 2>, <1 3>;
-			/* This could be a reference to BCM2835_CLOCK_TIMER,
-			 * but we don't have the driver using the common clock
-			 * support yet.
-			 */
-			clock-frequency = <1000000>;
-		};
-
-		dma: dma@7e007000 {
-			compatible = "brcm,bcm2835-dma";
-			reg = <0x7e007000 0xf00>;
-			interrupts = <1 16>,
-				     <1 17>,
-				     <1 18>,
-				     <1 19>,
-				     <1 20>,
-				     <1 21>,
-				     <1 22>,
-				     <1 23>,
-				     <1 24>,
-				     <1 25>,
-				     <1 26>,
-				     <1 27>,
-				     <1 28>;
-
-			#dma-cells = <1>;
-			brcm,dma-channel-mask = <0x7f35>;
-		};
-
-		intc: interrupt-controller@7e00b200 {
-			compatible = "brcm,bcm2835-armctrl-ic";
-			reg = <0x7e00b200 0x200>;
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		watchdog@7e100000 {
-			compatible = "brcm,bcm2835-pm-wdt";
-			reg = <0x7e100000 0x28>;
-		};
-
-		clocks: cprman@7e101000 {
-			compatible = "brcm,bcm2835-cprman";
-			#clock-cells = <1>;
-			reg = <0x7e101000 0x2000>;
-
-			/* CPRMAN derives everything from the platform's
-			 * oscillator.
-			 */
-			clocks = <&clk_osc>;
-		};
-
-		rng@7e104000 {
-			compatible = "brcm,bcm2835-rng";
-			reg = <0x7e104000 0x10>;
-		};
-
-		mailbox: mailbox@7e00b800 {
-			compatible = "brcm,bcm2835-mbox";
-			reg = <0x7e00b880 0x40>;
-			interrupts = <0 1>;
-			#mbox-cells = <0>;
-		};
-
-		gpio: gpio@7e200000 {
-			compatible = "brcm,bcm2835-gpio";
-			reg = <0x7e200000 0xb4>;
-			/*
-			 * The GPIO IP block is designed for 3 banks of GPIOs.
-			 * Each bank has a GPIO interrupt for itself.
-			 * There is an overall "any bank" interrupt.
-			 * In order, these are GIC interrupts 17, 18, 19, 20.
-			 * Since the BCM2835 only has 2 banks, the 2nd bank
-			 * interrupt output appears to be mirrored onto the
-			 * 3rd bank's interrupt signal.
-			 * So, a bank0 interrupt shows up on 17, 20, and
-			 * a bank1 interrupt shows up on 18, 19, 20!
-			 */
-			interrupts = <2 17>, <2 18>, <2 19>, <2 20>;
-
-			gpio-controller;
-			#gpio-cells = <2>;
-
-			interrupt-controller;
-			#interrupt-cells = <2>;
-		};
-
-		uart0: uart@7e201000 {
-			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
-			reg = <0x7e201000 0x1000>;
-			interrupts = <2 25>;
-			clocks = <&clocks BCM2835_CLOCK_UART>,
-				 <&clocks BCM2835_CLOCK_VPU>;
-			clock-names = "uartclk", "apb_pclk";
-			arm,primecell-periphid = <0x00241011>;
-		};
-
-		i2s: i2s@7e203000 {
-			compatible = "brcm,bcm2835-i2s";
-			reg = <0x7e203000 0x20>,
-			      <0x7e101098 0x02>;
-
-			dmas = <&dma 2>,
-			       <&dma 3>;
-			dma-names = "tx", "rx";
-			status = "disabled";
-		};
-
-		spi: spi@7e204000 {
-			compatible = "brcm,bcm2835-spi";
-			reg = <0x7e204000 0x1000>;
-			interrupts = <2 22>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		i2c0: i2c@7e205000 {
-			compatible = "brcm,bcm2835-i2c";
-			reg = <0x7e205000 0x1000>;
-			interrupts = <2 21>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		sdhci: sdhci@7e300000 {
-			compatible = "brcm,bcm2835-sdhci";
-			reg = <0x7e300000 0x100>;
-			interrupts = <2 30>;
-			clocks = <&clocks BCM2835_CLOCK_EMMC>;
-			status = "disabled";
-		};
-
-		i2c1: i2c@7e804000 {
-			compatible = "brcm,bcm2835-i2c";
-			reg = <0x7e804000 0x1000>;
-			interrupts = <2 21>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		i2c2: i2c@7e805000 {
-			compatible = "brcm,bcm2835-i2c";
-			reg = <0x7e805000 0x1000>;
-			interrupts = <2 21>;
-			clocks = <&clocks BCM2835_CLOCK_VPU>;
-			#address-cells = <1>;
-			#size-cells = <0>;
-			status = "disabled";
-		};
-
-		usb@7e980000 {
-			compatible = "brcm,bcm2835-usb";
-			reg = <0x7e980000 0x10000>;
-			interrupts = <1 9>;
-		};
-
 		arm-pmu {
 			compatible = "arm,arm1176-pmu";
 		};
 	};
-
-	clocks {
-		compatible = "simple-bus";
-		#address-cells = <1>;
-		#size-cells = <0>;
-
-		/* The oscillator is the root of the clock tree. */
-		clk_osc: clock@3 {
-			compatible = "fixed-clock";
-			reg = <3>;
-			#clock-cells = <0>;
-			clock-output-names = "osc";
-			clock-frequency = <19200000>;
-		};
-
-	};
 };
diff --git a/arch/arm/boot/dts/bcm283x.dtsi b/arch/arm/boot/dts/bcm283x.dtsi
new file mode 100644
index 0000000..8a7e727
--- /dev/null
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -0,0 +1,205 @@
+#include <dt-bindings/pinctrl/bcm2835.h>
+#include <dt-bindings/clock/bcm2835.h>
+#include "skeleton.dtsi"
+
+/* This include file covers the common peripherals and configuration between
+ * bcm2835 and bcm2836 implementations, leaving the CPU configuration to
+ * bcm2835.dtsi and bcm2836.dtsi.
+ */
+
+/ {
+	compatible = "brcm,bcm2835";
+	model = "BCM2835";
+	interrupt-parent = <&intc>;
+
+	chosen {
+		bootargs = "earlyprintk console=ttyAMA0";
+	};
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+
+		timer@7e003000 {
+			compatible = "brcm,bcm2835-system-timer";
+			reg = <0x7e003000 0x1000>;
+			interrupts = <1 0>, <1 1>, <1 2>, <1 3>;
+			/* This could be a reference to BCM2835_CLOCK_TIMER,
+			 * but we don't have the driver using the common clock
+			 * support yet.
+			 */
+			clock-frequency = <1000000>;
+		};
+
+		dma: dma@7e007000 {
+			compatible = "brcm,bcm2835-dma";
+			reg = <0x7e007000 0xf00>;
+			interrupts = <1 16>,
+				     <1 17>,
+				     <1 18>,
+				     <1 19>,
+				     <1 20>,
+				     <1 21>,
+				     <1 22>,
+				     <1 23>,
+				     <1 24>,
+				     <1 25>,
+				     <1 26>,
+				     <1 27>,
+				     <1 28>;
+
+			#dma-cells = <1>;
+			brcm,dma-channel-mask = <0x7f35>;
+		};
+
+		intc: interrupt-controller@7e00b200 {
+			compatible = "brcm,bcm2835-armctrl-ic";
+			reg = <0x7e00b200 0x200>;
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		watchdog@7e100000 {
+			compatible = "brcm,bcm2835-pm-wdt";
+			reg = <0x7e100000 0x28>;
+		};
+
+		clocks: cprman@7e101000 {
+			compatible = "brcm,bcm2835-cprman";
+			#clock-cells = <1>;
+			reg = <0x7e101000 0x2000>;
+
+			/* CPRMAN derives everything from the platform's
+			 * oscillator.
+			 */
+			clocks = <&clk_osc>;
+		};
+
+		rng@7e104000 {
+			compatible = "brcm,bcm2835-rng";
+			reg = <0x7e104000 0x10>;
+		};
+
+		mailbox: mailbox@7e00b800 {
+			compatible = "brcm,bcm2835-mbox";
+			reg = <0x7e00b880 0x40>;
+			interrupts = <0 1>;
+			#mbox-cells = <0>;
+		};
+
+		gpio: gpio@7e200000 {
+			compatible = "brcm,bcm2835-gpio";
+			reg = <0x7e200000 0xb4>;
+			/*
+			 * The GPIO IP block is designed for 3 banks of GPIOs.
+			 * Each bank has a GPIO interrupt for itself.
+			 * There is an overall "any bank" interrupt.
+			 * In order, these are GIC interrupts 17, 18, 19, 20.
+			 * Since the BCM2835 only has 2 banks, the 2nd bank
+			 * interrupt output appears to be mirrored onto the
+			 * 3rd bank's interrupt signal.
+			 * So, a bank0 interrupt shows up on 17, 20, and
+			 * a bank1 interrupt shows up on 18, 19, 20!
+			 */
+			interrupts = <2 17>, <2 18>, <2 19>, <2 20>;
+
+			gpio-controller;
+			#gpio-cells = <2>;
+
+			interrupt-controller;
+			#interrupt-cells = <2>;
+		};
+
+		uart0: uart@7e201000 {
+			compatible = "brcm,bcm2835-pl011", "arm,pl011", "arm,primecell";
+			reg = <0x7e201000 0x1000>;
+			interrupts = <2 25>;
+			clocks = <&clocks BCM2835_CLOCK_UART>,
+				 <&clocks BCM2835_CLOCK_VPU>;
+			clock-names = "uartclk", "apb_pclk";
+			arm,primecell-periphid = <0x00241011>;
+		};
+
+		i2s: i2s@7e203000 {
+			compatible = "brcm,bcm2835-i2s";
+			reg = <0x7e203000 0x20>,
+			      <0x7e101098 0x02>;
+
+			dmas = <&dma 2>,
+			       <&dma 3>;
+			dma-names = "tx", "rx";
+			status = "disabled";
+		};
+
+		spi: spi@7e204000 {
+			compatible = "brcm,bcm2835-spi";
+			reg = <0x7e204000 0x1000>;
+			interrupts = <2 22>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c0: i2c@7e205000 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e205000 0x1000>;
+			interrupts = <2 21>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		sdhci: sdhci@7e300000 {
+			compatible = "brcm,bcm2835-sdhci";
+			reg = <0x7e300000 0x100>;
+			interrupts = <2 30>;
+			clocks = <&clocks BCM2835_CLOCK_EMMC>;
+			status = "disabled";
+		};
+
+		i2c1: i2c@7e804000 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e804000 0x1000>;
+			interrupts = <2 21>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		i2c2: i2c@7e805000 {
+			compatible = "brcm,bcm2835-i2c";
+			reg = <0x7e805000 0x1000>;
+			interrupts = <2 21>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+		};
+
+		usb@7e980000 {
+			compatible = "brcm,bcm2835-usb";
+			reg = <0x7e980000 0x10000>;
+			interrupts = <1 9>;
+		};
+	};
+
+	clocks {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		/* The oscillator is the root of the clock tree. */
+		clk_osc: clock@3 {
+			compatible = "fixed-clock";
+			reg = <3>;
+			#clock-cells = <0>;
+			clock-output-names = "osc";
+			clock-frequency = <19200000>;
+		};
+
+	};
+};
-- 
2.3.10

