From 358875fd52ab8f00f66328cbf1a1d2486f265829 Mon Sep 17 00:00:00 2001
From: Jay Cornwall <jay@jcornwall.me>
Date: Wed, 10 Feb 2016 15:48:01 -0600
Subject: iommu/amd: Apply workaround for ATS write permission check

From: Jay Cornwall <jay@jcornwall.me>

commit 358875fd52ab8f00f66328cbf1a1d2486f265829 upstream.

The AMD Family 15h Models 30h-3Fh (Kaveri) BIOS and Kernel Developer's
Guide omitted part of the BIOS IOMMU L2 register setup specification.
Without this setup the IOMMU L2 does not fully respect write permissions
when handling an ATS translation request.

The IOMMU L2 will set PTE dirty bit when handling an ATS translation with
write permission request, even when PTE RW bit is clear. This may occur by
direct translation (which would cause a PPR) or by prefetch request from
the ATC.

This is observed in practice when the IOMMU L2 modifies a PTE which maps a
pagecache page. The ext4 filesystem driver BUGs when asked to writeback
these (non-modified) pages.

Enable ATS write permission check in the Kaveri IOMMU L2 if BIOS has not.

Signed-off-by: Jay Cornwall <jay@jcornwall.me>
Signed-off-by: Joerg Roedel <jroedel@suse.de>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>

---
 drivers/iommu/amd_iommu_init.c |   29 +++++++++++++++++++++++++++++
 1 file changed, 29 insertions(+)

--- a/drivers/iommu/amd_iommu_init.c
+++ b/drivers/iommu/amd_iommu_init.c
@@ -1016,6 +1016,34 @@ static void amd_iommu_erratum_746_workar
 }
 
 /*
+ * Family15h Model 30h-3fh (IOMMU Mishandles ATS Write Permission)
+ * Workaround:
+ *     BIOS should enable ATS write permission check by setting
+ *     L2_DEBUG_3[AtsIgnoreIWDis](D0F2xF4_x47[0]) = 1b
+ */
+static void amd_iommu_ats_write_check_workaround(struct amd_iommu *iommu)
+{
+	u32 value;
+
+	if ((boot_cpu_data.x86 != 0x15) ||
+	    (boot_cpu_data.x86_model < 0x30) ||
+	    (boot_cpu_data.x86_model > 0x3f))
+		return;
+
+	/* Test L2_DEBUG_3[AtsIgnoreIWDis] == 1 */
+	value = iommu_read_l2(iommu, 0x47);
+
+	if (value & BIT(0))
+		return;
+
+	/* Set L2_DEBUG_3[AtsIgnoreIWDis] = 1 */
+	iommu_write_l2(iommu, 0x47, value | BIT(0));
+
+	pr_info("AMD-Vi: Applying ATS write check workaround for IOMMU at %s\n",
+		dev_name(&iommu->dev->dev));
+}
+
+/*
  * This function clues the initialization function for one IOMMU
  * together and also allocates the command buffer and programs the
  * hardware. It does NOT enable the IOMMU. This is done afterwards.
@@ -1284,6 +1312,7 @@ static int iommu_init_pci(struct amd_iom
 	}
 
 	amd_iommu_erratum_746_workaround(iommu);
+	amd_iommu_ats_write_check_workaround(iommu);
 
 	iommu->iommu_dev = iommu_device_create(&iommu->dev->dev, iommu,
 					       amd_iommu_groups, "ivhd%d",
