From c1be3c1fc6178ca48750b4e66f1acb7c22b64997 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Wed, 16 Dec 2015 15:55:14 -0800
Subject: [PATCH 2/3] ARM: bcm2835: Add a compat string for bcm2836 machine
 probe

Supporting the 2836 requires using the new interrupt controller, which
we have support for.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/mach-bcm/board_bcm2835.c | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm/mach-bcm/board_bcm2835.c b/arch/arm/mach-bcm/board_bcm2835.c
index 0f7b9ea..834d676 100644
--- a/arch/arm/mach-bcm/board_bcm2835.c
+++ b/arch/arm/mach-bcm/board_bcm2835.c
@@ -36,7 +36,12 @@ static void __init bcm2835_init(void)
 }
 
 static const char * const bcm2835_compat[] = {
+#ifdef CONFIG_ARCH_MULTI_V6
 	"brcm,bcm2835",
+#endif
+#ifdef CONFIG_ARCH_MULTI_V7
+	"brcm,bcm2836",
+#endif
 	NULL
 };
 
-- 
2.3.10

