From c33319cd945001741d1b381655c8b7310d756163 Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Thu, 16 Apr 2015 15:26:45 -0700
Subject: [PATCH 3/4] ARM: bcm2835: Add devicetree for bcm2836 and Raspberry Pi
 2 B

The Pi 2 B ends up like a Pi 1 B+, with the same peripherals and
pinout, but the CPU and memory layout changed to use the 2836.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/Makefile            |  3 +-
 arch/arm/boot/dts/bcm2836-rpi-2-b.dts | 35 ++++++++++++++++
 arch/arm/boot/dts/bcm2836.dtsi        | 78 +++++++++++++++++++++++++++++++++++
 3 files changed, 115 insertions(+), 1 deletion(-)
 create mode 100644 arch/arm/boot/dts/bcm2836-rpi-2-b.dts
 create mode 100644 arch/arm/boot/dts/bcm2836.dtsi

diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index 30bbc37..54e8f6b 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -60,7 +60,8 @@ dtb-$(CONFIG_ARCH_BCM2835) += \
 	bcm2835-rpi-b.dtb \
 	bcm2835-rpi-b-rev2.dtb \
 	bcm2835-rpi-b-plus.dtb \
-	bcm2835-rpi-a-plus.dtb
+	bcm2835-rpi-a-plus.dtb \
+	bcm2836-rpi-2-b.dtb
 dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm4708-asus-rt-ac56u.dtb \
 	bcm4708-asus-rt-ac68u.dtb \
diff --git a/arch/arm/boot/dts/bcm2836-rpi-2-b.dts b/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
new file mode 100644
index 0000000..ff94666
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2836-rpi-2-b.dts
@@ -0,0 +1,35 @@
+/dts-v1/;
+#include "bcm2836.dtsi"
+#include "bcm2835-rpi.dtsi"
+
+/ {
+	compatible = "raspberrypi,2-model-b", "brcm,bcm2836";
+	model = "Raspberry Pi 2 Model B";
+
+	memory {
+		reg = <0 0x40000000>;
+	};
+
+	leds {
+		act {
+			gpios = <&gpio 47 0>;
+		};
+
+		pwr {
+			label = "PWR";
+			gpios = <&gpio 35 0>;
+			default-state = "keep";
+			linux,default-trigger = "default-on";
+		};
+	};
+};
+
+&gpio {
+	pinctrl-0 = <&gpioout &alt0 &i2s_alt0 &alt3>;
+
+	/* I2S interface */
+	i2s_alt0: i2s_alt0 {
+		brcm,pins = <18 19 20 21>;
+		brcm,function = <BCM2835_FSEL_ALT0>;
+	};
+};
diff --git a/arch/arm/boot/dts/bcm2836.dtsi b/arch/arm/boot/dts/bcm2836.dtsi
new file mode 100644
index 0000000..9d0651d
--- /dev/null
+++ b/arch/arm/boot/dts/bcm2836.dtsi
@@ -0,0 +1,78 @@
+#include "bcm283x.dtsi"
+
+/ {
+	compatible = "brcm,bcm2836";
+
+	soc {
+		ranges = <0x7e000000 0x3f000000 0x1000000>,
+			 <0x40000000 0x40000000 0x00001000>;
+		dma-ranges = <0xc0000000 0x00000000 0x3f000000>;
+
+		local_intc: local_intc {
+			compatible = "brcm,bcm2836-l1-intc";
+			reg = <0x40000000 0x100>;
+			interrupt-controller;
+			#interrupt-cells = <1>;
+			interrupt-parent = <&local_intc>;
+		};
+
+		arm-pmu {
+			compatible = "arm,cortex-a7-pmu";
+			interrupt-parent = <&local_intc>;
+			interrupts = <9>;
+		};
+	};
+
+	timer {
+		compatible = "arm,armv7-timer";
+		interrupt-parent = <&local_intc>;
+		interrupts = <0>, // PHYS_SECURE_PPI
+			     <1>, // PHYS_NONSECURE_PPI
+			     <3>, // VIRT_PPI
+			     <2>; // HYP_PPI
+		always-on;
+	};
+
+	cpus: cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		v7_cpu0: cpu@0 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf00>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu1: cpu@1 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf01>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu2: cpu@2 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf02>;
+			clock-frequency = <800000000>;
+		};
+
+		v7_cpu3: cpu@3 {
+			device_type = "cpu";
+			compatible = "arm,cortex-a7";
+			reg = <0xf03>;
+			clock-frequency = <800000000>;
+		};
+	};
+};
+
+/* Make the BCM2835-style global interrupt controller be a child of the
+ * CPU-local interrupt controller.
+ */
+&intc {
+	compatible = "brcm,bcm2836-armctrl-ic";
+	reg = <0x7e00b200 0x200>;
+	interrupt-parent = <&local_intc>;
+	interrupts = <8>;
+};
-- 
2.3.10

