
This patch adds missing module aliases for the old ieee1394 stack
to make it easier for endusers.

Note: firewire-sbp2 and firewire-ohci already contains the needed aliases.

Signed-off-by: Thomas Backlund <tmb@mageia.org>

diff -Nurp linux-2.6.38.4/drivers/firewire/core-transaction.c linux-2.6.38.4.fw/drivers/firewire/core-transaction.c
--- linux-2.6.38.4/drivers/firewire/core-transaction.c	2011-03-15 03:20:32.000000000 +0200
+++ linux-2.6.38.4.fw/drivers/firewire/core-transaction.c	2011-04-22 16:22:28.461386738 +0300
@@ -1174,6 +1174,9 @@ static struct fw_address_handler registe
 MODULE_AUTHOR("Kristian Hoegsberg <krh@bitplanet.net>");
 MODULE_DESCRIPTION("Core IEEE1394 transaction logic");
 MODULE_LICENSE("GPL");
+MODULE_ALIAS("ieee1394");
+MODULE_ALIAS("raw1394");
+MODULE_ALIAS("video1394");
 
 static const u32 vendor_textual_descriptor[] = {
 	/* textual descriptor leaf () */
diff -Nurp linux-2.6.38.4/drivers/firewire/net.c linux-2.6.38.4.fw/drivers/firewire/net.c
--- linux-2.6.38.4/drivers/firewire/net.c	2011-03-15 03:20:32.000000000 +0200
+++ linux-2.6.38.4.fw/drivers/firewire/net.c	2011-04-22 16:20:34.008883920 +0300
@@ -1719,3 +1719,4 @@ MODULE_AUTHOR("Jay Fenlason <fenlason@re
 MODULE_DESCRIPTION("IP over IEEE1394 as per RFC 2734/3146");
 MODULE_LICENSE("GPL");
 MODULE_DEVICE_TABLE(ieee1394, fwnet_id_table);
+MODULE_ALIAS("eth1394");
