From 53b6084357a44d7c34044504e1bf149d9156934f Mon Sep 17 00:00:00 2001
From: Eric Anholt <eric@anholt.net>
Date: Tue, 15 Dec 2015 15:35:59 -0800
Subject: [PATCH 4/4] ARM: bcm2835: Add the auxiliary clocks to the device
 tree.

These will be used for enabling UART1, SPI1, and SPI2.

Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/boot/dts/bcm283x.dtsi | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm/boot/dts/bcm283x.dtsi b/arch/arm/boot/dts/bcm283x.dtsi
index 8a7e727..971e741 100644
--- a/arch/arm/boot/dts/bcm283x.dtsi
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -152,6 +152,13 @@
 			status = "disabled";
 		};
 
+		aux: aux@0x7e215000 {
+			compatible = "brcm,bcm2835-aux";
+			#clock-cells = <1>;
+			reg = <0x7e215000 0x8>;
+			clocks = <&clocks BCM2835_CLOCK_VPU>;
+		};
+
 		sdhci: sdhci@7e300000 {
 			compatible = "brcm,bcm2835-sdhci";
 			reg = <0x7e300000 0x100>;
-- 
2.3.10

