From b63074fccbeb81e46b2553a200de54ff3bfadd10 Mon Sep 17 00:00:00 2001
From: Martin Sperl <kernel@martin.sperl.org>
Date: Fri, 11 Sep 2015 11:22:06 +0000
Subject: [PATCH 2/2] ARM: bcm2835: enable auxiliary spi driver in defconfig

add the auxiliary spi driver to the default config

Signed-off-by: Martin Sperl <kernel@martin.sperl.org>
Signed-off-by: Eric Anholt <eric@anholt.net>
---
 arch/arm/configs/bcm2835_defconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm/configs/bcm2835_defconfig b/arch/arm/configs/bcm2835_defconfig
index 0fda844..72def20 100644
--- a/arch/arm/configs/bcm2835_defconfig
+++ b/arch/arm/configs/bcm2835_defconfig
@@ -69,6 +69,7 @@ CONFIG_I2C_CHARDEV=y
 CONFIG_I2C_BCM2835=y
 CONFIG_SPI=y
 CONFIG_SPI_BCM2835=y
+CONFIG_SPI_BCM2835AUX=y
 CONFIG_GPIO_SYSFS=y
 # CONFIG_HWMON is not set
 CONFIG_WATCHDOG=y
-- 
2.3.10

