
splash.lss

05Welcome to XCP-ng.

  - To install or upgrade press the 0e<ENTER>05 key.
  - To install or upgrade without a serial console, type 
    0eno-serial <ENTER>05.
  - To install or upgrade in safe mode, type 0esafe <ENTER>05.
  - To install or upgrade to a multipathed root disk, type 0emultipath <ENTER>05.
  - To boot into a shell prompt, type 0eshell <ENTER>05.
    (This is an advanced option and should be used with care and as
     directed by a Technical Support Representative.)
  - To perform a memory test, type 0ememtest <ENTER>05.

0f[F1-Standard] [F2-Advanced]05
