From b3049cfd11aa0f3c124ed8f87e98a200201ecbdc Mon Sep 17 00:00:00 2001
From: Mate Kukri <km@mkukri.xyz>
Date: Fri, 22 Nov 2024 21:26:48 +0000
Subject: [PATCH 3/8] soc/intel/skylake: Enable 4E/4F PNP I/O ports in
 bootblock

Change-Id: I57c9d8a9513a268e2ca6a0abd1306cd038598173
Signed-off-by: Mate Kukri <km@mkukri.xyz>
---
 src/soc/intel/skylake/bootblock/pch.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/src/soc/intel/skylake/bootblock/pch.c b/src/soc/intel/skylake/bootblock/pch.c
index df00bb85a9..beaece960b 100644
--- a/src/soc/intel/skylake/bootblock/pch.c
+++ b/src/soc/intel/skylake/bootblock/pch.c
@@ -100,8 +100,8 @@ static void soc_config_pwrmbase(void)
 
 void pch_early_iorange_init(void)
 {
-	uint16_t io_enables = LPC_IOE_SUPERIO_2E_2F | LPC_IOE_KBC_60_64 |
-			LPC_IOE_EC_62_66;
+	uint16_t io_enables = LPC_IOE_EC_4E_4F | LPC_IOE_SUPERIO_2E_2F |
+			LPC_IOE_KBC_60_64 | LPC_IOE_EC_62_66;
 
 	const config_t *config = config_of_soc();
 
-- 
2.39.5

