From ce7d65790b9b8656ebbaa0ca715adff6a9c25588 Mon Sep 17 00:00:00 2001
From: Leah Rowe <info@minifree.org>
Date: Sat, 4 May 2024 02:00:53 +0100
Subject: [PATCH 26/51] nb/haswell: lock policy regs when disabling IOMMU

Angel Pons told me I should do it. See comments here:
https://review.coreboot.org/c/coreboot/+/81016

I see no harm in complying with the request. I'll merge
this into the main patch at a later date and try to
get this upstreamed.

Just a reminder: on Optiplex 9020 variants, Xorg locks up
under Linux when tested with a graphics card; disabling
IOMMU works around the issue. Intel graphics work just fine
with IOMMU turned on. Libreboot disables IOMMU by default,
on the 9020, so that users can install graphics cards easily.

Signed-off-by: Leah Rowe <info@minifree.org>
---
 src/northbridge/intel/haswell/early_init.c | 15 +++++++--------
 1 file changed, 7 insertions(+), 8 deletions(-)

diff --git a/src/northbridge/intel/haswell/early_init.c b/src/northbridge/intel/haswell/early_init.c
index 1a7e0b1076..e9506ee830 100644
--- a/src/northbridge/intel/haswell/early_init.c
+++ b/src/northbridge/intel/haswell/early_init.c
@@ -160,17 +160,16 @@ static void haswell_setup_iommu(void)
 	const u32 capid0_a = pci_read_config32(HOST_BRIDGE, CAPID0_A);
 	u8 enable_iommu = get_uint_option("iommu", 1);
 
-	if (!enable_iommu)
-		return;
-
 	if (capid0_a & VTD_DISABLE)
 		return;
 
-	/* Setup BARs: zeroize top 32 bits; set enable bit */
-	mchbar_write32(GFXVTBAR + 4, GFXVT_BASE_ADDRESS >> 32);
-	mchbar_write32(GFXVTBAR + 0, GFXVT_BASE_ADDRESS | 1);
-	mchbar_write32(VTVC0BAR + 4, VTVC0_BASE_ADDRESS >> 32);
-	mchbar_write32(VTVC0BAR + 0, VTVC0_BASE_ADDRESS | 1);
+	if (enable_iommu) {
+		/* Setup BARs: zeroize top 32 bits; set enable bit */
+		mchbar_write32(GFXVTBAR + 4, GFXVT_BASE_ADDRESS >> 32);
+		mchbar_write32(GFXVTBAR + 0, GFXVT_BASE_ADDRESS | 1);
+		mchbar_write32(VTVC0BAR + 4, VTVC0_BASE_ADDRESS >> 32);
+		mchbar_write32(VTVC0BAR + 0, VTVC0_BASE_ADDRESS | 1);
+	}
 
 	/* Set L3HIT2PEND_DIS, lock GFXVTBAR policy config registers */
 	u32 reg32;
-- 
2.39.5

