From 84d7f3201eb4492acd7d290a02d19c4850c85791 Mon Sep 17 00:00:00 2001
From: Nicholas Chin <nic.c3.14@gmail.com>
Date: Thu, 26 Oct 2017 21:26:43 +0800
Subject: [PATCH 17/51] mb/dell: Add Latitude E6230 (Ivy Bridge)

This was adapted from CB:22693 from Iru Cai, which was based on
autoport. I do not physically have this system. Someone with physical
access to an E6230 running version A11 of the vendor firmware sent me
the VBT after running the command `intelvbttool --inlegacy --outvbt
data.vbt`. This new version of the port has not yet been tested.

The EC is the SMSC MEC5055, which seems to be compatible with the
existing MEC5035 code. As with the other Dell systems with this EC, this
board is assumed to be internally flashable using an EC command that
tells it to pull the FDO pin low on the next boot, which also tells the
vendor firmware to disable all write protections to the flash [1].

[1] https://gitlab.com/nic3-14159/dell-flash-unlock

Original-Change-Id: I8cdc01e902e670310628809416290045c2102340
Change-Id: I32927beea7c29b96a851ab77ed15b0160f16d369
Signed-off-by: Nicholas Chin <nic.c3.14@gmail.com>
---
 src/mainboard/dell/snb_ivb_latitude/Kconfig   |  11 +-
 .../dell/snb_ivb_latitude/Kconfig.name        |   3 +
 .../snb_ivb_latitude/variants/e6230/data.vbt  | Bin 0 -> 4280 bytes
 .../variants/e6230/early_init.c               |  12 ++
 .../snb_ivb_latitude/variants/e6230/gpio.c    | 193 ++++++++++++++++++
 .../variants/e6230/hda_verb.c                 |  32 +++
 .../variants/e6230/overridetree.cb            |  40 ++++
 7 files changed, 290 insertions(+), 1 deletion(-)
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6230/data.vbt
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6230/early_init.c
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6230/gpio.c
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6230/hda_verb.c
 create mode 100644 src/mainboard/dell/snb_ivb_latitude/variants/e6230/overridetree.cb

diff --git a/src/mainboard/dell/snb_ivb_latitude/Kconfig b/src/mainboard/dell/snb_ivb_latitude/Kconfig
index 49bf225fe2..f6e097930b 100644
--- a/src/mainboard/dell/snb_ivb_latitude/Kconfig
+++ b/src/mainboard/dell/snb_ivb_latitude/Kconfig
@@ -56,6 +56,12 @@ config BOARD_DELL_LATITUDE_E5530
 	select BOARD_ROMSIZE_KB_12288
 	select SOUTHBRIDGE_INTEL_C216
 
+config BOARD_DELL_LATITUDE_E6230
+	select BOARD_DELL_SNB_IVB_LATITUDE_COMMON
+	select BOARD_ROMSIZE_KB_12288
+	select MAINBOARD_USES_IFD_GBE_REGION
+	select SOUTHBRIDGE_INTEL_C216
+
 config BOARD_DELL_LATITUDE_E6330
 	select BOARD_DELL_SNB_IVB_LATITUDE_COMMON
 	select BOARD_ROMSIZE_KB_12288
@@ -90,6 +96,7 @@ config MAINBOARD_PART_NUMBER
 	default "Latitude E6420" if BOARD_DELL_LATITUDE_E6420
 	default "Latitude E6520" if BOARD_DELL_LATITUDE_E6520
 	default "Latitude E5530" if BOARD_DELL_LATITUDE_E5530
+	default "Latitude E6230" if BOARD_DELL_LATITUDE_E6230
 	default "Latitude E6330" if BOARD_DELL_LATITUDE_E6330
 	default "Latitude E6430" if BOARD_DELL_LATITUDE_E6430
 	default "Latitude E6530" if BOARD_DELL_LATITUDE_E6530
@@ -108,6 +115,7 @@ config VARIANT_DIR
 	default "e6420" if BOARD_DELL_LATITUDE_E6420
 	default "e6520" if BOARD_DELL_LATITUDE_E6520
 	default "e5530" if BOARD_DELL_LATITUDE_E5530
+	default "e6230" if BOARD_DELL_LATITUDE_E6230
 	default "e6330" if BOARD_DELL_LATITUDE_E6330
 	default "e6430" if BOARD_DELL_LATITUDE_E6430
 	default "e6530" if BOARD_DELL_LATITUDE_E6530
@@ -121,7 +129,8 @@ config VGA_BIOS_ID
 		|| BOARD_DELL_LATITUDE_E5520 \
 		|| BOARD_DELL_LATITUDE_E6220 \
 		|| BOARD_DELL_LATITUDE_E6320
-	default "8086,0166" if BOARD_DELL_LATITUDE_E6430 \
+	default "8086,0166" if BOARD_DELL_LATITUDE_E6230 \
+		|| BOARD_DELL_LATITUDE_E6430 \
 		|| BOARD_DELL_LATITUDE_E6530
 
 endif
diff --git a/src/mainboard/dell/snb_ivb_latitude/Kconfig.name b/src/mainboard/dell/snb_ivb_latitude/Kconfig.name
index d6fc8eb224..cb7bbd5cdb 100644
--- a/src/mainboard/dell/snb_ivb_latitude/Kconfig.name
+++ b/src/mainboard/dell/snb_ivb_latitude/Kconfig.name
@@ -21,6 +21,9 @@ config BOARD_DELL_LATITUDE_E6520
 config BOARD_DELL_LATITUDE_E5530
 	bool "Latitude E5530"
 
+config BOARD_DELL_LATITUDE_E6230
+	bool "Latitude E6230"
+
 config BOARD_DELL_LATITUDE_E6330
 	bool "Latitude E6330"
 
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6230/data.vbt b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/data.vbt
new file mode 100644
index 0000000000000000000000000000000000000000..45ce8f435eea647a0bddaab3fd1e9282c87afc66
GIT binary patch
literal 4280
zcmdT{Yiu0V75-*tAG5PFyX&zDekA7P<*tbx&o1`j23L%CmvkLWvN7(mLa6alZ?J`9
zo3#m4YVlG`2;w12Ajppt<qra(R;8*G@uw*8gIcsg2vxi!q_pBkmGUD$s9IGi+jD1T
zO`Kg43n@JA>~|mMp8L%`XU@4ZyCa_(r`z|Z`bP4p-rEkOMn-R;Ntk#o`b)0sOKRl6
z?T0eM<HLtiqX*Kr(o5Kc<Iyk90h5ws=!y8i;K=M^X(l$-Eoeyyj>ZS*@LZWP#hD{>
z<r2jcJ;b8e!oAb;^QB2D#7*krI^IpA=?ra8?xvqj6=&}$QL2a1J(QuD($UfkElf=x
zUM!UtXmO4PP4h^;&)jWJvd(Pj0lIs7wpgAnE!1!MB1w8~{^#ZCd!`mCmhPs6X_~zW
zGae^<%aoog&+n$;nHd@rItw&bS}2u|mL_-Ws;&ZOWW_51k`IALAW8pAz~@C!!B)bs
z1x-OrK~}*8L07Po(5+xZL6I<}phTEf5QRsVJYHa{f^AWEV+2@lvrPVS%snsOn?N)w
zpKbvwOnk&Q_6Y?aB;r1=!TYwts;yA@BnbFfECo!7JVJq7g^yhYMUV;wlBjksp(hI2
z^<}E7r698{-pw!*{mH>SLslxYH@j~%H#VLx+<8~!;a@$n+>Q%xHrQ8KGI21_iL4sI
zF*$}m$R7Mr9z@Z*ir@Q9eClsSmC+t(g`q~VQ&nIxZenav_^Buc78s8*o@e|<QE{4a
zhVeGz1IFJN|784&5eTYiVstQeGWr-lWTY9lG45a#8TT^oXDl%uXFS9BHN$^DE>t}g
z1Z-O>lG`>pEuvmL-HpmgSANo!2hWQq2B>Zua$8%tfvQ>!1n@=m9ri_4`H|Rx#SH9n
zDdRF_-FDP&WjW`L$GK%a6x?yO8l2!^g0HJrtA7TknNzCO?|U!wCv2^-5pJ%LW6!+P
z)anX%E>`gP%3Er4c6+J9x=Atk1{Abrr1|WSY3P`SO5j!R5F*vbbQ%AaSHnR_+x&Op
zA%8C-Pk=-Hs+FL90B)E*y3FUTIA1J)&pxRF$tzAkNr7a6_-8v$@j~G~3keqYd5I<T
z`Kb3Q@LKkANhE_aMG_R&<ewt+nVbp5l*3G7mYJEKr<kXS;TA&^G;5`q5b>;y8g^P<
zfWO_D2@EyVVBxnpv*}hgTeeRzWz9BoISh>M%^k`WXG=5ti$_Wu99)~lWE-qubeXNk
zla9Tu=Jhyn5T<3$H#?Hfm-`+(d$7IBDx9cEvNv1i-LEDr>r7438bfkPcKod+mwd22
z%{^(w&NuG)MKl0fTMTXZFJEm~k;KCj*D60g=j!2jsP)<fOUGaEZa`&xE*)?FZuW#-
z8!Of7<|N(^R#xcjmZ&nZ%~{pC5y_T*PB2LdDjuI#Te}-4Qccvj+u4N3TBx|oVy*mP
z<9xfFziy4n?sPv3Sqo7jWMo3>{tzvOjAJ2nB}At~#%f4?FGT+d8LFnXXtYN&Mm06B
z(JwUPX-z$$(d(M=uBLvh@h6#K=;~&jQo1p&t3TCgSvQ{3)l)jXr5hjW>fd!z!bW>o
z-4UjJVdJi_dN@o^hK(1(>dRqzCv2PztLMTLjTqY^YEMMJ{=B#1IV)9~IMg|yl(NPF
zQSfMX`?(b5)))B!zjy0B$ua20CCLTPl^IS&2=T&Zid9-1*K{VAJP?rxjYC+zGDCe*
ziQI7VfF17@3`3W-qCN>lPC5CL_c?p0F<ekqB;g0q3P1R5KNubPsT>TGXaGB3i~{ZE
zr=QtIprytDnU7C*Wj%x0k)O{Y%nUnl%}K%F|J_iVaD&ubW4Qbtx;pZEb9}f^Yd;Ea
zI1Ha{7Yt~z{LAY++1QG{F6*_4WsUziY{x?%I9B}i5-Tphhk8FGm%J<d_0CUoV^%N&
zTe02j+LXk=ZyWoe7L$#wsEY@VC>f!3d-ysG_9>uk%#)4xpxb+ZkJdel#+h}l9j9`1
zt*M!5u?i4YtZ+WECo6$LJF06|G-mMZskGiV*lQJf-ItB+hltI<?{5E<^P=0rL<P+g
z(P)!c<?MlvMK0O~UwZ4*;x|ms(&&#Vn_-4{KM#g~a=;$N2QD7mSX0{t<cf>sId@e&
z-cN<SWA3VKCN6g3lx#+PySpWu*+pw}>vr(fgI)K*zkikg6TDJi?^}ghc*U*%A%EGg
Y$$8Z}9a~<{Q@y10T!W`-d%n2+Kj)*Kg#Z8m

literal 0
HcmV?d00001

diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6230/early_init.c b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/early_init.c
new file mode 100644
index 0000000000..24c1b32467
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/early_init.c
@@ -0,0 +1,12 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <bootblock_common.h>
+#include <device/pci_ops.h>
+#include <ec/dell/mec5035/mec5035.h>
+#include <southbridge/intel/bd82x6x/pch.h>
+
+void bootblock_mainboard_early_init(void)
+{
+	pci_write_config16(PCH_LPC_DEV, LPC_EN, CNF1_LPC_EN | MC_LPC_EN | KBC_LPC_EN);
+	mec5035_early_init();
+}
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6230/gpio.c b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/gpio.c
new file mode 100644
index 0000000000..c07e4b1c56
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/gpio.c
@@ -0,0 +1,193 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <southbridge/intel/common/gpio.h>
+
+static const struct pch_gpio_set1 pch_gpio_set1_mode = {
+	.gpio0 = GPIO_MODE_GPIO,
+	.gpio1 = GPIO_MODE_GPIO,
+	.gpio2 = GPIO_MODE_GPIO,
+	.gpio3 = GPIO_MODE_GPIO,
+	.gpio4 = GPIO_MODE_GPIO,
+	.gpio5 = GPIO_MODE_NATIVE,
+	.gpio6 = GPIO_MODE_GPIO,
+	.gpio7 = GPIO_MODE_GPIO,
+	.gpio8 = GPIO_MODE_GPIO,
+	.gpio9 = GPIO_MODE_NATIVE,
+	.gpio10 = GPIO_MODE_NATIVE,
+	.gpio11 = GPIO_MODE_NATIVE,
+	.gpio12 = GPIO_MODE_NATIVE,
+	.gpio13 = GPIO_MODE_GPIO,
+	.gpio14 = GPIO_MODE_GPIO,
+	.gpio15 = GPIO_MODE_GPIO,
+	.gpio16 = GPIO_MODE_GPIO,
+	.gpio17 = GPIO_MODE_GPIO,
+	.gpio18 = GPIO_MODE_NATIVE,
+	.gpio19 = GPIO_MODE_GPIO,
+	.gpio20 = GPIO_MODE_NATIVE,
+	.gpio21 = GPIO_MODE_GPIO,
+	.gpio22 = GPIO_MODE_GPIO,
+	.gpio23 = GPIO_MODE_NATIVE,
+	.gpio24 = GPIO_MODE_GPIO,
+	.gpio25 = GPIO_MODE_NATIVE,
+	.gpio26 = GPIO_MODE_NATIVE,
+	.gpio27 = GPIO_MODE_GPIO,
+	.gpio28 = GPIO_MODE_GPIO,
+	.gpio29 = GPIO_MODE_GPIO,
+	.gpio30 = GPIO_MODE_NATIVE,
+	.gpio31 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_direction = {
+	.gpio0 = GPIO_DIR_INPUT,
+	.gpio1 = GPIO_DIR_INPUT,
+	.gpio2 = GPIO_DIR_INPUT,
+	.gpio3 = GPIO_DIR_INPUT,
+	.gpio4 = GPIO_DIR_INPUT,
+	.gpio6 = GPIO_DIR_INPUT,
+	.gpio7 = GPIO_DIR_INPUT,
+	.gpio8 = GPIO_DIR_INPUT,
+	.gpio13 = GPIO_DIR_INPUT,
+	.gpio14 = GPIO_DIR_INPUT,
+	.gpio15 = GPIO_DIR_INPUT,
+	.gpio16 = GPIO_DIR_INPUT,
+	.gpio17 = GPIO_DIR_OUTPUT,
+	.gpio19 = GPIO_DIR_INPUT,
+	.gpio21 = GPIO_DIR_INPUT,
+	.gpio22 = GPIO_DIR_INPUT,
+	.gpio24 = GPIO_DIR_INPUT,
+	.gpio27 = GPIO_DIR_INPUT,
+	.gpio28 = GPIO_DIR_OUTPUT,
+	.gpio29 = GPIO_DIR_INPUT,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_level = {
+	.gpio17 = GPIO_LEVEL_HIGH,
+	.gpio28 = GPIO_LEVEL_LOW,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_reset = {
+	.gpio30 = GPIO_RESET_RSMRST,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_invert = {
+	.gpio0 = GPIO_INVERT,
+	.gpio8 = GPIO_INVERT,
+	.gpio13 = GPIO_INVERT,
+	.gpio14 = GPIO_INVERT,
+};
+
+static const struct pch_gpio_set1 pch_gpio_set1_blink = {
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_mode = {
+	.gpio32 = GPIO_MODE_NATIVE,
+	.gpio33 = GPIO_MODE_GPIO,
+	.gpio34 = GPIO_MODE_GPIO,
+	.gpio35 = GPIO_MODE_GPIO,
+	.gpio36 = GPIO_MODE_GPIO,
+	.gpio37 = GPIO_MODE_GPIO,
+	.gpio38 = GPIO_MODE_GPIO,
+	.gpio39 = GPIO_MODE_GPIO,
+	.gpio40 = GPIO_MODE_NATIVE,
+	.gpio41 = GPIO_MODE_NATIVE,
+	.gpio42 = GPIO_MODE_NATIVE,
+	.gpio43 = GPIO_MODE_NATIVE,
+	.gpio44 = GPIO_MODE_NATIVE,
+	.gpio45 = GPIO_MODE_GPIO,
+	.gpio46 = GPIO_MODE_NATIVE,
+	.gpio47 = GPIO_MODE_NATIVE,
+	.gpio48 = GPIO_MODE_GPIO,
+	.gpio49 = GPIO_MODE_GPIO,
+	.gpio50 = GPIO_MODE_NATIVE,
+	.gpio51 = GPIO_MODE_GPIO,
+	.gpio52 = GPIO_MODE_GPIO,
+	.gpio53 = GPIO_MODE_NATIVE,
+	.gpio54 = GPIO_MODE_GPIO,
+	.gpio55 = GPIO_MODE_NATIVE,
+	.gpio56 = GPIO_MODE_NATIVE,
+	.gpio57 = GPIO_MODE_GPIO,
+	.gpio58 = GPIO_MODE_NATIVE,
+	.gpio59 = GPIO_MODE_NATIVE,
+	.gpio60 = GPIO_MODE_GPIO,
+	.gpio61 = GPIO_MODE_NATIVE,
+	.gpio62 = GPIO_MODE_NATIVE,
+	.gpio63 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_direction = {
+	.gpio33 = GPIO_DIR_INPUT,
+	.gpio34 = GPIO_DIR_OUTPUT,
+	.gpio35 = GPIO_DIR_INPUT,
+	.gpio36 = GPIO_DIR_INPUT,
+	.gpio37 = GPIO_DIR_INPUT,
+	.gpio38 = GPIO_DIR_INPUT,
+	.gpio39 = GPIO_DIR_INPUT,
+	.gpio45 = GPIO_DIR_OUTPUT,
+	.gpio48 = GPIO_DIR_INPUT,
+	.gpio49 = GPIO_DIR_INPUT,
+	.gpio51 = GPIO_DIR_INPUT,
+	.gpio52 = GPIO_DIR_INPUT,
+	.gpio54 = GPIO_DIR_INPUT,
+	.gpio57 = GPIO_DIR_INPUT,
+	.gpio60 = GPIO_DIR_OUTPUT,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_level = {
+	.gpio34 = GPIO_LEVEL_HIGH,
+	.gpio45 = GPIO_LEVEL_LOW,
+	.gpio60 = GPIO_LEVEL_HIGH,
+};
+
+static const struct pch_gpio_set2 pch_gpio_set2_reset = {
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_mode = {
+	.gpio64 = GPIO_MODE_NATIVE,
+	.gpio65 = GPIO_MODE_NATIVE,
+	.gpio66 = GPIO_MODE_NATIVE,
+	.gpio67 = GPIO_MODE_NATIVE,
+	.gpio68 = GPIO_MODE_GPIO,
+	.gpio69 = GPIO_MODE_GPIO,
+	.gpio70 = GPIO_MODE_GPIO,
+	.gpio71 = GPIO_MODE_GPIO,
+	.gpio72 = GPIO_MODE_NATIVE,
+	.gpio73 = GPIO_MODE_NATIVE,
+	.gpio74 = GPIO_MODE_NATIVE,
+	.gpio75 = GPIO_MODE_NATIVE,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_direction = {
+	.gpio68 = GPIO_DIR_INPUT,
+	.gpio69 = GPIO_DIR_INPUT,
+	.gpio70 = GPIO_DIR_INPUT,
+	.gpio71 = GPIO_DIR_INPUT,
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_level = {
+};
+
+static const struct pch_gpio_set3 pch_gpio_set3_reset = {
+};
+
+const struct pch_gpio_map mainboard_gpio_map = {
+	.set1 = {
+		.mode		= &pch_gpio_set1_mode,
+		.direction	= &pch_gpio_set1_direction,
+		.level		= &pch_gpio_set1_level,
+		.blink		= &pch_gpio_set1_blink,
+		.invert		= &pch_gpio_set1_invert,
+		.reset		= &pch_gpio_set1_reset,
+	},
+	.set2 = {
+		.mode		= &pch_gpio_set2_mode,
+		.direction	= &pch_gpio_set2_direction,
+		.level		= &pch_gpio_set2_level,
+		.reset		= &pch_gpio_set2_reset,
+	},
+	.set3 = {
+		.mode		= &pch_gpio_set3_mode,
+		.direction	= &pch_gpio_set3_direction,
+		.level		= &pch_gpio_set3_level,
+		.reset		= &pch_gpio_set3_reset,
+	},
+};
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6230/hda_verb.c b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/hda_verb.c
new file mode 100644
index 0000000000..f6876f9e09
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/hda_verb.c
@@ -0,0 +1,32 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <device/azalia_device.h>
+
+const u32 cim_verb_data[] = {
+	0x111d76df, /* Codec Vendor / Device ID: IDT */
+	0x10280532, /* Subsystem ID */
+	11, /* Number of 4 dword sets */
+	AZALIA_SUBVENDOR(0, 0x10280532),
+	AZALIA_PIN_CFG(0, 0x0a, 0x03a11020),
+	AZALIA_PIN_CFG(0, 0x0b, 0x0321101f),
+	AZALIA_PIN_CFG(0, 0x0c, 0x400000f0),
+	AZALIA_PIN_CFG(0, 0x0d, 0x90170110),
+	AZALIA_PIN_CFG(0, 0x0e, 0x23011050),
+	AZALIA_PIN_CFG(0, 0x0f, 0x23a1102e),
+	AZALIA_PIN_CFG(0, 0x10, 0x400000f3),
+	AZALIA_PIN_CFG(0, 0x11, 0xd5a30130),
+	AZALIA_PIN_CFG(0, 0x1f, 0x400000f0),
+	AZALIA_PIN_CFG(0, 0x20, 0x400000f0),
+
+	0x80862806, /* Codec Vendor / Device ID: Intel */
+	0x80860101, /* Subsystem ID */
+	4, /* Number of 4 dword sets */
+	AZALIA_SUBVENDOR(3, 0x80860101),
+	AZALIA_PIN_CFG(3, 0x05, 0x18560010),
+	AZALIA_PIN_CFG(3, 0x06, 0x18560020),
+	AZALIA_PIN_CFG(3, 0x07, 0x18560030),
+};
+
+const u32 pc_beep_verbs[0] = {};
+
+AZALIA_ARRAY_SIZES;
diff --git a/src/mainboard/dell/snb_ivb_latitude/variants/e6230/overridetree.cb b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/overridetree.cb
new file mode 100644
index 0000000000..3a0fa720da
--- /dev/null
+++ b/src/mainboard/dell/snb_ivb_latitude/variants/e6230/overridetree.cb
@@ -0,0 +1,40 @@
+## SPDX-License-Identifier: GPL-2.0-or-later
+
+chip northbridge/intel/sandybridge
+	device domain 0 on
+		subsystemid 0x1028 0x0532 inherit
+
+		device ref igd on
+			register "gpu_cpu_backlight" = "0x000009e9"
+			register "gpu_pch_backlight" = "0x13121312"
+		end
+
+		chip southbridge/intel/bd82x6x
+			register "usb_port_config" = "{
+				{ 1, 1, 0 },
+				{ 1, 1, 0 },
+				{ 1, 0, 1 },
+				{ 1, 2, 1 },
+				{ 1, 0, 2 },
+				{ 1, 0, 2 },
+				{ 1, 0, 3 },
+				{ 1, 1, 3 },
+				{ 1, 2, 4 },
+				{ 1, 1, 4 },
+				{ 1, 1, 5 },
+				{ 1, 1, 5 },
+				{ 1, 2, 6 },
+				{ 1, 0, 6 },
+			}"
+
+			device ref xhci on
+				register "superspeed_capable_ports" = "0x0000000f"
+				register "xhci_overcurrent_mapping" = "0x00000c03"
+				register "xhci_switchable_ports" = "0x0000000f"
+			end
+			device ref sata1 on
+				register "sata_port_map" = "0x31"
+			end
+		end
+	end
+end
-- 
2.39.5

