From 496cdb9ccfe8908ec0fe7f703ce6f25e5abf1c18 Mon Sep 17 00:00:00 2001
From: Mate Kukri <kukri.mate@gmail.com>
Date: Thu, 24 Oct 2024 18:05:19 +0100
Subject: [PATCH 1/5] mb/dell: OptiPlex 3050 Micro port (Intel KabyLake)

- Boots Linux 6.11 (Debian)
- GRUB and SeaBIOS payloads work
- SMSC SCH5553 SIO/EC
  + Serial port works
  + PWM fan control works
- Realtek Gigabit LAN works
- WiFi slot works
- NVMe SSD slot works
- Extra: LPSS UART0
  + Stock FW sets undocumented power gating bit, RTC battery needs to
    be pulled for it to work.
  + Signals exposed on test points on the back of the board.
    FIXME: add documentation about this
- Needs 'deguard' to bypass BootGuard
  + See https://review.coreboot.org/plugins/gitiles/deguard
- Audio works
- All USB ports work
- Currently limited to the Micro form factor, but others are very
  similar
- HDA verbs and VBT by Leah Rowe

Change-Id: I8d443e39ee684a4eaa19c835a945cfe569c051e2
Signed-off-by: Mate Kukri <kukri.mate@gmail.com>
---
 src/mainboard/dell/optiplex_3050/Kconfig      |  37 ++
 src/mainboard/dell/optiplex_3050/Kconfig.name |   4 +
 src/mainboard/dell/optiplex_3050/Makefile.mk  |  12 +
 src/mainboard/dell/optiplex_3050/acpi/ec.asl  |   3 +
 .../dell/optiplex_3050/acpi/superio.asl       |   3 +
 .../dell/optiplex_3050/board_info.txt         |   7 +
 src/mainboard/dell/optiplex_3050/bootblock.c  | 107 ++++
 src/mainboard/dell/optiplex_3050/cmos.default |   5 +
 src/mainboard/dell/optiplex_3050/cmos.layout  |  54 ++
 src/mainboard/dell/optiplex_3050/data.vbt     | Bin 0 -> 4300 bytes
 .../dell/optiplex_3050/devicetree.cb          | 103 ++++
 src/mainboard/dell/optiplex_3050/dsdt.asl     |  27 +
 .../dell/optiplex_3050/gma-mainboard.ads      |  19 +
 src/mainboard/dell/optiplex_3050/hda_verb.c   |  90 +++
 .../dell/optiplex_3050/include/early_gpio.h   |  11 +
 .../dell/optiplex_3050/include/gpio.h         | 241 +++++++++
 src/mainboard/dell/optiplex_3050/ramstage.c   | 512 ++++++++++++++++++
 src/mainboard/dell/optiplex_3050/romstage.c   |  18 +
 src/mainboard/dell/optiplex_3050/sch5555_ec.c |  54 ++
 src/mainboard/dell/optiplex_3050/sch5555_ec.h |  10 +
 20 files changed, 1317 insertions(+)
 create mode 100644 src/mainboard/dell/optiplex_3050/Kconfig
 create mode 100644 src/mainboard/dell/optiplex_3050/Kconfig.name
 create mode 100644 src/mainboard/dell/optiplex_3050/Makefile.mk
 create mode 100644 src/mainboard/dell/optiplex_3050/acpi/ec.asl
 create mode 100644 src/mainboard/dell/optiplex_3050/acpi/superio.asl
 create mode 100644 src/mainboard/dell/optiplex_3050/board_info.txt
 create mode 100644 src/mainboard/dell/optiplex_3050/bootblock.c
 create mode 100644 src/mainboard/dell/optiplex_3050/cmos.default
 create mode 100644 src/mainboard/dell/optiplex_3050/cmos.layout
 create mode 100644 src/mainboard/dell/optiplex_3050/data.vbt
 create mode 100644 src/mainboard/dell/optiplex_3050/devicetree.cb
 create mode 100644 src/mainboard/dell/optiplex_3050/dsdt.asl
 create mode 100644 src/mainboard/dell/optiplex_3050/gma-mainboard.ads
 create mode 100644 src/mainboard/dell/optiplex_3050/hda_verb.c
 create mode 100644 src/mainboard/dell/optiplex_3050/include/early_gpio.h
 create mode 100644 src/mainboard/dell/optiplex_3050/include/gpio.h
 create mode 100644 src/mainboard/dell/optiplex_3050/ramstage.c
 create mode 100644 src/mainboard/dell/optiplex_3050/romstage.c
 create mode 100644 src/mainboard/dell/optiplex_3050/sch5555_ec.c
 create mode 100644 src/mainboard/dell/optiplex_3050/sch5555_ec.h

diff --git a/src/mainboard/dell/optiplex_3050/Kconfig b/src/mainboard/dell/optiplex_3050/Kconfig
new file mode 100644
index 0000000000..6c8e72956e
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/Kconfig
@@ -0,0 +1,37 @@
+## SPDX-License-Identifier: GPL-2.0-only
+
+if BOARD_DELL_OPTIPLEX_3050
+
+config BOARD_SPECIFIC_OPTIONS
+	def_bool y
+	select BOARD_ROMSIZE_KB_16384
+	select HAVE_ACPI_RESUME
+	select HAVE_ACPI_TABLES
+	select HAVE_CMOS_DEFAULT
+	select HAVE_OPTION_TABLE
+	select INTEL_GMA_ADD_VBT
+	select INTEL_GMA_HAVE_VBT
+	select MAINBOARD_HAS_LIBGFXINIT
+	select MAINBOARD_SUPPORTS_KABYLAKE_CPU
+	select MAINBOARD_SUPPORTS_SKYLAKE_CPU
+	select SKYLAKE_SOC_PCH_H
+	select SOC_INTEL_COMMON_BLOCK_HDA_VERB
+	select SOC_INTEL_KABYLAKE
+	select SUPERIO_SMSC_SCH555x
+
+config CBFS_SIZE
+	default 0x900000
+
+config MAINBOARD_DIR
+	default "dell/optiplex_3050"
+
+config MAINBOARD_PART_NUMBER
+	default "OptiPlex 3050 Micro"
+
+config INTEL_GMA_VBT_FILE
+	default "src/mainboard/\$(MAINBOARDDIR)/data.vbt"
+
+config DIMM_SPD_SIZE
+	default 512	# DDR4
+
+endif
diff --git a/src/mainboard/dell/optiplex_3050/Kconfig.name b/src/mainboard/dell/optiplex_3050/Kconfig.name
new file mode 100644
index 0000000000..14eab7f52c
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/Kconfig.name
@@ -0,0 +1,4 @@
+## SPDX-License-Identifier: GPL-2.0-only
+
+config BOARD_DELL_OPTIPLEX_3050
+	bool "OptiPlex 3050 Micro"
diff --git a/src/mainboard/dell/optiplex_3050/Makefile.mk b/src/mainboard/dell/optiplex_3050/Makefile.mk
new file mode 100644
index 0000000000..0bd72fe691
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/Makefile.mk
@@ -0,0 +1,12 @@
+## SPDX-License-Identifier: GPL-2.0-only
+
+bootblock-y += bootblock.c
+bootblock-y += sch5555_ec.c
+
+romstage-y += romstage.c
+
+ramstage-y += ramstage.c
+ramstage-y += sch5555_ec.c
+ramstage-y += hda_verb.c
+
+ramstage-$(CONFIG_MAINBOARD_USE_LIBGFXINIT) += gma-mainboard.ads
diff --git a/src/mainboard/dell/optiplex_3050/acpi/ec.asl b/src/mainboard/dell/optiplex_3050/acpi/ec.asl
new file mode 100644
index 0000000000..16990d45f4
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/acpi/ec.asl
@@ -0,0 +1,3 @@
+/* SPDX-License-Identifier: CC-PDDC */
+
+/* Please update the license if adding licensable material. */
diff --git a/src/mainboard/dell/optiplex_3050/acpi/superio.asl b/src/mainboard/dell/optiplex_3050/acpi/superio.asl
new file mode 100644
index 0000000000..16990d45f4
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/acpi/superio.asl
@@ -0,0 +1,3 @@
+/* SPDX-License-Identifier: CC-PDDC */
+
+/* Please update the license if adding licensable material. */
diff --git a/src/mainboard/dell/optiplex_3050/board_info.txt b/src/mainboard/dell/optiplex_3050/board_info.txt
new file mode 100644
index 0000000000..47a4a3a4f3
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/board_info.txt
@@ -0,0 +1,7 @@
+Category: desktop
+Board URL: https://www.dell.com/support/kbdoc/en-uk/000124265/dell-optiplex-3050-system-guide
+ROM package: SOIC-8
+ROM protocol: SPI
+ROM socketed: n
+Flashrom support: y
+Release year: 2017
diff --git a/src/mainboard/dell/optiplex_3050/bootblock.c b/src/mainboard/dell/optiplex_3050/bootblock.c
new file mode 100644
index 0000000000..10689c42a1
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/bootblock.c
@@ -0,0 +1,107 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <bootblock_common.h>
+#include <device/pnp_ops.h>
+#include <soc/gpio.h>
+#include <superio/smsc/sch555x/sch555x.h>
+#include "include/early_gpio.h"
+#include "sch5555_ec.h"
+
+struct ec_init_entry {
+	uint16_t addr;
+	uint8_t val;
+};
+
+static void bootblock_ec_init(void)
+{
+	/*
+	 * Early EC init
+	 */
+
+	static const struct ec_init_entry init_table1[] = {
+		{0x08cc, 0x11}, {0x08d0, 0x11}, {0x088c, 0x10}, {0x0890, 0x10},
+		{0x0894, 0x10}, {0x0898, 0x12}, {0x089c, 0x12}, {0x08a0, 0x10},
+		{0x08a4, 0x12}, {0x08a8, 0x10}, {0x0820, 0x12}, {0x0824, 0x12},
+		{0x0878, 0x12}, {0x0880, 0x12}, {0x0884, 0x12}, {0x08e0, 0x12},
+		{0x08e4, 0x12}, {0x083c, 0x10}, {0x0840, 0x10}, {0x0844, 0x10},
+		{0x0848, 0x10}, {0x084c, 0x10}, {0x0850, 0x10}, {0x0814, 0x11},
+	};
+
+	for (size_t i = 0; i < ARRAY_SIZE(init_table1); ++i)
+		sch5555_mbox_write(2, init_table1[i].addr, init_table1[i].val);
+
+	static const struct ec_init_entry init_table2[] = {
+		{0x0040, 0x00}, {0x00f8, 0x10}, {0x00f9, 0x00}, {0x00f0, 0x30},
+		{0x00fa, 0x00}, {0x00fb, 0x00}, {0x00ea, 0x00}, {0x00eb, 0x00},
+		{0x00ef, 0x7c}, {0x0005, 0x0f}, {0x0014, 0x01}, {0x0018, 0x2f},
+		{0x0019, 0x2f}, {0x001a, 0x2f}, {0x001b, 0x2f}, {0x01d8, 0x01},
+		{0x0040, 0x11},
+	};
+
+	for (size_t i = 0; i < ARRAY_SIZE(init_table2); ++i)
+		sch5555_mbox_write(1, init_table2[i].addr, init_table2[i].val);
+
+	sch5555_mbox_write(1, 0x000b, 0x01);
+	sch5555_mbox_write(4, 0x001a, 0x04);
+	sch5555_mbox_write(4, 0x0028, 0x18);
+	sch5555_mbox_write(4, 0x001a, 0x00);
+	sch5555_mbox_write(1, 0x000b, 0x03);
+
+	/*
+	 * Early HWM init
+	 */
+
+	sch5555_mbox_read(1, 0xcb);
+	sch5555_mbox_read(1, 0xb8);
+
+	static const struct ec_init_entry hwm_init_table[] = {
+		{0x02fc, 0xa0}, {0x02fd, 0x32}, {0x0005, 0x77}, {0x0019, 0x2f},
+		{0x001a, 0x2f}, {0x008a, 0x33}, {0x008b, 0x33}, {0x008c, 0x33},
+		{0x00ba, 0x10}, {0x00d1, 0xff}, {0x00d6, 0xff}, {0x00db, 0xff},
+		{0x0048, 0x00}, {0x0049, 0x00}, {0x007a, 0x00}, {0x007b, 0x00},
+		{0x007c, 0x00}, {0x0080, 0x00}, {0x0081, 0x00}, {0x0082, 0x00},
+		{0x0083, 0xbb}, {0x0084, 0xb0}, {0x01a1, 0x88}, {0x01a4, 0x80},
+		{0x0088, 0x00}, {0x0089, 0x00}, {0x00a0, 0x02}, {0x00a1, 0x02},
+		{0x00a2, 0x02}, {0x00a4, 0x04}, {0x00a5, 0x04}, {0x00a6, 0x04},
+		{0x00ab, 0x00}, {0x00ad, 0x3f}, {0x00b7, 0x07}, {0x0062, 0x50},
+		{0x0000, 0x46}, {0x0000, 0x50}, {0x0000, 0x46}, {0x0000, 0x50},
+		{0x0000, 0x46}, {0x0000, 0x98}, {0x0059, 0x98}, {0x0061, 0x7c},
+		{0x01bc, 0x00}, {0x01bd, 0x00}, {0x01bb, 0x00}, {0x0085, 0xdd},
+		{0x0086, 0xdd}, {0x0087, 0x07}, {0x0090, 0x82}, {0x0091, 0x5e},
+		{0x0095, 0x5d}, {0x0096, 0xa9}, {0x0097, 0x00}, {0x009b, 0x00},
+		{0x00ae, 0x86}, {0x00af, 0x86}, {0x00b3, 0x67}, {0x00c4, 0xff},
+		{0x00c5, 0xff}, {0x00c9, 0xff}, {0x0040, 0x01}, {0x02fc, 0x00},
+		{0x02b3, 0x9a}, {0x02b4, 0x05}, {0x02cc, 0x01}, {0x02d0, 0x4c},
+		{0x02d2, 0x01}, {0x02db, 0x01}, {0x006f, 0x01}, {0x0070, 0x02},
+		{0x0071, 0x03}, {0x018b, 0x03}, {0x018c, 0x03}, {0x0015, 0x33},
+		{0x018b, 0x00}, {0x018c, 0x00}, {0x02f8, 0x5e}, {0x02f9, 0x01},
+	};
+
+	for (size_t i = 0; i < ARRAY_SIZE(hwm_init_table); ++i)
+		sch5555_mbox_write(1, hwm_init_table[i].addr, hwm_init_table[i].val);
+}
+
+
+#define SCH555x_IOBASE	0x2e
+#define GLOBAL_DEV	PNP_DEV(SCH555x_IOBASE, SCH555x_LDN_GLOBAL)
+#define SERIAL_DEV	PNP_DEV(SCH555x_IOBASE, SCH555x_LDN_UART1)
+
+void bootblock_mainboard_early_init(void)
+{
+	gpio_configure_pads(early_gpio_table, ARRAY_SIZE(early_gpio_table));
+
+	// Super I/O early init will map Runtime and EMI registers
+	sch555x_early_init(GLOBAL_DEV);
+
+	// Changes LED color among a few other things
+	outb(1, SCH555x_RUNTIME_IOBASE + SCH555x_RUNTIME_PME_STS);
+	outb(1, SCH555x_RUNTIME_IOBASE + SCH555x_RUNTIME_PME_EN);
+	outb(0xf, SCH555x_RUNTIME_IOBASE + SCH555x_RUNTIME_LED);
+	outb(1, SCH555x_RUNTIME_IOBASE + SCH555x_RUNTIME_UNK1);
+
+	// Perform bootblock EC initialization
+	bootblock_ec_init();
+
+	// Bootblock EC initialization is required for UART1 to work
+	sch555x_enable_serial(SERIAL_DEV, CONFIG_TTYS0_BASE);
+}
diff --git a/src/mainboard/dell/optiplex_3050/cmos.default b/src/mainboard/dell/optiplex_3050/cmos.default
new file mode 100644
index 0000000000..79961f43d8
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/cmos.default
@@ -0,0 +1,5 @@
+## SPDX-License-Identifier: GPL-2.0-only
+
+boot_option=Fallback
+debug_level=Debug
+power_on_after_fail=Disable
diff --git a/src/mainboard/dell/optiplex_3050/cmos.layout b/src/mainboard/dell/optiplex_3050/cmos.layout
new file mode 100644
index 0000000000..54a5147b7d
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/cmos.layout
@@ -0,0 +1,54 @@
+## SPDX-License-Identifier: GPL-2.0-only
+
+# -----------------------------------------------------------------
+entries
+
+#start-bit length  config config-ID	name
+
+# -----------------------------------------------------------------
+0	120	r	0	reserved_memory
+
+# -----------------------------------------------------------------
+# RTC_BOOT_BYTE (coreboot hardcoded)
+384	1	e	4	boot_option
+388	4	h	0	reboot_counter
+
+# -----------------------------------------------------------------
+# coreboot config options: console
+395	4	e	6	debug_level
+
+# coreboot config options: southbridge
+409	2	e	7	power_on_after_fail
+
+# coreboot config options: bootloader
+#Used by ChromeOS:
+416	128	r	0	vbnv
+
+# coreboot config options: check sums
+984	16	h	0	check_sum
+
+# -----------------------------------------------------------------
+
+enumerations
+
+#ID	value	text
+1	0	Disable
+1	1	Enable
+4	0	Fallback
+4	1	Normal
+6	0	Emergency
+6	1	Alert
+6	2	Critical
+6	3	Error
+6	4	Warning
+6	5	Notice
+6	6	Info
+6	7	Debug
+6	8	Spew
+7	0	Disable
+7	1	Enable
+7	2	Keep
+# -----------------------------------------------------------------
+checksums
+
+checksum 392 415 984
diff --git a/src/mainboard/dell/optiplex_3050/data.vbt b/src/mainboard/dell/optiplex_3050/data.vbt
new file mode 100644
index 0000000000000000000000000000000000000000..6dc40cd99563bcd957ec2a9c4567e3b21e5d1d1f
GIT binary patch
literal 4300
zcmeHJZ)_A*5TD(>zi)T1ds~!pU>y<RuF$e~N-bJsuXmJ|7P*63&uGGx+#w{DmbQ?B
ze^_HpNECA))Sw}xiC;|p(!}^ljU+}T!9QpeKH4uPN;EMM;}_tZeY@?IBiNH@l!V#L
zn>X`jfBW9Nd2eS$e@7qg=y|L+*|P~<Du4l>Ybk24rH<}xJ9eg%eaW32z1vbf_%+-P
zC$uXU01ASzM2Q>g;@$hkii6SZG3@E+#eVw*w9N;N1g6_?YiB3s;_)?@>DbVf-r9}P
zO`Vx|jP%robSBQ#gsrAYO>p&IQpqWSxVK|yXmkvV`v!Im77N$TZXru*X!y{`-Y55r
zVKf!Pgkc!X2_qgyK4nY|jSRP7a&Qp0+diYXy*OGNIan;Ts7z%5ry$@FKoGo8XMq5h
z6OcC{V?x>l17U>+7I|RUgn|iuCftWGW>(Kf196=odH`0=A3;(GULp|y6Ks_T0R#_x
zlLt);9A0GWnQsLE?*|8{0RgE`gv2JC<6bXwubJ}!0Qv+3{3xJE9q#3H2<s&G0tf>5
z>@mL~p#5nF3*pl}^hKC<v1C31Ae!^M&^2;#l`=O_ZLQWF$7*Y}Uh$G>xt9(*`c-X6
zFkpAE5jIOv7?VVJPHKbYp3@KrBCHN-@DOp9_>7mqcf{Wl|3v&7@nvGak3pDtDe*nT
zYl+trr--)_KT146>^lIL%Ay5+{&h=mW!RCRdEk{8SSMWj3D+L{)!qr(URTPl<i;AB
za@p^PE9Ea6pj-}YuxDTr0>wf|yGUKG?B!CDGOpf7(oT__tC!2cJgEtK{*6}R$n1=r
z$PSguH+xU1hb?rHq(J+G2P}V^ryazPkEs%j0}In3b4gctpl8)ZC&3qS6o31yv0DC@
zBN6*5So*Vg*3aOq|DtfT{{PvtW2P<e%*HkB(yV?<-ipBd2rTP@b3v<wGk0i#{Bmcc
z@y0B7K0!Gt2Iyi?fd2i^HUB$v{Q!tv^fz~$94j}a>75FZ$;1Eo6%!)V*$4D5C>nt}
z7_D}&ricJyuY&X-!vUs`GWIOPx0wDOV;?d6f$4uRCdjx-*4N7{CF5RMe_CcQ%J`0~
ze<-uhWc)?e%Q6cpxK`1V3hPmDzoNgOuwx3otLUF7>?;L-S9HJ1!Ybac>fI{aq2eJ`
ze@SJpsrbICf1$GTDqdFgx)56u!i^z48)A=#)F$0)i8F!~4)H=KFrv`ilM@v#FA5q-
zZ`~^T%U!!Etw*TnvRA91loJ<5n5;vH=aymAq8i4g#?~Vu@R%z0b-pk{VF{Q?SZOpI
zZFLYDT8~J)KBGPNg2zT^r<&>dt1z12coq!P7_N5^Xb$wE-B-rFk(v<3F&oiLZ61P9
z^8O8kx7Uu(WFsrh-0{jBgc7g$6w^0d!yLLcn#Qi_glV3tAo!dLNa^?163N|n^-pD?
z(daC>dtpbi#Q&W%m0IHPOiO7pA89lVboYWH=_yh1N|ChuwX7oAZcPqP-%SWj_FFt3
zyd_?zD3jia8uH=I*yP#l#Bw9^#^N~y33zEtk*o#5XfjXdCkjSG)~N^WoRlb;h;B3|
zIfCjSc(I06T!_GA1{WKOk*chsMCXx5vW@41o#fZgYViT9VSih*nQN}>g+zCejX>9!
zZ{c$hGa+w5eO}YT_FH@}B)U(Dl-|zF&dk8R;^4yrPZe)YrI^k%j}0~VZ%*1PT98&h
z556thD#%T3IZc)NKi{(4RJn@8Dq3?JywFKA?WW585y(IR)(Ee|k5bDtz|lFnDY}0G
Ds8qe3

literal 0
HcmV?d00001

diff --git a/src/mainboard/dell/optiplex_3050/devicetree.cb b/src/mainboard/dell/optiplex_3050/devicetree.cb
new file mode 100644
index 0000000000..039709aa4a
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/devicetree.cb
@@ -0,0 +1,103 @@
+## SPDX-License-Identifier: GPL-2.0-only
+
+chip soc/intel/skylake
+	register "deep_sx_config" = "DSX_EN_WAKE_PIN | DSX_EN_LAN_WAKE_PIN"
+
+	# Enable Enhanced Intel SpeedStep
+	register "eist_enable" = "1"
+
+	device domain 0 on
+		device ref igpu on
+			register "PrimaryDisplay" = "Display_iGFX"
+		end
+
+		device ref south_xhci on
+			register "usb2_ports" = "{
+				[0] = USB2_PORT_MID(OC0),	// Front panel (blue)
+				[1] = USB2_PORT_MID(OC0),	// Front panel (blue)
+				[2] = USB2_PORT_MID(OC3),	// Back panel (black)
+				[3] = USB2_PORT_MID(OC2),	// Back panel (blue)
+				[4] = USB2_PORT_MID(OC1),	// Back panel (blue)
+				[6] = USB2_PORT_MID(OC1),	// Back panel (black)
+				[8] = USB2_PORT_MID(OC_SKIP),	// WiFi slot
+			}"
+			register "usb3_ports" = "{
+				[0] = USB3_PORT_DEFAULT(OC0),	// Front panel (blue)
+				[1] = USB3_PORT_DEFAULT(OC0),	// Front panel (blue)
+				[2] = USB3_PORT_DEFAULT(OC2),	// Back panel (blue)
+				[3] = USB3_PORT_DEFAULT(OC1),	// Back panel (blue)
+			}"
+		end
+
+		# ME interface is 'off' to avoid HECI reset delay due to HAP
+		device ref heci1 off end
+
+		device ref sata on
+			register "SataSalpSupport" = "1"
+			register "SataPortsEnable[0]" = "1"
+		end
+
+		# M.2 SSD
+		device ref pcie_rp21 on
+			register "PcieRpEnable[20]"                     = "1"
+			register "PcieRpClkReqSupport[20]"              = "1"
+			register "PcieRpClkReqNumber[20]"               = "3"
+			register "PcieRpAdvancedErrorReporting[20]"     = "1"
+			register "PcieRpLtrEnable[20]"                  = "1"
+			register "PcieRpClkSrcNumber[20]"               = "3"
+			register "PcieRpHotPlug[20]"                    = "1"
+		end
+
+		# Realtek LAN
+		device ref pcie_rp5 on
+			register "PcieRpEnable[4]"			= "1"
+			register "PcieRpClkReqSupport[4]"		= "0"
+			register "PcieRpHotPlug[4]"			= "0"
+		end
+
+		# M.2 WiFi
+		device ref pcie_rp8 on
+			register "PcieRpEnable[7]"			= "1"
+			register "PcieRpClkReqSupport[7]"		= "0"
+			register "PcieRpHotPlug[7]"			= "1"
+		end
+
+		# UART0 is exposed on test points on the bottom of the board
+		device ref uart0 on
+			register "SerialIoDevMode[PchSerialIoIndexUart0]" = "PchSerialIoPci"
+		end
+
+		device ref lpc_espi on
+			register "serirq_mode" = "SERIRQ_CONTINUOUS"
+
+			# I/O decode for EMI/Runtime registers
+			register "gen1_dec" = "0x007c0a01"
+
+			# SCH5553
+			chip superio/smsc/sch555x
+				device pnp 2e.0 on		# EMI
+					io 0x60 = 0xa00
+				end
+				device pnp 2e.1 off end		# 8042
+				device pnp 2e.7 on		# UART1
+					io 0x60 = 0x3f8
+					irq 0x0f = 2
+					irq 0x70 = 4
+				end
+				device pnp 2e.8 off end 	# UART2
+				device pnp 2e.c on		# LPC interface
+					io 0x60 = 0x2e
+				end
+				device pnp 2e.a on		# Runtime registers
+					io 0x60 = 0xa40
+				end
+				device pnp 2e.b  off end	# Floppy Controller
+				device pnp 2e.11 off end	# Parallel Port
+			end
+		end
+
+		device ref hda on end
+
+		device ref smbus on end
+	end
+end
diff --git a/src/mainboard/dell/optiplex_3050/dsdt.asl b/src/mainboard/dell/optiplex_3050/dsdt.asl
new file mode 100644
index 0000000000..9762f6ff74
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/dsdt.asl
@@ -0,0 +1,27 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <acpi/acpi.h>
+DefinitionBlock(
+	"dsdt.aml",
+	"DSDT",
+	ACPI_DSDT_REV_2,
+	OEM_ID,
+	ACPI_TABLE_CREATOR,
+	0x20110725
+)
+{
+	#include <acpi/dsdt_top.asl>
+	#include <soc/intel/common/block/acpi/acpi/globalnvs.asl>
+	#include <cpu/intel/common/acpi/cpu.asl>
+
+	Scope (\_SB)
+	{
+		Device (PCI0)
+		{
+			#include <soc/intel/skylake/acpi/systemagent.asl>
+			#include <soc/intel/skylake/acpi/pch.asl>
+		}
+	}
+
+	#include <southbridge/intel/common/acpi/sleepstates.asl>
+}
diff --git a/src/mainboard/dell/optiplex_3050/gma-mainboard.ads b/src/mainboard/dell/optiplex_3050/gma-mainboard.ads
new file mode 100644
index 0000000000..cb4c22f285
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/gma-mainboard.ads
@@ -0,0 +1,19 @@
+-- SPDX-License-Identifier: GPL-2.0-or-later
+
+with HW.GFX.GMA;
+with HW.GFX.GMA.Display_Probing;
+
+use HW.GFX.GMA;
+use HW.GFX.GMA.Display_Probing;
+
+private package GMA.Mainboard is
+
+   ports : constant Port_List :=
+      (HDMI1,  -- External HDMI
+       DP2,    -- External DP (native)
+       HDMI2,  -- External DP (DP++)
+       DP3,    -- Video I/O card: VGA (0PKGGG), DP (H64DC)
+       HDMI3,  -- Video I/O card: VGA (0PKGGG), DP (H64DC)
+       others => Disabled);
+
+end GMA.Mainboard;
diff --git a/src/mainboard/dell/optiplex_3050/hda_verb.c b/src/mainboard/dell/optiplex_3050/hda_verb.c
new file mode 100644
index 0000000000..621e4f7a52
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/hda_verb.c
@@ -0,0 +1,90 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <device/azalia_device.h>
+
+const u32 cim_verb_data[] = {
+	/* coreboot specific header, codec 0 */
+	0x10ec0255, /* Realtek ALC3234 */
+	0x102807a3, /* Subsystem ID */
+	11,	    /* Number of entries */
+
+	/* Pin Widget Verb Table */
+
+	AZALIA_SUBVENDOR(0, 0x102807a3),
+
+	AZALIA_PIN_CFG(0, 0x12, 0x40000000), // does not describe a jack or internal device
+	AZALIA_PIN_CFG(0, 0x14, AZALIA_PIN_DESC(
+		AZALIA_INTEGRATED,
+		AZALIA_INTERNAL,
+		AZALIA_SPEAKER,
+		AZALIA_OTHER_ANALOG,
+		AZALIA_COLOR_UNKNOWN,
+		AZALIA_NO_JACK_PRESENCE_DETECT,
+		5, 0
+	)),
+	AZALIA_PIN_CFG(0, 0x17, AZALIA_PIN_CFG_NC(0)),
+	AZALIA_PIN_CFG(0, 0x18, AZALIA_PIN_CFG_NC(0)),
+	AZALIA_PIN_CFG(0, 0x19, AZALIA_PIN_CFG_NC(0)),
+	AZALIA_PIN_CFG(0, 0x1a, AZALIA_PIN_CFG_NC(0)),
+	AZALIA_PIN_CFG(0, 0x1b, AZALIA_PIN_DESC(
+		AZALIA_JACK,
+		AZALIA_EXTERNAL_PRIMARY_CHASSIS | AZALIA_FRONT,
+		AZALIA_LINE_OUT,
+		AZALIA_STEREO_MONO_1_8,
+		AZALIA_BLACK,
+		AZALIA_JACK_PRESENCE_DETECT,
+		2, 0
+	)),
+	AZALIA_PIN_CFG(0, 0x1d, 0x4054c029), // does not describe a jack or internal device
+	AZALIA_PIN_CFG(0, 0x1e, AZALIA_PIN_CFG_NC(0)),
+	AZALIA_PIN_CFG(0, 0x21, AZALIA_PIN_DESC(
+		AZALIA_JACK,
+		AZALIA_EXTERNAL_PRIMARY_CHASSIS | AZALIA_FRONT,
+		AZALIA_HP_OUT,
+		AZALIA_STEREO_MONO_1_8,
+		AZALIA_BLACK,
+		AZALIA_JACK_PRESENCE_DETECT,
+		5, 15
+	)),
+
+	/* coreboot specific header, codec 2 */
+	0x80862809, /* Intel Skylake HDMI */
+	0x80860101, /* Subsystem ID */
+	4,	    /* Number of entries */
+
+	/* Pin Widget Verb Table */
+
+	AZALIA_SUBVENDOR(2, 0x80860101),
+
+	AZALIA_PIN_CFG(2, 0x05, AZALIA_PIN_DESC(
+		AZALIA_JACK,
+		AZALIA_DIGITAL_DISPLAY,
+		AZALIA_DIGITAL_OTHER_OUT,
+		AZALIA_OTHER_DIGITAL,
+		AZALIA_COLOR_UNKNOWN,
+		AZALIA_JACK_PRESENCE_DETECT,
+		1, 0
+	)),
+	AZALIA_PIN_CFG(2, 0x06, AZALIA_PIN_DESC(
+		AZALIA_JACK,
+		AZALIA_DIGITAL_DISPLAY,
+		AZALIA_DIGITAL_OTHER_OUT,
+		AZALIA_OTHER_DIGITAL,
+		AZALIA_COLOR_UNKNOWN,
+		AZALIA_JACK_PRESENCE_DETECT,
+		1, 0
+	)),
+	AZALIA_PIN_CFG(2, 0x07, AZALIA_PIN_DESC(
+		AZALIA_JACK,
+		AZALIA_DIGITAL_DISPLAY,
+		AZALIA_DIGITAL_OTHER_OUT,
+		AZALIA_OTHER_DIGITAL,
+		AZALIA_COLOR_UNKNOWN,
+		AZALIA_JACK_PRESENCE_DETECT,
+		1, 0
+	)),
+};
+
+const u32 pc_beep_verbs[] = {};
+
+AZALIA_ARRAY_SIZES;
diff --git a/src/mainboard/dell/optiplex_3050/include/early_gpio.h b/src/mainboard/dell/optiplex_3050/include/early_gpio.h
new file mode 100644
index 0000000000..17a16371e3
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/include/early_gpio.h
@@ -0,0 +1,11 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#ifndef __OPTIPLEX_3050_EARLY_GPIO_H__
+#define __OPTIPLEX_3050_EARLY_GPIO_H__
+
+static const struct pad_config early_gpio_table[] = {
+	PAD_CFG_NF(GPP_C8, NONE, DEEP, NF1),	/* UART0_RXD */
+	PAD_CFG_NF(GPP_C9, NONE, DEEP, NF1),	/* UART0_TXD */
+};
+
+#endif
diff --git a/src/mainboard/dell/optiplex_3050/include/gpio.h b/src/mainboard/dell/optiplex_3050/include/gpio.h
new file mode 100644
index 0000000000..83293c32a9
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/include/gpio.h
@@ -0,0 +1,241 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#ifndef __OPTIPLEX_3050_GPIO_H__
+#define __OPTIPLEX_3050_GPIO_H__
+
+static const struct pad_config gpio_table[] = {
+
+	/* ------- GPIO Community 0 ------- */
+
+	/* ------- GPIO Group GPP_A ------- */
+	PAD_CFG_NF(GPP_A0, UP_20K, PLTRST, NF1),			/* RCIN# */
+	PAD_CFG_NF(GPP_A1, UP_20K, PLTRST, NF1),			/* LAD0 */
+	PAD_CFG_NF(GPP_A2, UP_20K, PLTRST, NF1),			/* LAD1 */
+	PAD_CFG_NF(GPP_A3, UP_20K, PLTRST, NF1),			/* LAD2 */
+	PAD_CFG_NF(GPP_A4, UP_20K, PLTRST, NF1),			/* LAD3 */
+	PAD_CFG_NF(GPP_A5, NONE, PLTRST, NF1),				/* LFRAME# */
+	PAD_CFG_NF(GPP_A6, NONE, PLTRST, NF1),				/* SERIRQ */
+	PAD_CFG_GPI_TRIG_OWN(GPP_A7, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_A8, NONE, DEEP, NF1),				/* CLKRUN# */
+	PAD_CFG_NF(GPP_A9, NONE, PLTRST, NF1),				/* CLKOUT_LPC0 */
+	PAD_CFG_NF(GPP_A10, NONE, PLTRST, NF1),				/* CLKOUT_LPC1 */
+	PAD_CFG_NF(GPP_A11, UP_20K, DEEP, NF1),				/* PME# */
+	PAD_CFG_GPO(GPP_A12, 0, PLTRST),				/* GPIO */
+	PAD_CFG_NF(GPP_A13, NONE, PLTRST, NF1),				/* SUSWARN#/SUSPWRDNACK */
+	PAD_CFG_GPI_TRIG_OWN(GPP_A14, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_A15, UP_20K, PLTRST, NF1),			/* SUS_ACK# */
+	PAD_CFG_GPO(GPP_A16, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A17, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A18, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A19, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A20, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A21, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A22, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_A23, 0, PLTRST),				/* GPIO */
+
+	/* ------- GPIO Group GPP_B ------- */
+	PAD_CFG_GPO(GPP_B0, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_B1, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_B2, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_B3, 1, RSMRST),					/* GPIO (ME_CNTL, B3 -> LOW => HDA_SDO -> HIGH) */
+	PAD_CFG_GPI_TRIG_OWN(GPP_B4, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_B5, 1, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_B6, 1, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_B7, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_B8, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_B9, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_B10, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_B11, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_B12, NONE, PLTRST, NF1),				/* SLP_S0# */
+	PAD_CFG_NF(GPP_B13, NONE, PLTRST, NF1),				/* PLTRST# */
+	PAD_CFG_NF(GPP_B14, DN_20K, PLTRST, NF1),			/* SPKR */
+	PAD_CFG_GPO(GPP_B15, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_B16, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_B17, 0, PLTRST),				/* GPIO */
+	PAD_CFG_NF(GPP_B18, DN_20K, DEEP, NF1),				/* GSPIO_MOSI */
+	PAD_CFG_GPO(GPP_B19, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_B20, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_B21, 0, DEEP),					/* GPIO */
+	PAD_CFG_NF(GPP_B22, DN_20K, DEEP, NF1),				/* GSPI1_MOSI */
+	PAD_CFG_NF(GPP_B23, DN_20K, DEEP, NF2),				/* PCHHOT# */
+
+	/* ------- GPIO Community 1 ------- */
+
+	/* ------- GPIO Group GPP_C ------- */
+	PAD_CFG_NF(GPP_C0, NONE, DEEP, NF1),				/* SMBCLK */
+	PAD_CFG_NF(GPP_C1, NONE, DEEP, NF1),				/* SMBDATA */
+	PAD_CFG_GPI_TRIG_OWN(GPP_C2, DN_20K, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_C3, NONE, PLTRST, NF1),				/* SML0CLK */
+	PAD_CFG_NF(GPP_C4, NONE, PLTRST, NF1),				/* SML0DATA */
+	PAD_CFG_GPI_TRIG_OWN(GPP_C5, DN_20K, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_C6, NONE, DEEP, NF1),				/* SML1CLK */
+	PAD_CFG_NF(GPP_C7, NONE, DEEP, NF1),				/* SML1DATA */
+	PAD_CFG_NF(GPP_C8, NONE, DEEP, NF1),				/* UART0_RXD */
+	PAD_CFG_NF(GPP_C9, NONE, DEEP, NF1),				/* UART0_TXD */
+	PAD_CFG_GPO(GPP_C10, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C11, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C12, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C13, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C14, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C15, 0, PLTRST),				/* GPIO */
+	PAD_CFG_NF(GPP_C16, NONE, PLTRST, NF1),				/* I2C0_SDA */
+	PAD_CFG_NF(GPP_C17, NONE, PLTRST, NF1),				/* I2C0_SCL */
+	PAD_CFG_GPO(GPP_C18, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C19, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C20, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C21, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_C22, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPI_SCI(GPP_C23, NONE, DEEP, EDGE_SINGLE, INVERT),	/* GPIO */
+
+	/* ------- GPIO Group GPP_D ------- */
+	PAD_CFG_GPO(GPP_D0, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D1, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D2, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D3, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D4, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_D5, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_D6, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_D7, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D8, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D9, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_D10, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D11, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D12, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D13, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D14, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D15, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D16, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D17, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D18, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D19, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D20, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D21, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D22, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_D23, 0, PLTRST),				/* GPIO */
+
+	/* ------- GPIO Group GPP_E ------- */
+	PAD_CFG_NF(GPP_E0, NONE, DEEP, NF1),				/* SATAXPCIE0 */
+	PAD_CFG_NF(GPP_E1, NONE, DEEP, NF1),				/* SATAXPCIE1 */
+	PAD_CFG_NF(GPP_E2, NONE, DEEP, NF1),				/* SATAXPCIE2 */
+	PAD_CFG_GPO(GPP_E3, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_E4, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_E5, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_E6, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_E7, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_E8, NONE, PLTRST, NF1),				/* SATA_LED# */
+	PAD_CFG_NF(GPP_E9, UP_20K, PLTRST, NF1),			/* USB_OC0# */
+	PAD_CFG_NF(GPP_E10, UP_20K, PLTRST, NF1),			/* USB_OC1# */
+	PAD_CFG_NF(GPP_E11, UP_20K, PLTRST, NF1),			/* USB_OC2# */
+	PAD_CFG_NF(GPP_E12, UP_20K, PLTRST, NF1),			/* USB_OC3# */
+
+	/* ------- GPIO Group GPP_F ------- */
+	PAD_CFG_NF(GPP_F0, NONE, DEEP, NF1),				/* SATAXPCIE3 */
+	PAD_CFG_NF(GPP_F1, NONE, DEEP, NF1),				/* SATAXPCIE4 */
+	PAD_CFG_NF(GPP_F2, NONE, DEEP, NF1),				/* SATAXPCIE5 */
+	PAD_CFG_NF(GPP_F3, NONE, DEEP, NF1),				/* SATAXPCIE6 */
+	PAD_CFG_NF(GPP_F4, NONE, DEEP, NF1),				/* SATAXPCIE7 */
+	PAD_CFG_GPI_TRIG_OWN(GPP_F5, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_F6, NONE, RSMRST, NF1),				/* SATA_DEVSLP4 */
+	PAD_CFG_GPO(GPP_F7, 1, PLTRST),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_F8, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_F9, 0, RSMRST),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_F10, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_F11, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_F12, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_F13, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_F14, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_NF(GPP_F15, UP_20K, DEEP, NF1),				/* USB_OC4# */
+	PAD_CFG_NF(GPP_F16, UP_20K, DEEP, NF1),				/* USB_OC5# */
+	PAD_CFG_NF(GPP_F17, UP_20K, PLTRST, NF1),			/* USB_OC6# */
+	PAD_CFG_TERM_GPO(GPP_F18, 0, UP_20K, DEEP),			/* GPIO */
+	PAD_CFG_GPO(GPP_F19, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_F20, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_F21, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_F22, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_F23, 1, RSMRST),				/* GPIO */
+
+	/* ------- GPIO Group GPP_G ------- */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G0, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G1, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G2, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G3, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G4, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G5, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G6, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G7, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G8, NONE, PLTRST, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_G9, 1, PLTRST),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G10, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G11, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_G12, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPI_TRIG_OWN(GPP_G13, NONE, DEEP, OFF, ACPI),		/* GPIO */
+	PAD_CFG_GPO(GPP_G14, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G15, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G16, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G17, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G18, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_G19, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G20, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_G21, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G22, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_G23, 0, PLTRST),				/* GPIO */
+
+	/* ------- GPIO Group GPP_H ------- */
+	PAD_CFG_GPO(GPP_H0, 0, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_H1, 1, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H2, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H3, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H4, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H5, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H6, 1, DEEP),					/* GPIO */
+	PAD_CFG_GPO(GPP_H7, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H8, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H9, 0, PLTRST),					/* GPIO */
+	PAD_CFG_GPO(GPP_H10, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H11, 0, PLTRST),				/* GPIO */
+	PAD_CFG_TERM_GPO(GPP_H12, 1, DN_20K, DEEP),			/* GPIO */
+	PAD_CFG_GPO(GPP_H13, 1, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H14, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H15, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H16, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H17, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H18, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H19, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H20, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H21, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H22, 0, PLTRST),				/* GPIO */
+	PAD_CFG_GPO(GPP_H23, 0, PLTRST),				/* GPIO */
+
+	/* ------- GPIO Community 2 ------- */
+
+	/* -------- GPIO Group GPD -------- */
+	PAD_CFG_NF(GPD0, NONE, RSMRST, NF1),				/* BATLOW# */
+	PAD_CFG_GPO(GPD1, 0, PWROK),					/* GPIO */
+	PAD_CFG_NF(GPD2, NONE, RSMRST, NF1),				/* LAN_WAKE# */
+	PAD_CFG_NF(GPD3, UP_20K, RSMRST, NF1),				/* PWRBTN# */
+	PAD_CFG_NF(GPD4, NONE, RSMRST, NF1),				/* SLP_S3# */
+	PAD_CFG_NF(GPD5, NONE, RSMRST, NF1),				/* SLP_S4# */
+	PAD_CFG_NF(GPD6, NONE, RSMRST, NF1),				/* SLP_A# */
+	PAD_CFG_GPO(GPD7, 1, RSMRST),					/* GPIO */
+	PAD_CFG_NF(GPD8, NONE, RSMRST, NF1),				/* SUSCLK */
+	PAD_CFG_NF(GPD9, NONE, RSMRST, NF1),				/* SLP_WLAN# */
+	PAD_CFG_NF(GPD10, NONE, RSMRST, NF1),				/* SLP_S5# */
+	PAD_CFG_GPO(GPD11, 1, RSMRST),					/* GPIO */
+
+	/* ------- GPIO Community 3 ------- */
+
+	/* ------- GPIO Group GPP_I ------- */
+	PAD_CFG_NF(GPP_I0, NONE, PLTRST, NF1),				/* DDPB_HPD0 */
+	PAD_CFG_NF(GPP_I1, NONE, PLTRST, NF1),				/* DDPC_HPD1 */
+	PAD_CFG_NF(GPP_I2, NONE, PLTRST, NF1),				/* DDPD_HPD2 */
+	PAD_CFG_NF(GPP_I3, NONE, PLTRST, NF1),				/* DDPE_HPD3 */
+	PAD_CFG_NF(GPP_I4, NONE, PLTRST, NF1),				/* EDP_HPD */
+	PAD_CFG_NF(GPP_I5, NONE, PLTRST, NF1),				/* DDPB_CTRLCLK */
+	PAD_CFG_NF(GPP_I6, DN_20K, PLTRST, NF1),			/* DDPB_CTRLDATA */
+	PAD_CFG_NF(GPP_I7, NONE, PLTRST, NF1),				/* DDPC_CTRLCLK */
+	PAD_CFG_NF(GPP_I8, DN_20K, PLTRST, NF1),			/* DDPC_CTRLDATA */
+	PAD_CFG_NF(GPP_I9, NONE, PLTRST, NF1),				/* DDPD_CTRLCLK */
+	PAD_CFG_NF(GPP_I10, DN_20K, PLTRST, NF1),			/* DDPD_CTRLDATA */
+};
+
+#endif
diff --git a/src/mainboard/dell/optiplex_3050/ramstage.c b/src/mainboard/dell/optiplex_3050/ramstage.c
new file mode 100644
index 0000000000..94778f60c9
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/ramstage.c
@@ -0,0 +1,512 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <bootstate.h>
+#include <arch/cpuid.h>
+#include <cpu/x86/msr.h>
+#include <soc/gpio.h>
+#include <soc/ramstage.h>
+#include "include/gpio.h"
+#include "sch5555_ec.h"
+
+void mainboard_silicon_init_params(FSP_SIL_UPD *params)
+{
+	gpio_configure_pads(gpio_table, ARRAY_SIZE(gpio_table));
+}
+
+#define FORM_FACTOR_MICRO	0
+#define FORM_FACTOR_SFF		1
+// Probably DT and MT
+#define FORM_FACTOR_UNK2	2
+#define FORM_FACTOR_UNK3	3
+
+#define HWM_TAB_ADD_TEMP_TARGET	1
+#define HWM_TAB_PKG_POWER_ANY	0xffff
+
+struct hwm_tab_entry {
+	uint16_t addr;
+	uint8_t val;
+	uint8_t flags;
+	uint16_t pkg_power;
+};
+
+static const struct hwm_tab_entry HWM_TAB_MICRO_BASE[] = {
+	{ 0x005, 0x33, 0, 0xffff },
+	{ 0x018, 0x2f, 0, 0xffff },
+	{ 0x019, 0x2f, 0, 0xffff },
+	{ 0x01a, 0x2f, 0, 0xffff },
+	{ 0x01b, 0x0f, 0, 0xffff },
+	{ 0x057, 0xff, 0, 0xffff },
+	{ 0x059, 0xff, 0, 0xffff },
+	{ 0x05b, 0xff, 0, 0xffff },
+	{ 0x05d, 0xff, 0, 0xffff },
+	{ 0x05f, 0xff, 0, 0xffff },
+	{ 0x061, 0xff, 0, 0xffff },
+	{ 0x06e, 0x00, 0, 0xffff },
+	{ 0x06f, 0x03, 0, 0xffff },
+	{ 0x070, 0x03, 0, 0xffff },
+	{ 0x071, 0x02, 0, 0xffff },
+	{ 0x072, 0x02, 0, 0xffff },
+	{ 0x073, 0x01, 0, 0xffff },
+	{ 0x074, 0x06, 0, 0xffff },
+	{ 0x075, 0x07, 0, 0xffff },
+	{ 0x080, 0x00, 0, 0xffff },
+	{ 0x081, 0x80, 0, 0xffff },
+	{ 0x082, 0x80, 0, 0xffff },
+	{ 0x083, 0xbb, 0, 0xffff },
+	{ 0x085, 0xf1, 0, 0xffff },
+	{ 0x086, 0x88, 0, 0xffff },
+	{ 0x087, 0x61, 0, 0xffff },
+	{ 0x088, 0x08, 0, 0xffff },
+	{ 0x089, 0x00, 0, 0xffff },
+	{ 0x08a, 0x73, 0, 0xffff },
+	{ 0x08b, 0x73, 0, 0xffff },
+	{ 0x08c, 0x73, 0, 0xffff },
+	{ 0x090, 0x6d, 0, 0xffff },
+	{ 0x091, 0x7e, 0, 0xffff },
+	{ 0x092, 0x66, 0, 0xffff },
+	{ 0x093, 0xa4, 0, 0xffff },
+	{ 0x094, 0x7c, 0, 0xffff },
+	{ 0x095, 0xa4, 0, 0xffff },
+	{ 0x096, 0xa4, 0, 0xffff },
+	{ 0x097, 0xa4, 0, 0xffff },
+	{ 0x098, 0xa4, 0, 0xffff },
+	{ 0x099, 0xa4, 0, 0xffff },
+	{ 0x09a, 0xa4, 0, 0xffff },
+	{ 0x09b, 0xa4, 0, 0xffff },
+	{ 0x0a0, 0x2e, 0, 0xffff },
+	{ 0x0a1, 0x00, 0, 0xffff },
+	{ 0x0a2, 0x00, 0, 0xffff },
+	{ 0x0ae, 0xa4, 0, 0xffff },
+	{ 0x0af, 0xa4, 0, 0xffff },
+	{ 0x0b0, 0xa4, 0, 0xffff },
+	{ 0x0b1, 0xa4, 0, 0xffff },
+	{ 0x0b2, 0xa4, 0, 0xffff },
+	{ 0x0b3, 0xa4, 0, 0xffff },
+	{ 0x0b6, 0x00, 0, 0xffff },
+	{ 0x0b7, 0x00, 0, 0xffff },
+	{ 0x0d1, 0xff, 0, 0xffff },
+	{ 0x0d6, 0xff, 0, 0xffff },
+	{ 0x0db, 0xff, 0, 0xffff },
+	{ 0x0ea, 0x5c, 0, 0xffff },
+	{ 0x0eb, 0x5c, 0, 0xffff },
+	{ 0x0ef, 0xff, 0, 0xffff },
+	{ 0x0f8, 0x15, 0, 0xffff },
+	{ 0x0f9, 0x00, 0, 0xffff },
+	{ 0x0f0, 0x30, 0, 0xffff },
+	{ 0x184, 0xff, 0, 0xffff },
+	{ 0x186, 0xff, 0, 0xffff },
+	{ 0x1a1, 0xce, 0, 0xffff },
+	{ 0x1a2, 0x0c, 0, 0xffff },
+	{ 0x1a3, 0x0c, 0, 0xffff },
+	{ 0x1a6, 0x00, 0, 0xffff },
+	{ 0x1a7, 0x00, 0, 0xffff },
+	{ 0x1a8, 0xa4, 0, 0xffff },
+	{ 0x1a9, 0xa4, 0, 0xffff },
+	{ 0x1ab, 0x2d, 0, 0xffff },
+	{ 0x1ac, 0x2d, 0, 0xffff },
+	{ 0x1b1, 0x00, 0, 0xffff },
+	{ 0x1bb, 0x00, 0, 0xffff },
+	{ 0x1bc, 0x00, 0, 0xffff },
+	{ 0x1bd, 0x00, 0, 0xffff },
+	{ 0x1be, 0x01, 0, 0xffff },
+	{ 0x1bf, 0x01, 0, 0xffff },
+	{ 0x1c0, 0x01, 0, 0xffff },
+	{ 0x1c1, 0x01, 0, 0xffff },
+	{ 0x1c2, 0x01, 0, 0xffff },
+	{ 0x280, 0x00, 0, 0xffff },
+	{ 0x281, 0x00, 0, 0xffff },
+	{ 0x282, 0x03, 0, 0xffff },
+	{ 0x283, 0x0a, 0, 0xffff },
+	{ 0x284, 0x80, 0, 0xffff },
+	{ 0x285, 0x03, 0, 0xffff },
+	{ 0x040, 0x01, 0, 0xffff },
+};
+
+static const struct hwm_tab_entry HWM_TAB_MICRO_TEMP80[] = {
+	{ 0x005, 0x33, 0, 0xffff },
+	{ 0x018, 0x2f, 0, 0xffff },
+	{ 0x019, 0x2f, 0, 0xffff },
+	{ 0x01a, 0x2f, 0, 0xffff },
+	{ 0x01b, 0x0f, 0, 0xffff },
+	{ 0x057, 0xff, 0, 0xffff },
+	{ 0x059, 0xff, 0, 0xffff },
+	{ 0x05b, 0xff, 0, 0xffff },
+	{ 0x05d, 0xff, 0, 0xffff },
+	{ 0x05f, 0xff, 0, 0xffff },
+	{ 0x061, 0xff, 0, 0xffff },
+	{ 0x06e, 0x00, 0, 0xffff },
+	{ 0x06f, 0x03, 0, 0xffff },
+	{ 0x070, 0x03, 0, 0xffff },
+	{ 0x071, 0x02, 0, 0xffff },
+	{ 0x072, 0x02, 0, 0xffff },
+	{ 0x073, 0x01, 0, 0xffff },
+	{ 0x074, 0x06, 0, 0xffff },
+	{ 0x075, 0x07, 0, 0xffff },
+	{ 0x080, 0x00, 0, 0xffff },
+	{ 0x081, 0x80, 0, 0xffff },
+	{ 0x082, 0x80, 0, 0xffff },
+	{ 0x083, 0xbb, 0, 0xffff },
+	{ 0x085, 0xf6, 0, 0xffff },
+	{ 0x086, 0x88, 0, 0xffff },
+	{ 0x087, 0x61, 0, 0xffff },
+	{ 0x088, 0x08, 0, 0xffff },
+	{ 0x089, 0x00, 0, 0xffff },
+	{ 0x08a, 0x73, 0, 0xffff },
+	{ 0x08b, 0x73, 0, 0xffff },
+	{ 0x08c, 0x73, 0, 0xffff },
+	{ 0x090, 0x6d, 0, 0xffff },
+	{ 0x091, 0x86, 0, 0xffff },
+	{ 0x092, 0x66, 0, 0xffff },
+	{ 0x093, 0xa4, 0, 0xffff },
+	{ 0x094, 0x7c, 0, 0xffff },
+	{ 0x095, 0xa4, 0, 0xffff },
+	{ 0x096, 0xa4, 0, 0xffff },
+	{ 0x097, 0xa4, 0, 0xffff },
+	{ 0x098, 0xa4, 0, 0xffff },
+	{ 0x099, 0xa4, 0, 0xffff },
+	{ 0x09a, 0xa4, 0, 0xffff },
+	{ 0x09b, 0xa4, 0, 0xffff },
+	{ 0x0a0, 0x2e, 0, 0xffff },
+	{ 0x0a1, 0x00, 0, 0xffff },
+	{ 0x0a2, 0x00, 0, 0xffff },
+	{ 0x0ae, 0xa4, 0, 0xffff },
+	{ 0x0af, 0xa4, 0, 0xffff },
+	{ 0x0b0, 0xa4, 0, 0xffff },
+	{ 0x0b1, 0xa4, 0, 0xffff },
+	{ 0x0b2, 0xa4, 0, 0xffff },
+	{ 0x0b3, 0xa4, 0, 0xffff },
+	{ 0x0b6, 0x00, 0, 0xffff },
+	{ 0x0b7, 0x00, 0, 0xffff },
+	{ 0x0d1, 0xff, 0, 0xffff },
+	{ 0x0d6, 0xff, 0, 0xffff },
+	{ 0x0db, 0xff, 0, 0xffff },
+	{ 0x0ea, 0x50, 0, 0xffff },
+	{ 0x0eb, 0x50, 0, 0xffff },
+	{ 0x0ef, 0xff, 0, 0xffff },
+	{ 0x0f8, 0x15, 0, 0xffff },
+	{ 0x0f9, 0x00, 0, 0xffff },
+	{ 0x0f0, 0x30, 0, 0xffff },
+	{ 0x184, 0xff, 0, 0xffff },
+	{ 0x186, 0xff, 0, 0xffff },
+	{ 0x1a1, 0xce, 0, 0xffff },
+	{ 0x1a2, 0x0c, 0, 0xffff },
+	{ 0x1a3, 0x0c, 0, 0xffff },
+	{ 0x1a6, 0x00, 0, 0xffff },
+	{ 0x1a7, 0x00, 0, 0xffff },
+	{ 0x1a8, 0xa4, 0, 0xffff },
+	{ 0x1a9, 0xa4, 0, 0xffff },
+	{ 0x1ab, 0x2d, 0, 0xffff },
+	{ 0x1ac, 0x2d, 0, 0xffff },
+	{ 0x1b1, 0x00, 0, 0xffff },
+	{ 0x1bb, 0x00, 0, 0xffff },
+	{ 0x1bc, 0x00, 0, 0xffff },
+	{ 0x1bd, 0x00, 0, 0xffff },
+	{ 0x1be, 0x01, 0, 0xffff },
+	{ 0x1bf, 0x01, 0, 0xffff },
+	{ 0x1c0, 0x01, 0, 0xffff },
+	{ 0x1c1, 0x01, 0, 0xffff },
+	{ 0x1c2, 0x01, 0, 0xffff },
+	{ 0x280, 0x00, 0, 0xffff },
+	{ 0x281, 0x00, 0, 0xffff },
+	{ 0x282, 0x03, 0, 0xffff },
+	{ 0x283, 0x0a, 0, 0xffff },
+	{ 0x284, 0x80, 0, 0xffff },
+	{ 0x285, 0x03, 0, 0xffff },
+	{ 0x040, 0x01, 0, 0xffff },
+};
+
+static const struct hwm_tab_entry HWM_TAB_MICRO_EARLY_STEPPING[] = {
+	{ 0x005, 0x33, 0, 0xffff },
+	{ 0x018, 0x2f, 0, 0xffff },
+	{ 0x019, 0x2f, 0, 0xffff },
+	{ 0x01a, 0x2f, 0, 0xffff },
+	{ 0x01b, 0x0f, 0, 0xffff },
+	{ 0x057, 0xff, 0, 0xffff },
+	{ 0x059, 0xff, 0, 0xffff },
+	{ 0x05b, 0xff, 0, 0xffff },
+	{ 0x05d, 0xff, 0, 0xffff },
+	{ 0x05f, 0xff, 0, 0xffff },
+	{ 0x061, 0xff, 0, 0xffff },
+	{ 0x06e, 0x01, 0, 0xffff },
+	{ 0x06f, 0x03, 0, 0xffff },
+	{ 0x070, 0x03, 0, 0xffff },
+	{ 0x071, 0x02, 0, 0xffff },
+	{ 0x072, 0x02, 0, 0xffff },
+	{ 0x073, 0x01, 0, 0xffff },
+	{ 0x074, 0x06, 0, 0xffff },
+	{ 0x075, 0x07, 0, 0xffff },
+	{ 0x080, 0x00, 0, 0xffff },
+	{ 0x081, 0x80, 0, 0xffff },
+	{ 0x082, 0x80, 0, 0xffff },
+	{ 0x083, 0xbb, 0, 0xffff },
+	{ 0x085, 0xfd, 0, 0xffff },
+	{ 0x086, 0x60, 0, 0xffff },
+	{ 0x087, 0x50, 0, 0xffff },
+	{ 0x088, 0x08, 0, 0xffff },
+	{ 0x089, 0x00, 0, 0xffff },
+	{ 0x08a, 0x73, 0, 0xffff },
+	{ 0x08b, 0x73, 0, 0xffff },
+	{ 0x08c, 0x73, 0, 0xffff },
+	{ 0x090, 0x6d, 0, 0xffff },
+	{ 0x091, 0x7a, 0, 0xffff },
+	{ 0x092, 0x6b, 0, 0xffff },
+	{ 0x093, 0xa4, 0, 0xffff },
+	{ 0x094, 0x78, 0, 0xffff },
+	{ 0x095, 0xa4, 0, 0xffff },
+	{ 0x096, 0xa4, 0, 0xffff },
+	{ 0x097, 0xa4, 0, 0xffff },
+	{ 0x098, 0xa4, 0, 0xffff },
+	{ 0x099, 0xa4, 0, 0xffff },
+	{ 0x09a, 0xa4, 0, 0xffff },
+	{ 0x09b, 0xa4, 0, 0xffff },
+	{ 0x0a0, 0x2e, 0, 0xffff },
+	{ 0x0a1, 0x00, 0, 0xffff },
+	{ 0x0a2, 0x00, 0, 0xffff },
+	{ 0x0ae, 0xa4, 0, 0xffff },
+	{ 0x0af, 0xa4, 0, 0xffff },
+	{ 0x0b0, 0xa4, 0, 0xffff },
+	{ 0x0b1, 0xa4, 0, 0xffff },
+	{ 0x0b2, 0xa4, 0, 0xffff },
+	{ 0x0b3, 0xa4, 0, 0xffff },
+	{ 0x0b6, 0x00, 0, 0xffff },
+	{ 0x0b7, 0x00, 0, 0xffff },
+	{ 0x0d1, 0xff, 0, 0xffff },
+	{ 0x0d6, 0xff, 0, 0xffff },
+	{ 0x0db, 0xff, 0, 0xffff },
+	{ 0x0ea, 0x64, 0, 0xffff },
+	{ 0x0eb, 0x64, 0, 0xffff },
+	{ 0x0ef, 0xff, 0, 0xffff },
+	{ 0x0f8, 0x15, 0, 0xffff },
+	{ 0x0f9, 0x00, 0, 0xffff },
+	{ 0x0f0, 0x30, 0, 0xffff },
+	{ 0x184, 0xff, 0, 0xffff },
+	{ 0x186, 0xff, 0, 0xffff },
+	{ 0x1a1, 0xce, 0, 0xffff },
+	{ 0x1a2, 0x0c, 0, 0xffff },
+	{ 0x1a3, 0x0c, 0, 0xffff },
+	{ 0x1a6, 0x00, 0, 0xffff },
+	{ 0x1a7, 0x00, 0, 0xffff },
+	{ 0x1a8, 0xa4, 0, 0xffff },
+	{ 0x1a9, 0xa4, 0, 0xffff },
+	{ 0x1ab, 0x2d, 0, 0xffff },
+	{ 0x1ac, 0x2d, 0, 0xffff },
+	{ 0x1b1, 0x00, 0, 0xffff },
+	{ 0x1bb, 0x00, 0, 0xffff },
+	{ 0x1bc, 0x00, 0, 0xffff },
+	{ 0x1bd, 0x00, 0, 0xffff },
+	{ 0x1be, 0x01, 0, 0xffff },
+	{ 0x1bf, 0x01, 0, 0xffff },
+	{ 0x1c0, 0x01, 0, 0xffff },
+	{ 0x1c1, 0x01, 0, 0xffff },
+	{ 0x1c2, 0x01, 0, 0xffff },
+	{ 0x280, 0x00, 0, 0xffff },
+	{ 0x281, 0x00, 0, 0xffff },
+	{ 0x282, 0x03, 0, 0xffff },
+	{ 0x283, 0x0a, 0, 0xffff },
+	{ 0x284, 0x80, 0, 0xffff },
+	{ 0x285, 0x03, 0, 0xffff },
+	{ 0x040, 0x01, 0, 0xffff },
+};
+
+static const struct hwm_tab_entry HWM_TAB_SFF[] = {
+	{ 0x019, 0x2f, 0, 0xffff },
+	{ 0x040, 0x01, 0, 0xffff },
+	{ 0x072, 0x03, 0, 0xffff },
+	{ 0x075, 0x06, 0, 0xffff },
+	{ 0x07c, 0x00, 0, 0xffff },
+	{ 0x080, 0x00, 0, 0xffff },
+	{ 0x081, 0x00, 0, 0xffff },
+	{ 0x083, 0xbb, 0, 0xffff },
+	{ 0x085, 0x59, 0, 0xffff },
+	{ 0x086, 0x6a, 0, 0xffff },
+	{ 0x087, 0xc0, 0, 0xffff },
+	{ 0x08a, 0x33, 0, 0xffff },
+	{ 0x090, 0x77, 0, 0xffff },
+	{ 0x091, 0x66, 0, 0xffff },
+	{ 0x092, 0x94, 0, 0xffff },
+	{ 0x093, 0x90, 0, 0xffff },
+	{ 0x094, 0x68, 0, 0xffff },
+	{ 0x096, 0xa4, 0, 0xffff },
+	{ 0x097, 0xa4, 0, 0xffff },
+	{ 0x098, 0xa4, 0, 0xffff },
+	{ 0x099, 0xa4, 0, 0xffff },
+	{ 0x09a, 0xa4, 0, 0xffff },
+	{ 0x09b, 0xa4, 0, 0xffff },
+	{ 0x0a0, 0x3e, 0, 0xffff },
+	{ 0x0ae, 0x86, 0, 0xffff },
+	{ 0x0af, 0x86, 0, 0xffff },
+	{ 0x0b0, 0xa4, 0, 0xffff },
+	{ 0x0b1, 0xa4, 0, 0xffff },
+	{ 0x0b2, 0x90, 0, 0xffff },
+	{ 0x0b6, 0x48, 0, 0xffff },
+	{ 0x0b7, 0x48, 0, 0xffff },
+	{ 0x0ea, 0x64, 0, 0xffff },
+	{ 0x0f0, 0x30, 0, 0xffff },
+	{ 0x1b1, 0x48, 0, 0xffff },
+	{ 0x1b8, 0x00, 0, 0xffff },
+	{ 0x1be, 0x95, 0, 0xffff },
+	{ 0x1c1, 0x90, 0, 0xffff },
+	{ 0x1c6, 0x00, 0, 0xffff },
+	{ 0x1c9, 0x00, 0, 0xffff },
+	{ 0x280, 0x68, 0, 0xffff },
+	{ 0x281, 0x10, 0, 0xffff },
+	{ 0x282, 0x03, 0, 0xffff },
+	{ 0x283, 0x0a, 0, 0xffff },
+	{ 0x284, 0x80, 0, 0xffff },
+	{ 0x285, 0x03, 0, 0xffff}
+};
+
+static const struct hwm_tab_entry HWM_TAB_MT[] = {
+	{ 0x005, 0x33, 0, 0xffff },
+	{ 0x018, 0x2f, 0, 0xffff },
+	{ 0x019, 0x2f, 0, 0xffff },
+	{ 0x01a, 0x2f, 0, 0xffff },
+	{ 0x080, 0x00, 0, 0xffff },
+	{ 0x081, 0x00, 0, 0xffff },
+	{ 0x082, 0x80, 0, 0xffff },
+	{ 0x083, 0xbb, 0, 0xffff },
+	{ 0x085, 0xb9, 0, 0x0010 },
+	{ 0x086, 0xac, 0, 0x0010 },
+	{ 0x087, 0x87, 0, 0x0010 },
+	{ 0x08a, 0x51, 0, 0x0010 },
+	{ 0x08b, 0x39, 0, 0x0010 },
+	{ 0x090, 0x78, 0, 0xffff },
+	{ 0x091, 0x6a, 0, 0xffff },
+	{ 0x092, 0x8f, 0, 0xffff },
+	{ 0x094, 0x68, 0, 0xffff },
+	{ 0x095, 0x5b, 0, 0xffff },
+	{ 0x096, 0x92, 0, 0xffff },
+	{ 0x097, 0x86, 0, 0xffff },
+	{ 0x098, 0xa4, 0, 0xffff },
+	{ 0x09a, 0x8b, 0, 0xffff },
+	{ 0x0a0, 0x0a, 0, 0xffff },
+	{ 0x0a1, 0x26, 0, 0xffff },
+	{ 0x0a2, 0xd1, 0, 0xffff },
+	{ 0x0ae, 0x7c, 0, 0xffff },
+	{ 0x0af, 0x7c, 0, 0xffff },
+	{ 0x0b0, 0x9a, 0, 0xffff },
+	{ 0x0b3, 0x7c, 0, 0xffff },
+	{ 0x0b6, 0x08, 0, 0xffff },
+	{ 0x0b7, 0x00, 0, 0xffff },
+	{ 0x0ea, 0x64, 0, 0xffff },
+	{ 0x0ef, 0xff, 0, 0xffff },
+	{ 0x0f8, 0x15, 0, 0xffff },
+	{ 0x0f9, 0x00, 0, 0xffff },
+	{ 0x0f0, 0x30, 0, 0xffff },
+	{ 0x0fd, 0x01, 0, 0xffff },
+	{ 0x1a1, 0x99, 0, 0xffff },
+	{ 0x1a2, 0x00, 0, 0xffff },
+	{ 0x1a4, 0x00, 0, 0xffff },
+	{ 0x1b1, 0x00, 0, 0xffff },
+	{ 0x1be, 0x90, 0, 0xffff },
+	{ 0x280, 0xc4, 0, 0xffff },
+	{ 0x281, 0x09, 0, 0xffff },
+	{ 0x282, 0x0a, 0, 0xffff },
+	{ 0x283, 0x14, 0, 0xffff },
+	{ 0x284, 0x01, 0, 0xffff },
+	{ 0x285, 0x01, 0, 0xffff },
+	{ 0x288, 0x94, 0, 0xffff },
+	{ 0x289, 0x11, 0, 0xffff },
+	{ 0x28a, 0x0a, 0, 0xffff },
+	{ 0x28b, 0x14, 0, 0xffff },
+	{ 0x28c, 0x01, 0, 0xffff },
+	{ 0x28d, 0x01, 0, 0xffff },
+	{ 0x294, 0x24, 0, 0xffff },
+};
+
+static uint8_t get_temp_target(void)
+{
+	uint8_t val = rdmsr(0x1a2).lo >> 8 & 0xff;
+	if (!val)
+		val = 20;
+	return 0x95 - val;
+}
+
+static uint16_t get_pkg_power(void)
+{
+	const unsigned int pkg_power = rdmsr(0x614).lo & 0x7fff;
+	const unsigned int power_unit = 1 << (rdmsr(0x606).lo & 0xf);
+	if (pkg_power / power_unit > 65)
+		return 32;
+	else
+		return 16;
+}
+
+static uint8_t get_core_cnt(void)
+{
+	// Intel describes this CPUID field as:
+	// > Maximum number of addressable IDs for processor cores in the physical package
+	if (cpuid(0).eax >= 4)
+		return cpuid_ext(4, 0).eax >> 26;
+	return 0;
+}
+
+static void apply_hwm_tab(const struct hwm_tab_entry *arr, size_t size)
+{
+	uint8_t temp_target = get_temp_target();
+	uint16_t pkg_power = get_pkg_power();
+
+	printk(BIOS_DEBUG, "Temp target = %#x\n", temp_target);
+	printk(BIOS_DEBUG, "Package power = %#x\n", pkg_power);
+
+	for (size_t i = 0; i < size; ++i) {
+		// Skip entry if it doesn't apply for this package power
+		if (arr[i].pkg_power != pkg_power &&
+		    arr[i].pkg_power != HWM_TAB_PKG_POWER_ANY)
+			continue;
+
+		uint8_t val = arr[i].val;
+
+		// Add temp target to value if requested (current tables never do)
+		if (arr[i].flags & HWM_TAB_ADD_TEMP_TARGET)
+			val += temp_target;
+
+		// Perform write
+		sch5555_mbox_write(1, arr[i].addr, val);
+	}
+}
+
+static void sch5555_ec_hwm_init(void *arg)
+{
+	uint8_t form_fac_id, saved_2fc, core_cnt;
+
+	printk(BIOS_DEBUG, "OptiPlex 3050 late HWM init\n");
+
+	form_fac_id = gpio_get(GPP_G2) | gpio_get(GPP_G3) << 1;
+	printk(BIOS_DEBUG, "Form Factor ID = %#x\n", form_fac_id);
+
+	saved_2fc = sch5555_mbox_read(1, 0x2fc);
+	sch5555_mbox_write(1, 0x2fc, 0xa0);
+	sch5555_mbox_write(1, 0x2fd, 0x32);
+
+	switch (form_fac_id) {
+	case FORM_FACTOR_MICRO:
+		// CPU stepping <= 3
+		if ((cpuid(1).eax & 0xf) <= 3)
+			apply_hwm_tab(HWM_TAB_MICRO_EARLY_STEPPING, ARRAY_SIZE(HWM_TAB_MICRO_EARLY_STEPPING));
+		// Tjunction == 80
+		else if ((rdmsr(0x1a2).lo >> 16 & 0xff) == 80)
+			apply_hwm_tab(HWM_TAB_MICRO_TEMP80, ARRAY_SIZE(HWM_TAB_MICRO_TEMP80));
+		else
+			apply_hwm_tab(HWM_TAB_MICRO_BASE, ARRAY_SIZE(HWM_TAB_MICRO_BASE));
+		break;
+	case FORM_FACTOR_SFF:
+		apply_hwm_tab(HWM_TAB_SFF, ARRAY_SIZE(HWM_TAB_SFF));
+		break;
+	default:
+		apply_hwm_tab(HWM_TAB_MT, ARRAY_SIZE(HWM_TAB_MT));
+		break;
+	}
+
+	core_cnt = get_core_cnt();
+	printk(BIOS_DEBUG, "CPU Core Count = %#x\n", core_cnt);
+	if (core_cnt > 2) {
+		sch5555_mbox_write(1, 0x9e, 0x30);
+		sch5555_mbox_write(1, 0xeb, sch5555_mbox_read(1, 0xea));
+	}
+
+	sch5555_mbox_write(1, 0x2fc, saved_2fc);
+	sch5555_mbox_read(1, 0xb8);
+}
+
+BOOT_STATE_INIT_ENTRY(BS_POST_DEVICE, BS_ON_EXIT, sch5555_ec_hwm_init, NULL);
diff --git a/src/mainboard/dell/optiplex_3050/romstage.c b/src/mainboard/dell/optiplex_3050/romstage.c
new file mode 100644
index 0000000000..501b254232
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/romstage.c
@@ -0,0 +1,18 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <soc/romstage.h>
+#include <spd_bin.h>
+
+void mainboard_memory_init_params(FSPM_UPD *mupd)
+{
+	struct spd_block blk = { .addr_map = { 0x50, 0x52, } };
+	get_spd_smbus(&blk);
+	dump_spd_info(&blk);
+
+	FSP_M_CONFIG *mem_cfg = &mupd->FspmConfig;
+	mem_cfg->DqPinsInterleaved = true;
+	mem_cfg->CaVrefConfig      = 2;
+	mem_cfg->MemorySpdDataLen  = blk.len;
+	mem_cfg->MemorySpdPtr00    = (uintptr_t)blk.spd_array[0];
+	mem_cfg->MemorySpdPtr10    = (uintptr_t)blk.spd_array[1];
+}
diff --git a/src/mainboard/dell/optiplex_3050/sch5555_ec.c b/src/mainboard/dell/optiplex_3050/sch5555_ec.c
new file mode 100644
index 0000000000..1df5026531
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/sch5555_ec.c
@@ -0,0 +1,54 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#include <arch/io.h>
+#include <device/pnp_ops.h>
+#include <superio/smsc/sch555x/sch555x.h>
+#include "sch5555_ec.h"
+
+uint8_t sch5555_mbox_read(uint8_t addr1, uint16_t addr2)
+{
+	// clear ec-to-host mailbox
+	uint8_t tmp = inb(SCH555x_EMI_IOBASE + 1);
+	outb(tmp, SCH555x_EMI_IOBASE + 1);
+
+	// send address
+	outw(0 | 0x8001, SCH555x_EMI_IOBASE + 2);
+	outw((addr1 * 2) | 0x100, SCH555x_EMI_IOBASE + 4);
+
+	outw(4 | 0x8002, SCH555x_EMI_IOBASE + 2);
+	outl(addr2 << 16, SCH555x_EMI_IOBASE + 4);
+
+	// send message to ec
+	outb(1, SCH555x_EMI_IOBASE);
+
+	// wait for ack
+	for (size_t retry = 0; retry < 0xfff; ++retry)
+		if (inb(SCH555x_EMI_IOBASE + 1) & 1)
+			break;
+
+	// read result
+	outw(4 | 0x8000, SCH555x_EMI_IOBASE + 2);
+	return inb(SCH555x_EMI_IOBASE + 4);
+}
+
+void sch5555_mbox_write(uint8_t addr1, uint16_t addr2, uint8_t val)
+{
+	// clear ec-to-host mailbox
+	uint8_t tmp = inb(SCH555x_EMI_IOBASE + 1);
+	outb(tmp, SCH555x_EMI_IOBASE + 1);
+
+	// send address and value
+	outw(0 | 0x8001, SCH555x_EMI_IOBASE + 2);
+	outw((addr1 * 2) | 0x101, SCH555x_EMI_IOBASE + 4);
+
+	outw(4 | 0x8002, SCH555x_EMI_IOBASE + 2);
+	outl(val | (addr2 << 16), SCH555x_EMI_IOBASE + 4);
+
+	// send message to ec
+	outb(1, SCH555x_EMI_IOBASE);
+
+	// wait for ack
+	for (size_t retry = 0; retry < 0xfff; ++retry)
+		if (inb(SCH555x_EMI_IOBASE + 1) & 1)
+			break;
+}
diff --git a/src/mainboard/dell/optiplex_3050/sch5555_ec.h b/src/mainboard/dell/optiplex_3050/sch5555_ec.h
new file mode 100644
index 0000000000..9d262d5787
--- /dev/null
+++ b/src/mainboard/dell/optiplex_3050/sch5555_ec.h
@@ -0,0 +1,10 @@
+/* SPDX-License-Identifier: GPL-2.0-only */
+
+#ifndef __SCH5555_EC_H__
+#define __SCH5555_EC_H__
+
+uint8_t sch5555_mbox_read(uint8_t addr1, uint16_t addr2);
+
+void sch5555_mbox_write(uint8_t addr1, uint16_t addr2, uint8_t val);
+
+#endif
-- 
2.39.5

