From 81ae1f94aa00121cedd839540c5d7839a485d61e Mon Sep 17 00:00:00 2001
From: Leah Rowe <info@minifree.org>
Date: Wed, 5 Aug 2015 00:49:12 +0100
Subject: [PATCH 1/7] mainboards/lenovo: Copy X200 board to R500 for future
 expansion

Change-Id: I45633be3d8548c211360c2ffc3ad4e5f10a6df0f
Signed-off-by: Leah Rowe <info@minifree.org>
---
 src/mainboard/lenovo/r500/Kconfig                |  51 ++++++
 src/mainboard/lenovo/r500/Kconfig.name           |   2 +
 src/mainboard/lenovo/r500/Makefile.inc           |  21 +++
 src/mainboard/lenovo/r500/acpi/dock.asl          |  72 ++++++++
 src/mainboard/lenovo/r500/acpi/ec.asl            |   1 +
 src/mainboard/lenovo/r500/acpi/gm45_pci_irqs.asl |  84 +++++++++
 src/mainboard/lenovo/r500/acpi/gpe.asl           |  28 +++
 src/mainboard/lenovo/r500/acpi/ich9_pci_irqs.asl | 108 +++++++++++
 src/mainboard/lenovo/r500/acpi/platform.asl      | 205 +++++++++++++++++++++
 src/mainboard/lenovo/r500/acpi/superio.asl       |   0
 src/mainboard/lenovo/r500/acpi_tables.c          |  71 ++++++++
 src/mainboard/lenovo/r500/board_info.txt         |   6 +
 src/mainboard/lenovo/r500/cmos.default           |  16 ++
 src/mainboard/lenovo/r500/cmos.layout            | 144 +++++++++++++++
 src/mainboard/lenovo/r500/cstates.c              |  41 +++++
 src/mainboard/lenovo/r500/devicetree.cb          | 222 +++++++++++++++++++++++
 src/mainboard/lenovo/r500/dock.c                 |  64 +++++++
 src/mainboard/lenovo/r500/dock.h                 |  26 +++
 src/mainboard/lenovo/r500/dsdt.asl               |  58 ++++++
 src/mainboard/lenovo/r500/fadt.c                 | 157 ++++++++++++++++
 src/mainboard/lenovo/r500/hda_verb.c             |  51 ++++++
 src/mainboard/lenovo/r500/mainboard.c            |  49 +++++
 src/mainboard/lenovo/r500/mptable.c              |   1 +
 src/mainboard/lenovo/r500/romstage.c             | 203 +++++++++++++++++++++
 src/mainboard/lenovo/r500/smihandler.c           |  49 +++++
 25 files changed, 1730 insertions(+)
 create mode 100644 src/mainboard/lenovo/r500/Kconfig
 create mode 100644 src/mainboard/lenovo/r500/Kconfig.name
 create mode 100644 src/mainboard/lenovo/r500/Makefile.inc
 create mode 100644 src/mainboard/lenovo/r500/acpi/dock.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi/ec.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi/gm45_pci_irqs.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi/gpe.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi/ich9_pci_irqs.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi/platform.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi/superio.asl
 create mode 100644 src/mainboard/lenovo/r500/acpi_tables.c
 create mode 100644 src/mainboard/lenovo/r500/board_info.txt
 create mode 100644 src/mainboard/lenovo/r500/cmos.default
 create mode 100644 src/mainboard/lenovo/r500/cmos.layout
 create mode 100644 src/mainboard/lenovo/r500/cstates.c
 create mode 100644 src/mainboard/lenovo/r500/devicetree.cb
 create mode 100644 src/mainboard/lenovo/r500/dock.c
 create mode 100644 src/mainboard/lenovo/r500/dock.h
 create mode 100644 src/mainboard/lenovo/r500/dsdt.asl
 create mode 100644 src/mainboard/lenovo/r500/fadt.c
 create mode 100644 src/mainboard/lenovo/r500/hda_verb.c
 create mode 100644 src/mainboard/lenovo/r500/mainboard.c
 create mode 100644 src/mainboard/lenovo/r500/mptable.c
 create mode 100644 src/mainboard/lenovo/r500/romstage.c
 create mode 100644 src/mainboard/lenovo/r500/smihandler.c

diff --git a/src/mainboard/lenovo/r500/Kconfig b/src/mainboard/lenovo/r500/Kconfig
new file mode 100644
index 0000000..7bae12d
--- /dev/null
+++ b/src/mainboard/lenovo/r500/Kconfig
@@ -0,0 +1,51 @@
+if BOARD_LENOVO_X200
+
+config BOARD_SPECIFIC_OPTIONS # dummy
+	def_bool y
+	select SYSTEM_TYPE_LAPTOP
+	select CPU_INTEL_SOCKET_BGA956
+	select NORTHBRIDGE_INTEL_GM45
+	select SOUTHBRIDGE_INTEL_I82801IX
+	select EC_LENOVO_PMH7
+	select EC_LENOVO_H8
+	select NO_UART_ON_SUPERIO
+	select DRIVERS_ICS_954309
+	select BOARD_ROMSIZE_KB_8192
+	select DRIVERS_GENERIC_IOAPIC
+	select HAVE_MP_TABLE
+	select HAVE_ACPI_TABLES
+	select EC_ACPI
+	select HAVE_OPTION_TABLE
+	select HAVE_CMOS_DEFAULT
+	select HAVE_ACPI_RESUME
+	select MAINBOARD_HAS_NATIVE_VGA_INIT
+	select MAINBOARD_HAS_NATIVE_VGA_INIT_TEXTMODECFG
+	select INTEL_INT15
+	select SUPERIO_NSC_PC87382
+	select DRIVERS_LENOVO_WACOM
+
+config MAINBOARD_DIR
+	string
+	default lenovo/x200
+
+config MAINBOARD_PART_NUMBER
+	string
+	default "ThinkPad X200"
+
+config MMCONF_BASE_ADDRESS
+	hex
+	default 0xf0000000
+
+config USBDEBUG_HCD_INDEX
+	int
+	default 2
+
+config MAX_CPUS
+	int
+	default 2
+
+config CBFS_SIZE
+	hex
+	default 0x200000
+
+endif # BOARD_LENOVO_X200
diff --git a/src/mainboard/lenovo/r500/Kconfig.name b/src/mainboard/lenovo/r500/Kconfig.name
new file mode 100644
index 0000000..8e1dd43
--- /dev/null
+++ b/src/mainboard/lenovo/r500/Kconfig.name
@@ -0,0 +1,2 @@
+config BOARD_LENOVO_X200
+	bool "ThinkPad X200 / X200t"
diff --git a/src/mainboard/lenovo/r500/Makefile.inc b/src/mainboard/lenovo/r500/Makefile.inc
new file mode 100644
index 0000000..b2e5c2a
--- /dev/null
+++ b/src/mainboard/lenovo/r500/Makefile.inc
@@ -0,0 +1,21 @@
+##
+## This file is part of the coreboot project.
+##
+## Copyright (C) 2012 secunet Security Networks AG
+##
+## This program is free software; you can redistribute it and/or modify
+## it under the terms of the GNU General Public License as published by
+## the Free Software Foundation; version 2 of the License.
+##
+## This program is distributed in the hope that it will be useful,
+## but WITHOUT ANY WARRANTY; without even the implied warranty of
+## MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+## GNU General Public License for more details.
+##
+## You should have received a copy of the GNU General Public License
+## along with this program; if not, write to the Free Software
+## Foundation, Inc.
+##
+
+ramstage-y += dock.c
+ramstage-y += cstates.c
diff --git a/src/mainboard/lenovo/r500/acpi/dock.asl b/src/mainboard/lenovo/r500/acpi/dock.asl
new file mode 100644
index 0000000..f817acf
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi/dock.asl
@@ -0,0 +1,72 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (c) 2011 Sven Schnelle <svens@stackframe.org>
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+Scope (\_SB)
+{
+	Device(DOCK)
+	{
+		Name(_HID, "ACPI0003")
+		Name(_UID, 0x00)
+		Name(_PCL, Package() { \_SB } )
+
+		Method(_DCK, 1, NotSerialized)
+		{
+			if (Arg0) {
+			   /* connect dock */
+			   Store (1, \GP28)
+			   Store (1, \_SB.PCI0.LPCB.EC.DKR1)
+			} else {
+			   /* disconnect dock */
+			   Store (0, \GP28)
+			   Store (0, \_SB.PCI0.LPCB.EC.DKR1)
+			}
+			Xor(Arg0, \_SB.PCI0.LPCB.EC.DKR1, Local0)
+			Return (Local0)
+		}
+
+		Method(_STA, 0, NotSerialized)
+		{
+			Return (\_SB.PCI0.LPCB.EC.DKR1)
+		}
+	}
+}
+
+Scope(\_SB.PCI0.LPCB.EC)
+{
+	Method(_Q18, 0, NotSerialized)
+	{
+		Notify(\_SB.DOCK, 3)
+	}
+
+	Method(_Q45, 0, NotSerialized)
+	{
+		Notify(\_SB.DOCK, 3)
+	}
+
+	Method(_Q58, 0, NotSerialized)
+	{
+		Notify(\_SB.DOCK, 0)
+	}
+
+	Method(_Q37, 0, NotSerialized)
+	{
+		Notify(\_SB.DOCK, 0)
+	}
+}
diff --git a/src/mainboard/lenovo/r500/acpi/ec.asl b/src/mainboard/lenovo/r500/acpi/ec.asl
new file mode 100644
index 0000000..c3569e8
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi/ec.asl
@@ -0,0 +1 @@
+#include <ec/lenovo/h8/acpi/ec.asl>
diff --git a/src/mainboard/lenovo/r500/acpi/gm45_pci_irqs.asl b/src/mainboard/lenovo/r500/acpi/gm45_pci_irqs.asl
new file mode 100644
index 0000000..93b4525
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi/gm45_pci_irqs.asl
@@ -0,0 +1,84 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2009 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+/* This is board specific information: IRQ routing for the
+ * gm45
+ */
+
+
+// PCI Interrupt Routing
+Method(_PRT)
+{
+	If (PICM) {
+		Return (Package() {
+			// PCIe Graphics		0:1.0
+			Package() { 0x0001ffff, 0, 0, 16 },
+			// Onboard graphics (IGD)	0:2.0
+			Package() { 0x0002ffff, 0, 0, 16 },
+			// USB and EHCI			0:1a.x
+			Package() { 0x001affff, 0, 0, 16 },
+			Package() { 0x001affff, 1, 0, 17 },
+			Package() { 0x001affff, 2, 0, 18 },
+			// High Definition Audio	0:1b.0
+			Package() { 0x001bffff, 0, 0, 16 },
+			// PCIe Root Ports		0:1c.x
+			Package() { 0x001cffff, 0, 0, 16 },
+			// USB and EHCI			0:1d.x
+			Package() { 0x001dffff, 0, 0, 16 },
+			Package() { 0x001dffff, 1, 0, 17 },
+			Package() { 0x001dffff, 2, 0, 18 },
+			// FIXME
+			// CardBus/IEEE1394		0:1e.2, 0:1e.3
+			// Package() { 0x001effff, 0, 0, 22 },
+			// Package() { 0x001effff, 1, 0, 20 },
+			// LPC device			0:1f.0
+			Package() { 0x001fffff, 0, 0, 16 },
+			Package() { 0x001fffff, 1, 0, 17 },
+			Package() { 0x001fffff, 2, 0, 18 }
+		})
+	} Else {
+		Return (Package() {
+			// PCIe Graphics		0:1.0
+			Package() { 0x0001ffff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			// Onboard graphics (IGD)	0:2.0
+			Package() { 0x0002ffff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			// USB and EHCI			0:1a.x
+			Package() { 0x001affff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			Package() { 0x001affff, 1, \_SB.PCI0.LPCB.LNKB, 0 },
+			Package() { 0x001affff, 2, \_SB.PCI0.LPCB.LNKC, 0 },
+			// High Definition Audio	0:1b.0
+			Package() { 0x001bffff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			// PCIe Root Ports		0:1c.x
+			Package() { 0x001cffff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			// USB and EHCI			0:1d.x
+			Package() { 0x001dffff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			Package() { 0x001dffff, 1, \_SB.PCI0.LPCB.LNKB, 0 },
+			Package() { 0x001dffff, 2, \_SB.PCI0.LPCB.LNKC, 0 },
+			// FIXME
+			// CardBus/IEEE1394		0:1e.2, 0:1e.3
+			// Package() { 0x001effff, 0, \_SB.PCI0.LPCB.LNKG, 0 },
+			// Package() { 0x001effff, 1, \_SB.PCI0.LPCB.LNKE, 0 },
+			// LPC device			0:1f.0
+			Package() { 0x001fffff, 0, \_SB.PCI0.LPCB.LNKA, 0 },
+			Package() { 0x001fffff, 1, \_SB.PCI0.LPCB.LNKB, 0 },
+			Package() { 0x001fffff, 2, \_SB.PCI0.LPCB.LNKC, 0 }
+		})
+	}
+}
diff --git a/src/mainboard/lenovo/r500/acpi/gpe.asl b/src/mainboard/lenovo/r500/acpi/gpe.asl
new file mode 100644
index 0000000..e1c806f
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi/gpe.asl
@@ -0,0 +1,28 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (c) 2011 Sven Schnelle <svens@stackframe.org>
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+Scope (\_GPE)
+{
+	Method(_L18, 0, NotSerialized)
+	{
+		/* Read EC register to clear wake status */
+		Store(\_SB.PCI0.LPCB.EC.WAKE, Local0)
+	}
+}
diff --git a/src/mainboard/lenovo/r500/acpi/ich9_pci_irqs.asl b/src/mainboard/lenovo/r500/acpi/ich9_pci_irqs.asl
new file mode 100644
index 0000000..3ef5d3b
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi/ich9_pci_irqs.asl
@@ -0,0 +1,108 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2009 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+/* This is board specific information: IRQ routing for the
+ * 0:1e.0 PCI bridge of the ICH9
+ */
+
+/* TODO: which slots are actually relevant? */
+If (PICM) {
+	Return (Package() {
+		// PCI Slot 1 routes ABCD
+		Package() { 0x0000ffff, 0, 0, 16},
+		Package() { 0x0000ffff, 1, 0, 17},
+		Package() { 0x0000ffff, 2, 0, 18},
+		Package() { 0x0000ffff, 3, 0, 19},
+
+		// PCI Slot 2 routes BCDA
+		Package() { 0x0001ffff, 0, 0, 17},
+		Package() { 0x0001ffff, 1, 0, 18},
+		Package() { 0x0001ffff, 2, 0, 19},
+		Package() { 0x0001ffff, 3, 0, 16},
+
+		// PCI Slot 3 routes CDAB
+		Package() { 0x0002ffff, 0, 0, 18},
+		Package() { 0x0002ffff, 1, 0, 19},
+		Package() { 0x0002ffff, 2, 0, 16},
+		Package() { 0x0002ffff, 3, 0, 17},
+
+		// PCI Slot 4 routes ABCD
+		Package() { 0x0003ffff, 0, 0, 16},
+		Package() { 0x0003ffff, 1, 0, 17},
+		Package() { 0x0003ffff, 2, 0, 18},
+		Package() { 0x0003ffff, 3, 0, 19},
+
+		// PCI Slot 5 routes ABCD
+		Package() { 0x0004ffff, 0, 0, 16},
+		Package() { 0x0004ffff, 1, 0, 17},
+		Package() { 0x0004ffff, 2, 0, 18},
+		Package() { 0x0004ffff, 3, 0, 19},
+
+		// PCI Slot 6 routes BCDA
+		Package() { 0x0005ffff, 0, 0, 17},
+		Package() { 0x0005ffff, 1, 0, 18},
+		Package() { 0x0005ffff, 2, 0, 19},
+		Package() { 0x0005ffff, 3, 0, 16},
+
+		// FIXME: what's this supposed to mean? (adopted from ich7)
+		//Package() { 0x0008ffff, 0, 0, 20},
+	})
+} Else {
+	Return (Package() {
+		// PCI Slot 1 routes ABCD
+		Package() { 0x0000ffff, 0, \_SB.PCI0.LPCB.LNKA, 0},
+		Package() { 0x0000ffff, 1, \_SB.PCI0.LPCB.LNKB, 0},
+		Package() { 0x0000ffff, 2, \_SB.PCI0.LPCB.LNKC, 0},
+		Package() { 0x0000ffff, 3, \_SB.PCI0.LPCB.LNKD, 0},
+
+		// PCI Slot 2 routes BCDA
+		Package() { 0x0001ffff, 0, \_SB.PCI0.LPCB.LNKB, 0},
+		Package() { 0x0001ffff, 1, \_SB.PCI0.LPCB.LNKC, 0},
+		Package() { 0x0001ffff, 2, \_SB.PCI0.LPCB.LNKD, 0},
+		Package() { 0x0001ffff, 3, \_SB.PCI0.LPCB.LNKA, 0},
+
+		// PCI Slot 3 routes CDAB
+		Package() { 0x0002ffff, 0, \_SB.PCI0.LPCB.LNKC, 0},
+		Package() { 0x0002ffff, 1, \_SB.PCI0.LPCB.LNKD, 0},
+		Package() { 0x0002ffff, 2, \_SB.PCI0.LPCB.LNKA, 0},
+		Package() { 0x0002ffff, 3, \_SB.PCI0.LPCB.LNKB, 0},
+
+		// PCI Slot 4 routes ABCD
+		Package() { 0x0003ffff, 0, \_SB.PCI0.LPCB.LNKA, 0},
+		Package() { 0x0003ffff, 1, \_SB.PCI0.LPCB.LNKB, 0},
+		Package() { 0x0003ffff, 2, \_SB.PCI0.LPCB.LNKC, 0},
+		Package() { 0x0003ffff, 3, \_SB.PCI0.LPCB.LNKD, 0},
+
+		// PCI Slot 5 routes ABCD
+		Package() { 0x0004ffff, 0, \_SB.PCI0.LPCB.LNKA, 0},
+		Package() { 0x0004ffff, 1, \_SB.PCI0.LPCB.LNKB, 0},
+		Package() { 0x0004ffff, 2, \_SB.PCI0.LPCB.LNKC, 0},
+		Package() { 0x0004ffff, 3, \_SB.PCI0.LPCB.LNKD, 0},
+
+		// PCI Slot 6 routes BCDA
+		Package() { 0x0005ffff, 0, \_SB.PCI0.LPCB.LNKB, 0},
+		Package() { 0x0005ffff, 1, \_SB.PCI0.LPCB.LNKC, 0},
+		Package() { 0x0005ffff, 2, \_SB.PCI0.LPCB.LNKD, 0},
+		Package() { 0x0005ffff, 3, \_SB.PCI0.LPCB.LNKA, 0},
+
+		// FIXME
+		// Package() { 0x0008ffff, 0, \_SB.PCI0.LPCB.LNKE, 0},
+	})
+}
diff --git a/src/mainboard/lenovo/r500/acpi/platform.asl b/src/mainboard/lenovo/r500/acpi/platform.asl
new file mode 100644
index 0000000..d5cb076
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi/platform.asl
@@ -0,0 +1,205 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2009 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+/* These come from the dynamically created CPU SSDT */
+External(PDC0)
+External(PDC1)
+
+/* The APM port can be used for generating software SMIs */
+
+OperationRegion (APMP, SystemIO, 0xb2, 2)
+Field (APMP, ByteAcc, NoLock, Preserve)
+{
+	APMC, 8,	// APM command
+	APMS, 8		// APM status
+}
+
+/* Port 80 POST */
+
+OperationRegion (POST, SystemIO, 0x80, 1)
+Field (POST, ByteAcc, Lock, Preserve)
+{
+	DBG0, 8
+}
+
+/* SMI I/O Trap */
+Method(TRAP, 1, Serialized)
+{
+	Store (Arg0, SMIF)	// SMI Function
+	Store (0, TRP0)		// Generate trap
+	Return (SMIF)		// Return value of SMI handler
+}
+
+/* The _PIC method is called by the OS to choose between interrupt
+ * routing via the i8259 interrupt controller or the APIC.
+ *
+ * _PIC is called with a parameter of 0 for i8259 configuration and
+ * with a parameter of 1 for Local Apic/IOAPIC configuration.
+ */
+
+Method(_PIC, 1)
+{
+	// Remember the OS' IRQ routing choice.
+	Store(Arg0, PICM)
+}
+
+/* The _PTS method (Prepare To Sleep) is called before the OS is
+ * entering a sleep state. The sleep state number is passed in Arg0
+ */
+
+Method(_PTS,1)
+{
+	// Call a trap so SMI can prepare for Sleep as well.
+	// TRAP(0x55)
+	\_SB.PCI0.LPCB.EC.RADI(0)
+}
+
+/* The _WAK method is called on system wakeup */
+
+Method(_WAK,1)
+{
+	// CPU specific part
+
+	// Notify PCI Express slots in case a card
+	// was inserted while a sleep state was active.
+
+	// Are we going to S3?
+	If (LEqual(Arg0, 3)) {
+		// ..
+	}
+
+	// Are we going to S4?
+	If (LEqual(Arg0, 4)) {
+		// ..
+	}
+
+	// TODO: Windows XP SP2 P-State restore
+
+	// TODO: Return Arg0 as second value if S-Arg0 was entered
+	// before.
+
+	Return(Package(){0,0})
+}
+
+// Power notification
+
+External (\_PR_.CP00, DeviceObj)
+External (\_PR_.CP01, DeviceObj)
+
+Method (PNOT)
+{
+	If (MPEN) {
+		If(And(PDC0, 0x08)) {
+			Notify (\_PR_.CP00, 0x80)	 // _PPC
+
+			If (And(PDC0, 0x10)) {
+				Sleep(100)
+				Notify(\_PR_.CP00, 0x81) // _CST
+			}
+		}
+
+		If(And(PDC1, 0x08)) {
+			Notify (\_PR_.CP01, 0x80)	 // _PPC
+			If (And(PDC1, 0x10)) {
+				Sleep(100)
+				Notify(\_PR_.CP01, 0x81) // _CST
+			}
+		}
+
+	} Else { // UP
+		Notify (\_PR_.CP00, 0x80)
+		Sleep(0x64)
+		Notify(\_PR_.CP00, 0x81)
+	}
+
+}
+
+/* System Bus */
+
+Scope(\_SB)
+{
+	/* This method is placed on the top level, so we can make sure it's the
+	 * first executed _INI method.
+	 */
+	Method(_INI, 0)
+	{
+		/* The DTS data in NVS is probably not up to date.
+		 * Update temperature values and make sure AP thermal
+		 * interrupts can happen
+		 */
+
+		// TRAP(71) // TODO
+
+		/* Determine the Operating System and save the value in OSYS.
+		 * We have to do this in order to be able to work around
+		 * certain windows bugs.
+		 *
+		 *    OSYS value | Operating System
+		 *    -----------+------------------
+		 *       2000    | Windows 2000
+		 *       2001    | Windows XP(+SP1)
+		 *       2002    | Windows XP SP2
+		 *       2006    | Windows Vista
+		 *       ????    | Windows 7
+		 */
+
+		/* Let's assume we're running at least Windows 2000 */
+		Store (2000, OSYS)
+
+		If (CondRefOf(_OSI, Local0)) {
+			/* Linux answers _OSI with "True" for a couple of
+			 * Windows version queries. But unlike Windows it
+			 * needs a Video repost, so let's determine whether
+			 * we're running Linux.
+			 */
+
+			If (_OSI("Linux")) {
+				Store (1, LINX)
+			}
+
+			If (_OSI("Windows 2001")) {
+				Store (2001, OSYS)
+			}
+
+			If (_OSI("Windows 2001 SP1")) {
+				Store (2001, OSYS)
+			}
+
+			If (_OSI("Windows 2001 SP2")) {
+				Store (2002, OSYS)
+			}
+
+			If (_OSI("Windows 2006")) {
+				Store (2006, OSYS)
+			}
+		}
+
+		/* And the OS workarounds start right after we know what we're
+		 * running: Windows XP SP1 needs to have C-State coordination
+		 * enabled in SMM.
+		 */
+		If (LAnd(LEqual(OSYS, 2001), MPEN)) {
+			// TRAP(61) // TODO
+		}
+
+		/* SMM power state and C4-on-C3 settings need to be updated */
+		// TRAP(43) // TODO
+	}
+}
diff --git a/src/mainboard/lenovo/r500/acpi/superio.asl b/src/mainboard/lenovo/r500/acpi/superio.asl
new file mode 100644
index 0000000..e69de29
diff --git a/src/mainboard/lenovo/r500/acpi_tables.c b/src/mainboard/lenovo/r500/acpi_tables.c
new file mode 100644
index 0000000..fa69e7a
--- /dev/null
+++ b/src/mainboard/lenovo/r500/acpi_tables.c
@@ -0,0 +1,71 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2009 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#include <string.h>
+#include <console/console.h>
+#include <arch/io.h>
+#include <arch/ioapic.h>
+#include <arch/acpi.h>
+#include <arch/acpigen.h>
+#include <arch/smp/mpspec.h>
+#include <device/device.h>
+#include <device/pci.h>
+#include <device/pci_ids.h>
+
+#include "southbridge/intel/i82801ix/nvs.h"
+void acpi_create_gnvs(global_nvs_t *gnvs)
+{
+	memset((void *)gnvs, 0, sizeof(*gnvs));
+	gnvs->apic = 1;
+	gnvs->mpen = 1; /* Enable Multi Processing */
+
+	/* Enable both COM ports */
+	gnvs->cmap = 0x01;
+	gnvs->cmbp = 0x01;
+
+}
+
+unsigned long acpi_fill_madt(unsigned long current)
+{
+	/* Local APICs */
+	current = acpi_create_madt_lapics(current);
+
+	/* IOAPIC */
+	current += acpi_create_madt_ioapic((acpi_madt_ioapic_t *) current,
+				2, IO_APIC_ADDR, 0);
+
+	/* LAPIC_NMI */
+	current += acpi_create_madt_lapic_nmi((acpi_madt_lapic_nmi_t *)
+				current, 0,
+				MP_IRQ_POLARITY_HIGH |
+				MP_IRQ_TRIGGER_EDGE, 0x01);
+	current += acpi_create_madt_lapic_nmi((acpi_madt_lapic_nmi_t *)
+				current, 1, MP_IRQ_POLARITY_HIGH |
+				MP_IRQ_TRIGGER_EDGE, 0x01);
+
+	/* INT_SRC_OVR */
+	current += acpi_create_madt_irqoverride((acpi_madt_irqoverride_t *)
+		 current, 0, 0, 2, MP_IRQ_POLARITY_HIGH | MP_IRQ_TRIGGER_EDGE);
+	current += acpi_create_madt_irqoverride((acpi_madt_irqoverride_t *)
+		 current, 0, 9, 9, MP_IRQ_POLARITY_HIGH | MP_IRQ_TRIGGER_LEVEL);
+
+
+	return current;
+}
diff --git a/src/mainboard/lenovo/r500/board_info.txt b/src/mainboard/lenovo/r500/board_info.txt
new file mode 100644
index 0000000..a78a21b
--- /dev/null
+++ b/src/mainboard/lenovo/r500/board_info.txt
@@ -0,0 +1,6 @@
+Category: laptop
+ROM package: SOIC-16
+ROM protocol: SPI
+ROM socketed: n
+Flashrom support: n
+Release year: 2008
diff --git a/src/mainboard/lenovo/r500/cmos.default b/src/mainboard/lenovo/r500/cmos.default
new file mode 100644
index 0000000..67b8920
--- /dev/null
+++ b/src/mainboard/lenovo/r500/cmos.default
@@ -0,0 +1,16 @@
+boot_option=Fallback
+last_boot=Fallback
+baud_rate=115200
+debug_level=Spew
+power_on_after_fail=Disable
+volume=0x3
+first_battery=Primary
+bluetooth=Enable
+wwan=Enable
+wlan=Enable
+trackpoint=Enable
+fn_ctrl_swap=Disable
+sticky_fn=Disable
+power_management_beeps=Enable
+low_battery_beep=Enable
+sata_mode=AHCI
diff --git a/src/mainboard/lenovo/r500/cmos.layout b/src/mainboard/lenovo/r500/cmos.layout
new file mode 100644
index 0000000..39ced9b
--- /dev/null
+++ b/src/mainboard/lenovo/r500/cmos.layout
@@ -0,0 +1,144 @@
+#
+# This file is part of the coreboot project.
+#
+# Copyright (C) 2007-2008 coresystems GmbH
+#               2012 secunet Security Networks AG
+#
+# This program is free software; you can redistribute it and/or
+# modify it under the terms of the GNU General Public License as
+# published by the Free Software Foundation; version 2 of
+# the License.
+#
+# This program is distributed in the hope that it will be useful,
+# but WITHOUT ANY WARRANTY; without even the implied warranty of
+# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+# GNU General Public License for more details.
+#
+# You should have received a copy of the GNU General Public License
+# along with this program; if not, write to the Free Software
+# Foundation, Inc.
+#
+
+# -----------------------------------------------------------------
+entries
+
+# -----------------------------------------------------------------
+# Status Register A
+# -----------------------------------------------------------------
+# Status Register B
+# -----------------------------------------------------------------
+# Status Register C
+#96           4       r       0        status_c_rsvd
+#100          1       r       0        uf_flag
+#101          1       r       0        af_flag
+#102          1       r       0        pf_flag
+#103          1       r       0        irqf_flag
+# -----------------------------------------------------------------
+# Status Register D
+#104          7       r       0        status_d_rsvd
+#111          1       r       0        valid_cmos_ram
+# -----------------------------------------------------------------
+# Diagnostic Status Register
+#112          8       r       0        diag_rsvd1
+
+# -----------------------------------------------------------------
+0           120       r       0        reserved_memory
+#120        240       r       0        unused
+
+# -----------------------------------------------------------------
+# RTC_BOOT_BYTE (coreboot hardcoded)
+384           1       e       4        boot_option
+385           1       e       4        last_boot
+388           4       r       0        reboot_bits
+#390          2       r       0        unused?
+
+# -----------------------------------------------------------------
+# coreboot config options: console
+392           3       e       5        baud_rate
+395           4       e       6        debug_level
+#399          1       r       0        unused
+
+# coreboot config options: EC
+400         8       h       0        volume
+
+# coreboot config options: southbridge
+408         1       e       10        sata_mode
+409         2       e       7         power_on_after_fail
+
+# coreboot config options: EC
+411         1       e       9        first_battery
+412         1       e       1        bluetooth
+413         1       e       1        wwan
+414         1       e       1        wlan
+415         1       e       1        trackpoint
+416         1       e       1        fn_ctrl_swap
+417         1       e       1        sticky_fn
+
+# coreboot config options: bootloader
+418         512       s       0        boot_devices
+930           8       h       0        boot_default
+
+938         1       e       1        power_management_beeps
+939         1       e       1        low_battery_beep
+940         1       e       1        uwb
+
+# coreboot config options: northbridge
+941         3       e       11       gfx_uma_size
+
+#944          2       r       0        unused
+
+# coreboot config options: check sums
+984          16       h       0        check_sum
+#1000        24       r       0        unused
+
+# ram initialization internal data
+1024        128       r       0        read_training_results
+
+# -----------------------------------------------------------------
+
+enumerations
+
+#ID value   text
+1     0     Disable
+1     1     Enable
+2     0     Enable
+2     1     Disable
+4     0     Fallback
+4     1     Normal
+5     0     115200
+5     1     57600
+5     2     38400
+5     3     19200
+5     4     9600
+5     5     4800
+5     6     2400
+5     7     1200
+6     1     Emergency
+6     2     Alert
+6     3     Critical
+6     4     Error
+6     5     Warning
+6     6     Notice
+6     7     Info
+6     8     Debug
+6     9     Spew
+7     0     Disable
+7     1     Enable
+7     2     Keep
+8     0     No
+8     1     Yes
+9     0     Secondary
+9     1     Primary
+10    0     AHCI
+10    1     Compatible
+11    0     32M
+11    1     48M
+11    2     64M
+11    3     128M
+11    5     96M
+11    6     160M
+
+# -----------------------------------------------------------------
+checksums
+
+checksum 392 983 984
diff --git a/src/mainboard/lenovo/r500/cstates.c b/src/mainboard/lenovo/r500/cstates.c
new file mode 100644
index 0000000..1062308
--- /dev/null
+++ b/src/mainboard/lenovo/r500/cstates.c
@@ -0,0 +1,41 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2012 secunet Security Networks AG
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; version 2 of the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#include <arch/acpigen.h>
+#include <device/device.h> /* fix for i82801ix.h */
+#include <southbridge/intel/i82801ix/i82801ix.h>
+
+static acpi_cstate_t cst_entries[] = {
+	{
+		/* acpi C1 / cpu C1 */
+		1, 0x01, 1000,
+		{ ACPI_ADDRESS_SPACE_FIXED, 1, 2, { 1 }, 0, 0 }
+	},
+	{
+		/* acpi C2 / cpu C2 */
+		2, 0x01,  500,
+		{ ACPI_ADDRESS_SPACE_FIXED, 1, 2, { 1 }, 0x10, 0 }
+	},
+};
+
+int get_cst_entries(acpi_cstate_t **entries)
+{
+	*entries = cst_entries;
+	return ARRAY_SIZE(cst_entries);
+}
diff --git a/src/mainboard/lenovo/r500/devicetree.cb b/src/mainboard/lenovo/r500/devicetree.cb
new file mode 100644
index 0000000..cb4a021
--- /dev/null
+++ b/src/mainboard/lenovo/r500/devicetree.cb
@@ -0,0 +1,222 @@
+chip northbridge/intel/gm45
+	# IGD Displays
+	register "gfx.ndid" = "3"
+	register "gfx.did" = "{ 0x80000100, 0x80000240, 0x80000410, 0x80000410, 0x00000005 }"
+
+	register "gfx.use_spread_spectrum_clock" = "1"
+	register "gfx.lvds_dual_channel" = "0"
+	register "gfx.link_frequency_270_mhz" = "1"
+	register "gfx.lvds_num_lanes" = "4"
+
+	device cpu_cluster 0 on
+		chip cpu/intel/socket_BGA956
+			device lapic 0 on end
+		end
+		chip cpu/intel/model_1067x
+			# Magic APIC ID to locate this chip
+			device lapic 0xACAC off end
+
+			# Enable Super LFM
+			register "slfm" = "1"
+
+			# Enable C5, C6
+			register "c5" = "1"
+			register "c6" = "1"
+		end
+	end
+
+	device domain 0 on
+		device pci 00.0 on
+			subsystemid 0x17aa 0x20e0
+		end # host bridge
+		device pci 02.0 on # VGA
+			subsystemid 0x17aa 0x20e4
+			ioapic_irq 2 INTA 0x10
+		end
+		device pci 02.1 on
+			subsystemid 0x17aa 0x20e4
+		end # Display
+		device pci 03.0 on
+			subsystemid 0x17aa 0x20e6
+		end # ME
+		device pci 03.1 off end # ME
+		device pci 03.2 off end # ME
+		device pci 03.3 off end # ME
+		chip southbridge/intel/i82801ix
+			register "pirqa_routing" = "0x0b"
+			register "pirqb_routing" = "0x0b"
+			register "pirqc_routing" = "0x0b"
+			register "pirqd_routing" = "0x0b"
+			register "pirqe_routing" = "0x80"
+			register "pirqf_routing" = "0x80"
+			register "pirqg_routing" = "0x80"
+			register "pirqh_routing" = "0x80"
+
+			register "gpi8_routing"  = "2"
+			register "gpe0_en" = "0x01000000"
+			register "gpi1_routing"  = "2"
+
+			# Set AHCI mode, enable ports 1 and 2.
+			register "sata_port_map"		= "0x03"
+			register "sata_clock_request"		= "0"
+			register "sata_traffic_monitor"		= "0"
+
+			# Set c-state support
+			register "c4onc3_enable"		= "0"
+			register "c5_enable"			= "1"
+			register "c6_enable"			= "1"
+
+			# Set thermal throttling to 75%.
+			register "throttle_duty"		= "THTL_75_0"
+
+			# Enable PCIe ports 1,2,4 as slots (Mini * PCIe).
+			register "pcie_slot_implemented"	= "0xb"
+			# Set power limits to 10 * 10^0 watts.
+			# Maybe we should set less for Mini PCIe.
+			register "pcie_power_limits" = "{ { 10, 0 }, { 10, 0 }, { 0, 0 }, { 10, 0 }, { 0, 0 }, { 0, 0 } }"
+			register "pcie_hotplug_map" = "{ 0, 0, 0, 1, 0, 0, 0, 0 }"
+
+			chip drivers/generic/ioapic
+				register "have_isa_interrupts" = "1"
+				register "irq_on_fsb" = "1"
+				register "enable_virtual_wire" = "1"
+				register "base" = "(void *)0xfec00000"
+				device ioapic 2 on end
+			end
+
+			device pci 19.0 on end # LAN
+			device pci 1a.0 on # UHCI
+				subsystemid 0x17aa 0x20f0
+				ioapic_irq 2 INTA 0x10
+			end
+			device pci 1a.1 on # UHCI
+				subsystemid 0x17aa 0x20f0
+				ioapic_irq 2 INTB 0x11
+			end
+			device pci 1a.2 on # UHCI
+				subsystemid 0x17aa 0x20f0
+				ioapic_irq 2 INTC 0x12
+			end
+			device pci 1a.7 on # EHCI
+				subsystemid 0x17aa 0x20f1
+				ioapic_irq 2 INTC 0x12
+			end
+			device pci 1b.0 on # HD Audio
+				subsystemid 0x17aa 0x20f2
+				ioapic_irq 2 INTA 0x10
+			end
+			device pci 1c.0 on # PCIe Port #1
+				subsystemid 0x17aa 0x20f3 # WWAN
+				ioapic_irq 2 INTA 0x10
+			end
+			device pci 1c.1 on
+				subsystemid 0x17aa 0x20f3 # WLAN
+			end # PCIe Port #2
+			device pci 1c.2 on
+				subsystemid 0x17aa 0x20f3 # UWB
+			end # PCIe Port #3
+			device pci 1c.3 on
+				subsystemid 0x17aa 0x20f3 # Expresscard
+			end # PCIe Port #4
+			device pci 1c.4 off end # PCIe Port #5
+			device pci 1c.5 off end # PCIe Port #6
+			device pci 1d.0 on # UHCI
+				subsystemid 0x17aa 0x20f0
+				ioapic_irq 2 INTA 0x10
+			end
+			device pci 1d.1 on # UHCI
+				subsystemid 0x17aa 0x20f0
+				ioapic_irq 2 INTB 0x11
+			end
+			device pci 1d.2 on # UHCI
+				subsystemid 0x17aa 0x20f0
+				ioapic_irq 2 INTC 0x12
+			end
+			device pci 1d.7 on # EHCI
+				subsystemid 0x17aa 0x20f1
+				ioapic_irq 2 INTA 0x10
+			end
+			device pci 1e.0 on # PCI
+				subsystemid 0x17aa 0x20f4
+			end
+			device pci 1f.0 on # LPC bridge
+				subsystemid 0x17aa 0x20f5
+				chip ec/lenovo/pmh7
+					device pnp ff.1 on # dummy
+					end
+					register "backlight_enable" = "0x01"
+					register "dock_event_enable" = "0x01"
+				end
+
+				chip ec/lenovo/h8
+					device pnp ff.2 on # dummy
+						io 0x60 = 0x62
+						io 0x62 = 0x66
+						io 0x64 = 0x1600
+						io 0x66 = 0x1604
+					end
+
+					register "config0" = "0xa6"
+					register "config1" = "0x04"
+					register "config2" = "0xa0"
+					register "config3" = "0x01"
+
+					register "beepmask0" = "0xfe"
+					register "beepmask1" = "0x96"
+					register "has_power_management_beeps" = "1"
+					register "has_uwb" = "1"
+
+					register "event2_enable" = "0xff"
+					register "event3_enable" = "0xff"
+					register "event4_enable" = "0xf4"
+					register "event5_enable" = "0x3c"
+					register "event6_enable" = "0x80"
+					register "event7_enable" = "0x01"
+					register "event8_enable" = "0x01"
+					register "event9_enable" = "0xff"
+					register "eventa_enable" = "0xff"
+					register "eventb_enable" = "0xff"
+					register "eventc_enable" = "0xff"
+					register "eventd_enable" = "0xff"
+				end
+
+				chip superio/nsc/pc87382
+					device pnp 164e.3 on # Digitizer
+						io 0x60 = 0x200
+						irq 0x29 = 0xb0
+						irq 0x70 = 0x5
+						irq 0xf0 = 0x82
+					end
+					# IR, not connected
+					device pnp 164e.2 off end
+					# GPIO, not connected
+					device pnp 164e.7 off end
+					# DLPC, not connected
+					device pnp 164e.19 off end
+				end
+
+			end
+			device pci 1f.2 on # SATA/IDE 1
+				subsystemid 0x17aa 0x20f8
+				ioapic_irq 2 INTB 0x11
+			end
+			device pci 1f.3 on # SMBus
+				subsystemid 0x17aa 0x20f9
+				ioapic_irq 2 INTC 0x12
+			        # eeprom, 8 virtual devices, same chip
+				chip drivers/i2c/at24rf08c
+					device i2c 54 on end
+					device i2c 55 on end
+					device i2c 56 on end
+					device i2c 57 on end
+					device i2c 5c on end
+					device i2c 5d on end
+					device i2c 5e on end
+					device i2c 5f on end
+				end
+			end
+			device pci 1f.5 off end # SATA/IDE 2
+			device pci 1f.6 off end # Thermal
+		end
+	end
+end
diff --git a/src/mainboard/lenovo/r500/dock.c b/src/mainboard/lenovo/r500/dock.c
new file mode 100644
index 0000000..63d4563
--- /dev/null
+++ b/src/mainboard/lenovo/r500/dock.c
@@ -0,0 +1,64 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2011 Sven Schnelle <svens@stackframe.org>
+ * Copyright (C) 2013 Vladimir Serbinenko <phcoder@gmail.com>
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#define __SIMPLE_DEVICE__
+#include <console/console.h>
+#include <arch/io.h>
+#include <device/device.h>
+#include <device/pci.h>
+#include <delay.h>
+#include "dock.h"
+#include "southbridge/intel/i82801ix/i82801ix.h"
+#include "ec/lenovo/h8/h8.h"
+#include <ec/acpi/ec.h>
+
+#define LPC_DEV PCI_DEV(0, 0x1f, 0)
+
+void h8_mainboard_init_dock (void)
+{
+	if (dock_present()) {
+		printk(BIOS_DEBUG, "dock is connected\n");
+		dock_connect();
+	} else
+		printk(BIOS_DEBUG, "dock is not connected\n");
+}
+
+void dock_connect(void)
+{
+	u16 gpiobase = pci_read_config16(LPC_DEV, D31F0_GPIO_BASE) & 0xfffc;
+	ec_set_bit(0x02, 0);
+	outl(inl(gpiobase + 0x0c) | (1 << 28), gpiobase + 0x0c);
+}
+
+void dock_disconnect(void)
+{
+	u16 gpiobase = pci_read_config16(LPC_DEV, D31F0_GPIO_BASE) & 0xfffc;
+	ec_clr_bit(0x02, 0);
+	outl(inl(gpiobase + 0x0c) & ~(1 << 28), gpiobase + 0x0c);
+}
+
+int dock_present(void)
+{
+	u16 gpiobase = pci_read_config16(LPC_DEV, D31F0_GPIO_BASE) & 0xfffc;
+	u8 st = inb(gpiobase + 0x0c);
+
+	return ((st >> 2) & 7) != 7;
+}
diff --git a/src/mainboard/lenovo/r500/dock.h b/src/mainboard/lenovo/r500/dock.h
new file mode 100644
index 0000000..a5029e1
--- /dev/null
+++ b/src/mainboard/lenovo/r500/dock.h
@@ -0,0 +1,26 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2011 Sven Schnelle <svens@stackframe.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; version 2 of the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#ifndef THINKPAD_X200_DOCK_H
+#define THINKPAD_X200_DOCK_H
+
+extern void dock_connect(void);
+extern void dock_disconnect(void);
+extern int dock_present(void);
+#endif
diff --git a/src/mainboard/lenovo/r500/dsdt.asl b/src/mainboard/lenovo/r500/dsdt.asl
new file mode 100644
index 0000000..5545c94
--- /dev/null
+++ b/src/mainboard/lenovo/r500/dsdt.asl
@@ -0,0 +1,58 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2009 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#define THINKPAD_EC_GPE 17
+#define BRIGHTNESS_UP \_SB.PCI0.GFX0.INCB
+#define BRIGHTNESS_DOWN \_SB.PCI0.GFX0.DECB
+#define ACPI_VIDEO_DEVICE \_SB.PCI0.GFX0
+#define DISPLAY_DEVICE_2_IS_LCD_SCREEN 1
+
+DefinitionBlock(
+	"dsdt.aml",
+	"DSDT",
+	0x03,		// DSDT revision: ACPI v3.0
+	"COREv4",	// OEM id
+	"COREBOOT",	// OEM table id
+	0x20090419	// OEM revision
+)
+{
+	// Some generic macros
+	#include "acpi/platform.asl"
+
+	// global NVS and variables
+	#include <southbridge/intel/i82801ix/acpi/globalnvs.asl>
+
+	// General Purpose Events
+	#include "acpi/gpe.asl"
+
+	Scope (\_SB) {
+		Device (PCI0)
+		{
+			#include <northbridge/intel/gm45/acpi/gm45.asl>
+			#include <southbridge/intel/i82801ix/acpi/ich9.asl>
+		}
+	}
+
+	/* Chipset specific sleep states */
+	#include <southbridge/intel/i82801ix/acpi/sleepstates.asl>
+
+	/* Dock support code */
+	#include "acpi/dock.asl"
+}
diff --git a/src/mainboard/lenovo/r500/fadt.c b/src/mainboard/lenovo/r500/fadt.c
new file mode 100644
index 0000000..3833d26
--- /dev/null
+++ b/src/mainboard/lenovo/r500/fadt.c
@@ -0,0 +1,157 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2008 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#include <string.h>
+#include <device/pci.h>
+#include <arch/acpi.h>
+#include <cpu/x86/smm.h>
+
+void acpi_create_fadt(acpi_fadt_t * fadt, acpi_facs_t * facs, void *dsdt)
+{
+	acpi_header_t *header = &(fadt->header);
+	u16 pmbase = pci_read_config16(dev_find_slot(0, PCI_DEVFN(0x1f,0)), 0x40) & 0xfffe;
+
+	memset((void *) fadt, 0, sizeof(acpi_fadt_t));
+	memcpy(header->signature, "FACP", 4);
+	header->length = sizeof(acpi_fadt_t);
+	header->revision = 3;
+	memcpy(header->oem_id, OEM_ID, 6);
+	memcpy(header->oem_table_id, ACPI_TABLE_CREATOR, 8);
+	memcpy(header->asl_compiler_id, ASLC, 4);
+	header->asl_compiler_revision = 0;
+
+	fadt->firmware_ctrl = (unsigned long) facs;
+	fadt->dsdt = (unsigned long) dsdt;
+	fadt->model = 0x00;
+	fadt->preferred_pm_profile = PM_MOBILE;
+	fadt->sci_int = 0x9;
+	fadt->smi_cmd = APM_CNT;
+	fadt->acpi_enable = APM_CNT_ACPI_ENABLE;
+	fadt->acpi_disable = APM_CNT_ACPI_DISABLE;
+	fadt->s4bios_req = 0x0;
+	fadt->pstate_cnt = APM_CNT_PST_CONTROL;
+
+	fadt->pm1a_evt_blk = pmbase;
+	fadt->pm1b_evt_blk = 0x0;
+	fadt->pm1a_cnt_blk = pmbase + 0x4;
+	fadt->pm1b_cnt_blk = 0x0;
+	fadt->pm2_cnt_blk = pmbase + 0x50;
+	fadt->pm_tmr_blk = pmbase + 0x8;
+	fadt->gpe0_blk = pmbase + 0x20;
+	fadt->gpe1_blk = 0;
+
+	fadt->pm1_evt_len = 4;
+	fadt->pm1_cnt_len = 2; /* Upper word is reserved and
+				  Linux complains about 32 bit. */
+	fadt->pm2_cnt_len = 1;
+	fadt->pm_tmr_len = 4;
+	fadt->gpe0_blk_len = 16;
+	fadt->gpe1_blk_len = 0;
+	fadt->gpe1_base = 0;
+	fadt->cst_cnt = APM_CNT_CST_CONTROL;
+	fadt->p_lvl2_lat = 1;
+	fadt->p_lvl3_lat = 0x39;
+	fadt->flush_size = 0;
+	fadt->flush_stride = 0;
+	fadt->duty_offset = 1;
+	fadt->duty_width = 3;
+	fadt->day_alrm = 0xd;
+	fadt->mon_alrm = 0x00;
+	fadt->century = 0x32;
+	fadt->iapc_boot_arch = 0x00;
+	fadt->flags = ACPI_FADT_WBINVD | ACPI_FADT_C1_SUPPORTED |
+			ACPI_FADT_SLEEP_BUTTON | ACPI_FADT_S4_RTC_WAKE |
+			ACPI_FADT_DOCKING_SUPPORTED | ACPI_FADT_RESET_REGISTER |
+			ACPI_FADT_PLATFORM_CLOCK;
+
+	fadt->reset_reg.space_id = ACPI_ADDRESS_SPACE_IO;
+	fadt->reset_reg.bit_width = 8;
+	fadt->reset_reg.bit_offset = 0;
+	fadt->reset_reg.resv = 0;
+	fadt->reset_reg.addrl = 0xcf9;
+	fadt->reset_reg.addrh = 0;
+	fadt->reset_value = 0x06;
+
+	fadt->x_firmware_ctl_l = 0; /* Set X_FIRMWARE_CTRL only if FACS is */
+	fadt->x_firmware_ctl_h = 0; /* above 4GB. If X_FIRMWARE_CTRL is set, */
+				    /* then FIRMWARE_CTRL must be zero. */
+	fadt->x_dsdt_l = (unsigned long)dsdt;
+	fadt->x_dsdt_h = 0;
+
+	fadt->x_pm1a_evt_blk.space_id = 1;
+	fadt->x_pm1a_evt_blk.bit_width = 32;
+	fadt->x_pm1a_evt_blk.bit_offset = 0;
+	fadt->x_pm1a_evt_blk.resv = 0;
+	fadt->x_pm1a_evt_blk.addrl = pmbase;
+	fadt->x_pm1a_evt_blk.addrh = 0x0;
+
+	fadt->x_pm1b_evt_blk.space_id = 0;
+	fadt->x_pm1b_evt_blk.bit_width = 0;
+	fadt->x_pm1b_evt_blk.bit_offset = 0;
+	fadt->x_pm1b_evt_blk.resv = 0;
+	fadt->x_pm1b_evt_blk.addrl = 0x0;
+	fadt->x_pm1b_evt_blk.addrh = 0x0;
+
+	fadt->x_pm1a_cnt_blk.space_id = 1;
+	fadt->x_pm1a_cnt_blk.bit_width = 16; /* Upper word is reserved and
+						Linux complains about 32 bit. */
+	fadt->x_pm1a_cnt_blk.bit_offset = 0;
+	fadt->x_pm1a_cnt_blk.resv = 0;
+	fadt->x_pm1a_cnt_blk.addrl = pmbase + 0x4;
+	fadt->x_pm1a_cnt_blk.addrh = 0x0;
+
+	fadt->x_pm1b_cnt_blk.space_id = 0;
+	fadt->x_pm1b_cnt_blk.bit_width = 0;
+	fadt->x_pm1b_cnt_blk.bit_offset = 0;
+	fadt->x_pm1b_cnt_blk.resv = 0;
+	fadt->x_pm1b_cnt_blk.addrl = 0x0;
+	fadt->x_pm1b_cnt_blk.addrh = 0x0;
+
+	fadt->x_pm2_cnt_blk.space_id = 1;
+	fadt->x_pm2_cnt_blk.bit_width = 8;
+	fadt->x_pm2_cnt_blk.bit_offset = 0;
+	fadt->x_pm2_cnt_blk.resv = 0;
+	fadt->x_pm2_cnt_blk.addrl = pmbase + 0x50;
+	fadt->x_pm2_cnt_blk.addrh = 0x0;
+
+	fadt->x_pm_tmr_blk.space_id = 1;
+	fadt->x_pm_tmr_blk.bit_width = 32;
+	fadt->x_pm_tmr_blk.bit_offset = 0;
+	fadt->x_pm_tmr_blk.resv = 0;
+	fadt->x_pm_tmr_blk.addrl = pmbase + 0x8;
+	fadt->x_pm_tmr_blk.addrh = 0x0;
+
+	fadt->x_gpe0_blk.space_id = 1;
+	fadt->x_gpe0_blk.bit_width = 128;
+	fadt->x_gpe0_blk.bit_offset = 0;
+	fadt->x_gpe0_blk.resv = 0;
+	fadt->x_gpe0_blk.addrl = pmbase + 0x20;
+	fadt->x_gpe0_blk.addrh = 0x0;
+
+	fadt->x_gpe1_blk.space_id = 0;
+	fadt->x_gpe1_blk.bit_width = 0;
+	fadt->x_gpe1_blk.bit_offset = 0;
+	fadt->x_gpe1_blk.resv = 0;
+	fadt->x_gpe1_blk.addrl = 0x0;
+	fadt->x_gpe1_blk.addrh = 0x0;
+
+	header->checksum =
+	    acpi_checksum((void *) fadt, header->length);
+}
diff --git a/src/mainboard/lenovo/r500/hda_verb.c b/src/mainboard/lenovo/r500/hda_verb.c
new file mode 100644
index 0000000..beb637f
--- /dev/null
+++ b/src/mainboard/lenovo/r500/hda_verb.c
@@ -0,0 +1,51 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2007-2009 coresystems GmbH
+ *               2012 secunet Security Networks AG
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#include <device/azalia_device.h>
+
+const u32 cim_verb_data[] = {
+	/* coreboot specific header */
+	0x14f15051,	// Conexant CX20561 (Hermosa)
+	0x17aa20ff,	// Subsystem ID
+	0x00000008,	// Number of entries
+
+	/* Pin Widget Verb Table */
+
+	AZALIA_PIN_CFG(0, 0x16, 0x042140f0),
+	AZALIA_PIN_CFG(0, 0x17, 0x61a190f0),
+	AZALIA_PIN_CFG(0, 0x18, 0x04a190f0),
+	AZALIA_PIN_CFG(0, 0x19, 0x612140f0),
+	AZALIA_PIN_CFG(0, 0x1a, 0x901701f0),
+	AZALIA_PIN_CFG(0, 0x1b, 0x40f001f0),
+	AZALIA_PIN_CFG(0, 0x1c, 0x40f001f0),
+	AZALIA_PIN_CFG(0, 0x1d, 0x90a601f0)
+};
+
+const u32 pc_beep_verbs[] = {
+	0x00170500,	/* power up codec */
+	0x01470500,	/* power up speakers */
+	0x01470100,	/* select lout1 (input 0x0) for speakers */
+	0x01470740,	/* enable speakers output */
+	0x00b37517,	/* unmute beep (mixer's input 0x5), set amp 0dB */
+	0x00c37100,	/* unmute mixer in lout1 (lout1 input 0x1) */
+	0x00c3b015,	/* set lout1 output volume -15dB */
+	0x0143b000,	/* unmute speakers */
+};
+AZALIA_ARRAY_SIZES;
diff --git a/src/mainboard/lenovo/r500/mainboard.c b/src/mainboard/lenovo/r500/mainboard.c
new file mode 100644
index 0000000..d91e225
--- /dev/null
+++ b/src/mainboard/lenovo/r500/mainboard.c
@@ -0,0 +1,49 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2012 secunet Security Networks AG
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; version 2 of the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#include <stdint.h>
+#include <stdlib.h>
+#include <arch/io.h>
+#include <device/device.h>
+#include <console/console.h>
+#include <drivers/intel/gma/int15.h>
+#include <pc80/keyboard.h>
+#include <ec/acpi/ec.h>
+#include <smbios.h>
+#include <string.h>
+#include <ec/lenovo/pmh7/pmh7.h>
+#include <ec/acpi/ec.h>
+#include <ec/lenovo/h8/h8.h>
+#include "drivers/lenovo/lenovo.h"
+
+static void fill_ssdt(device_t device)
+{
+	drivers_lenovo_serial_ports_ssdt_generate("\\_SB.PCI0.LPCB", 0);
+}
+
+static void mainboard_enable(device_t dev)
+{
+	install_intel_vga_int15_handler(GMA_INT15_ACTIVE_LFP_INT_LVDS, GMA_INT15_PANEL_FIT_CENTERING, GMA_INT15_BOOT_DISPLAY_DEFAULT, 2);
+
+	dev->ops->acpi_fill_ssdt_generator = fill_ssdt;
+}
+
+struct chip_operations mainboard_ops = {
+	.enable_dev = mainboard_enable,
+};
diff --git a/src/mainboard/lenovo/r500/mptable.c b/src/mainboard/lenovo/r500/mptable.c
new file mode 100644
index 0000000..f1839f0
--- /dev/null
+++ b/src/mainboard/lenovo/r500/mptable.c
@@ -0,0 +1 @@
+/* dummy file */
diff --git a/src/mainboard/lenovo/r500/romstage.c b/src/mainboard/lenovo/r500/romstage.c
new file mode 100644
index 0000000..455dd35
--- /dev/null
+++ b/src/mainboard/lenovo/r500/romstage.c
@@ -0,0 +1,203 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2012 secunet Security Networks AG
+ *
+ * This program is free software; you can redistribute it and/or
+ * modify it under the terms of the GNU General Public License as
+ * published by the Free Software Foundation; version 2 of
+ * the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+// __PRE_RAM__ means: use "unsigned" for device, not a struct.
+
+#include <stdint.h>
+#include <string.h>
+#include <arch/io.h>
+#include <cpu/x86/lapic.h>
+#include <cpu/x86/msr.h>
+#include <cpu/x86/tsc.h>
+#include <cbmem.h>
+#include <lib.h>
+#include <pc80/mc146818rtc.h>
+#include <console/console.h>
+#include <southbridge/intel/i82801ix/i82801ix.h>
+#include <northbridge/intel/gm45/gm45.h>
+#include <cpu/intel/romstage.h>
+
+#define LPC_DEV PCI_DEV(0, 0x1f, 0)
+#define MCH_DEV PCI_DEV(0, 0, 0)
+
+static void default_southbridge_gpio_setup(void)
+{
+	outl(0x197e23fe, DEFAULT_GPIOBASE + GP_IO_USE_SEL);
+	outl(0xe1a66dfe, DEFAULT_GPIOBASE + GP_IO_SEL);
+	outl(0xe3faef3f, DEFAULT_GPIOBASE + GP_LVL);
+
+	/* Disable blink [31:0]. */
+	outl(0x00000000, DEFAULT_GPIOBASE + GPO_BLINK);
+	/* Set input inversion [31:0]. */
+	outl(0x00000102, DEFAULT_GPIOBASE + GPI_INV);
+
+	/* Enable GPIOs [60:32]. */
+	outl(0x030306f6, DEFAULT_GPIOBASE + GP_IO_USE_SEL2);
+	/* Set input/output mode [60:32] (0 == out, 1 == in). */
+	outl(0x1f55f9f1, DEFAULT_GPIOBASE + GP_IO_SEL2);
+	/* Set gpio levels [60:32].  */
+	outl(0x1dffff53, DEFAULT_GPIOBASE + GP_LVL2);
+}
+
+static void early_lpc_setup(void)
+{
+	/* Set up SuperIO LPC forwards */
+
+	/* Configure serial IRQs.*/
+	pci_write_config8(LPC_DEV, D31F0_SERIRQ_CNTL, 0xd0);
+	/* Map COMa on 0x3f8, COMb on 0x2f8. */
+	pci_write_config16(LPC_DEV, D31F0_LPC_IODEC, 0x0010);
+	pci_write_config16(LPC_DEV, D31F0_LPC_EN, 0x3f0f);
+	pci_write_config32(LPC_DEV, D31F0_GEN1_DEC, 0x7c1601);
+	pci_write_config32(LPC_DEV, D31F0_GEN2_DEC, 0xc15e1);
+	pci_write_config32(LPC_DEV, D31F0_GEN3_DEC, 0x1c1681);
+}
+
+void main(unsigned long bist)
+{
+	sysinfo_t sysinfo;
+	int s3resume = 0;
+	int cbmem_initted;
+	u16 reg16;
+
+	/* basic northbridge setup, including MMCONF BAR */
+	gm45_early_init();
+
+	if (bist == 0)
+		enable_lapic();
+
+	/* First, run everything needed for console output. */
+	i82801ix_early_init();
+	early_lpc_setup();
+	console_init();
+	printk(BIOS_DEBUG, "running main(bist = %lu)\n", bist);
+
+	reg16 = pci_read_config16(LPC_DEV, D31F0_GEN_PMCON_3);
+	pci_write_config16(LPC_DEV, D31F0_GEN_PMCON_3, reg16);
+	if ((MCHBAR16(SSKPD_MCHBAR) == 0xCAFE) && !(reg16 & (1 << 9))) {
+		printk(BIOS_DEBUG, "soft reset detected, rebooting properly\n");
+		gm45_early_reset();
+	}
+
+	default_southbridge_gpio_setup();
+
+	/* ASPM related setting, set early by original BIOS. */
+	DMIBAR16(0x204) &= ~(3 << 10);
+
+	/* Check for S3 resume. */
+	const u32 pm1_cnt = inl(DEFAULT_PMBASE + 0x04);
+	if (((pm1_cnt >> 10) & 7) == 5) {
+#if CONFIG_HAVE_ACPI_RESUME
+		printk(BIOS_DEBUG, "Resume from S3 detected.\n");
+		s3resume = 1;
+		/* Clear SLP_TYPE. This will break stage2 but
+		 * we care for that when we get there.
+		 */
+		outl(pm1_cnt & ~(7 << 10), DEFAULT_PMBASE + 0x04);
+#else
+		printk(BIOS_DEBUG, "Resume from S3 detected, but disabled.\n");
+#endif
+	}
+
+	/* RAM initialization */
+	enter_raminit_or_reset();
+	memset(&sysinfo, 0, sizeof(sysinfo));
+	sysinfo.spd_map[0] = 0x50;
+	sysinfo.spd_map[2] = 0x51;
+	sysinfo.enable_igd = 1;
+	sysinfo.enable_peg = 0;
+	get_gmch_info(&sysinfo);
+	raminit(&sysinfo, s3resume);
+
+	const u32 deven = pci_read_config32(MCH_DEV, D0F0_DEVEN);
+	/* Disable D4F0 (unknown signal controller). */
+	pci_write_config32(MCH_DEV, D0F0_DEVEN, deven & ~0x4000);
+
+	init_pm(&sysinfo, 0);
+
+	i82801ix_dmi_setup();
+	gm45_late_init(sysinfo.stepping);
+	i82801ix_dmi_poll_vc1();
+
+	MCHBAR16(SSKPD_MCHBAR) = 0xCAFE;
+	/* Enable ethernet.  */
+	RCBA32(0x3414) &= ~0x20;
+
+	RCBA32(0x0238) = 0x00543210;
+	RCBA32(0x0240) = 0x009c0b02;
+	RCBA32(0x0244) = 0x00a20b1a;
+	RCBA32(0x0248) = 0x005402cb;
+	RCBA32(0x0254) = 0x00470966;
+	RCBA32(0x0258) = 0x00470473;
+	RCBA32(0x0260) = 0x00e90825;
+	RCBA32(0x0278) = 0x00bc0efb;
+	RCBA32(0x027c) = 0x00c00f0b;
+	RCBA32(0x0280) = 0x00670000;
+	RCBA32(0x0284) = 0x006d0000;
+	RCBA32(0x0288) = 0x00600b4e;
+	RCBA32(0x1e10) = 0x00020800;
+	RCBA32(0x1e18) = 0x36ea00a0;
+	RCBA32(0x1e80) = 0x000c0801;
+	RCBA32(0x1e84) = 0x000200f0;
+	RCBA32(0x2028) = 0x04c8f95e;
+	RCBA32(0x202c) = 0x055c095e;
+	RCBA32(0x204c) = 0x001ffc00;
+	RCBA32(0x2050) = 0x00100fff;
+	RCBA32(0x2090) = 0x37000000;
+	RCBA32(0x20b0) = 0x0c000000;
+	RCBA32(0x20d0) = 0x09000000;
+	RCBA32(0x20f0) = 0x05000000;
+	RCBA32(0x3400) = 0x0000001c;
+	RCBA32(0x3410) = 0x00100461;
+	RCBA32(0x3414) = 0x00000000;
+	RCBA32(0x341c) = 0xbf4f001f;
+	RCBA32(0x3420) = 0x00000000;
+	RCBA32(0x3430) = 0x00000001;
+
+	init_iommu();
+
+	/* FIXME: make a proper SMBUS mux support.  */
+	outl(inl(DEFAULT_GPIOBASE + 0x38) & ~0x400, DEFAULT_GPIOBASE + 0x38);
+
+	cbmem_initted = !cbmem_recovery(s3resume);
+#if CONFIG_HAVE_ACPI_RESUME
+	/* If there is no high memory area, we didn't boot before, so
+	 * this is not a resume. In that case we just create the cbmem toc.
+	 */
+	if (s3resume && cbmem_initted) {
+		void *resume_backup_memory = cbmem_find(CBMEM_ID_RESUME);
+
+		/* copy 1MB - 64K to high tables ram_base to prevent memory corruption
+		 * through stage 2. We could keep stuff like stack and heap in high tables
+		 * memory completely, but that's a wonderful clean up task for another
+		 * day.
+		 */
+		if (resume_backup_memory)
+			memcpy(resume_backup_memory, (void *)CONFIG_RAMBASE, HIGH_MEMORY_SAVE);
+
+		/* Magic for S3 resume */
+		pci_write_config32(PCI_DEV(0, 0, 0), D0F0_SKPD, SKPAD_ACPI_S3_MAGIC);
+	} else {
+		/* Magic for S3 resume */
+		pci_write_config32(PCI_DEV(0, 0, 0), D0F0_SKPD, SKPAD_NORMAL_BOOT_MAGIC);
+	}
+#endif
+	printk(BIOS_SPEW, "exit main()\n");
+}
diff --git a/src/mainboard/lenovo/r500/smihandler.c b/src/mainboard/lenovo/r500/smihandler.c
new file mode 100644
index 0000000..622b31a
--- /dev/null
+++ b/src/mainboard/lenovo/r500/smihandler.c
@@ -0,0 +1,49 @@
+/*
+ * This file is part of the coreboot project.
+ *
+ * Copyright (C) 2008-2009 coresystems GmbH
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; version 2 of the License.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc.
+ */
+
+#include <arch/io.h>
+#include <console/console.h>
+#include <cpu/x86/smm.h>
+#include <southbridge/intel/i82801ix/nvs.h>
+#include <southbridge/intel/i82801ix/i82801ix.h>
+#include <ec/acpi/ec.h>
+
+void mainboard_smi_gpi(u32 gpi_sts)
+{
+	if (gpi_sts & (1 << 1)) {
+		printk(BIOS_DEBUG, "EC/SMI\n");
+		/* TODO */
+	}
+}
+
+int mainboard_smi_apmc(u8 apmc)
+{
+	switch (apmc) {
+	case APM_CNT_ACPI_ENABLE:
+		send_ec_command(0x05); /* Set_SMI_Disable */
+		send_ec_command(0xaa); /* Set_ACPI_Enable */
+		break;
+
+	case APM_CNT_ACPI_DISABLE:
+		send_ec_command(0x04); /* Set_SMI_Enable */
+		send_ec_command(0xab); /* Set_ACPI_Disable */
+		break;
+	}
+	return 0;
+}
-- 
1.9.1

