From 51e23836f586c79d63ca402bad738bd7a4149572 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Sat, 5 Sep 2015 18:46:54 -0500
Subject: [PATCH 016/143] cpu/amd/model_10xxx: Clean up debugging statements

Change-Id: I6dff74b3857e1fb384aefc87b44e7679bd4aab07
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/cpu/amd/model_10xxx/fidvid.c |   42 ++++++++++++++++++--------------------
 1 file changed, 20 insertions(+), 22 deletions(-)

diff --git a/src/cpu/amd/model_10xxx/fidvid.c b/src/cpu/amd/model_10xxx/fidvid.c
index 36bdf36..5b1c581 100644
--- a/src/cpu/amd/model_10xxx/fidvid.c
+++ b/src/cpu/amd/model_10xxx/fidvid.c
@@ -460,35 +460,35 @@ static void config_clk_power_ctrl_reg0(int node, u32 cpuRev, u8 procPkg) {
 
 static void config_power_ctrl_misc_reg(device_t dev,u32 cpuRev, u8 procPkg) {
 	/* check PVI/SVI */
-	u32 dword = pci_read_config32(dev, 0xA0);
+	u32 dword = pci_read_config32(dev, 0xa0);
 
-        /* BKDG r31116 2010-04-22  2.4.1.7 step b F3xA0[VSSlamVidMod] */
-        /* PllLockTime and PsiVidEn set in ruleset in defaults.h */
+	/* BKDG r31116 2010-04-22  2.4.1.7 step b F3xA0[VSSlamVidMod] */
+	/* PllLockTime and PsiVidEn set in ruleset in defaults.h */
 	if (dword & PVI_MODE) {	/* PVI */
 		/* set slamVidMode to 0 for PVI */
 		dword &= VID_SLAM_OFF ;
 	} else {	/* SVI */
 		/* set slamVidMode to 1 for SVI */
 		dword |= VID_SLAM_ON;
-        }
+	}
         /* set the rest of A0 since we're at it... */
 
-        if (cpuRev & (AMD_DA_Cx | AMD_RB_C3 )) {
-	     dword |= NB_PSTATE_FORCE_ON;
+	if (cpuRev & (AMD_DA_Cx | AMD_RB_C3 )) {
+		dword |= NB_PSTATE_FORCE_ON;
 	} // else should we clear it ?
 
 
         if ((procPkg == AMD_PKGTYPE_G34) || (procPkg == AMD_PKGTYPE_C32) ) {
-	  dword |= BP_INS_TRI_EN_ON ;
+		dword |= BP_INS_TRI_EN_ON ;
 	}
 
 	   /* TODO: look into C1E state and F3xA0[IdleExitEn]*/
         #if CONFIG_SVI_HIGH_FREQ
-	   if (cpuRev & AMD_FAM10_C3) {
-	     dword |= SVI_HIGH_FREQ_ON;
-           }
-        #endif
-	pci_write_config32(dev, 0xA0, dword);
+	if (cpuRev & AMD_FAM10_C3) {
+		dword |= SVI_HIGH_FREQ_ON;
+	}
+	#endif
+	pci_write_config32(dev, 0xa0, dword);
 }
 
 static void config_nb_syn_ptr_adj(device_t dev, u32 cpuRev) {
@@ -581,7 +581,7 @@ static void prep_fid_change(void)
 	nodes = get_nodes();
 
 	for (i = 0; i < nodes; i++) {
-		printk(BIOS_DEBUG, "Prep FID/VID Node:%02x \n", i);
+		printk(BIOS_DEBUG, "Prep FID/VID Node:%02x\n", i);
 		dev = NODE_PCI(i, 3);
                 u32 cpuRev = mctGetLogicalCPUID(0xFF) ;
 	        u8 procPkg =  mctGetProcessorPackageType();
@@ -591,25 +591,23 @@ static void prep_fid_change(void)
 		/* Figure out the value for VsSlamTime and program it */
 		recalculateVsSlamTimeSettingOnCorePre(dev);
 
-                config_clk_power_ctrl_reg0(i,cpuRev,procPkg);
+		config_clk_power_ctrl_reg0(i,cpuRev,procPkg);
 
                 config_power_ctrl_misc_reg(dev,cpuRev,procPkg);
 		config_nb_syn_ptr_adj(dev,cpuRev);
 
-                config_acpi_pwr_state_ctrl_regs(dev,cpuRev,procPkg);
+		config_acpi_pwr_state_ctrl_regs(dev,cpuRev,procPkg);
 
 		dword = pci_read_config32(dev, 0x80);
-		printk(BIOS_DEBUG, "  F3x80: %08x \n", dword);
+		printk(BIOS_DEBUG, "  F3x80: %08x\n", dword);
 		dword = pci_read_config32(dev, 0x84);
-		printk(BIOS_DEBUG, "  F3x84: %08x \n", dword);
+		printk(BIOS_DEBUG, "  F3x84: %08x\n", dword);
 		dword = pci_read_config32(dev, 0xD4);
-		printk(BIOS_DEBUG, "  F3xD4: %08x \n", dword);
+		printk(BIOS_DEBUG, "  F3xD4: %08x\n", dword);
 		dword = pci_read_config32(dev, 0xD8);
-		printk(BIOS_DEBUG, "  F3xD8: %08x \n", dword);
+		printk(BIOS_DEBUG, "  F3xD8: %08x\n", dword);
 		dword = pci_read_config32(dev, 0xDC);
-		printk(BIOS_DEBUG, "  F3xDC: %08x \n", dword);
-
-
+		printk(BIOS_DEBUG, "  F3xDC: %08x\n", dword);
 	}
 }
 
-- 
1.7.9.5

