From 8249f770fd166cc1ce8d6c033c01103d36763977 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Wed, 21 Oct 2015 15:27:02 -0500
Subject: [PATCH 019/143] mainboard/asrock/e350m1: Update CMOS layout to match
 SIO changes

Change-Id: I3f1f33b50f788b6d57f1a7986c4bdb912426e4f0
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/mainboard/asrock/e350m1/cmos.layout |    5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

diff --git a/src/mainboard/asrock/e350m1/cmos.layout b/src/mainboard/asrock/e350m1/cmos.layout
index 996160e..bc8de75 100644
--- a/src/mainboard/asrock/e350m1/cmos.layout
+++ b/src/mainboard/asrock/e350m1/cmos.layout
@@ -29,7 +29,7 @@ entries
 396          1       e       1        interleave_chip_selects
 397          2       e       8        max_mem_clock
 399          1       e       2        multi_core
-400          1       e       1        power_on_after_fail
+400          2       e       3        power_on_after_fail
 412          4       e       6        debug_level
 440          4       e       9        slow_cpu
 444          1       e       1        nmi
@@ -49,6 +49,9 @@ enumerations
 1     1     Enable
 2     0     Enable
 2     1     Disable
+3     0     Off
+3     1     On
+3     2     Last
 4     0     Fallback
 4     1     Normal
 5     0     115200
-- 
1.7.9.5

