From 9eb389b0273cf07add859cd162c1411d15806149 Mon Sep 17 00:00:00 2001
From: Paul Kocialkowski <contact@paulk.fr>
Date: Mon, 10 Aug 2015 20:30:14 +0200
Subject: [PATCH 6/7] fdt: nonvolatile-context-storage report to mkbp for EC NV
 storage

This allows old versions of crossystem to detect that it should use mosys to
access NV storage in case it is stored on the EC.

Signed-off-by: Paul Kocialkowski <contact@paulk.fr>
---
 src/vboot/crossystem/fdt.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/vboot/crossystem/fdt.c b/src/vboot/crossystem/fdt.c
index a79b192..0487513 100644
--- a/src/vboot/crossystem/fdt.c
+++ b/src/vboot/crossystem/fdt.c
@@ -56,7 +56,7 @@ static int install_crossystem_data(DeviceTreeFixup *fixup, DeviceTree *tree)
 		dt_add_string_prop(node, "nonvolatile-context-storage","nvram");
 	} else if (CONFIG_NV_STORAGE_CROS_EC) {
 		dt_add_string_prop(node,
-				"nonvolatile-context-storage", "cros-ec");
+				"nonvolatile-context-storage", "mkbp");
 	} else if (CONFIG_NV_STORAGE_DISK) {
 		dt_add_string_prop(node, "nonvolatile-context-storage", "disk");
 		dt_add_u32_prop(node, "nonvolatile-context-lba",
-- 
1.9.1

