From 3cc65b99ac7b00ba5960c5c40a984bebafcf379a Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Tue, 2 Jun 2015 13:25:23 -0500
Subject: [PATCH 039/143] cpu/amd/car: Increase Family 10h CAR size limit to
 128k

This resolves issues with 4-node (32-core) systems not having
sufficient CAR memory to boot.

Change-Id: I5378df7fe8c034ba30f7fdf454f81dd10a0c2ae4
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/cpu/amd/car/post_cache_as_ram.c |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/cpu/amd/car/post_cache_as_ram.c b/src/cpu/amd/car/post_cache_as_ram.c
index 787bedd..2282cee 100644
--- a/src/cpu/amd/car/post_cache_as_ram.c
+++ b/src/cpu/amd/car/post_cache_as_ram.c
@@ -114,7 +114,7 @@ void post_cache_as_ram(void)
 	 * boundary during romstage execution
 	 */
 	volatile uint32_t *lower_stack_boundary;
-	lower_stack_boundary = (void *)((CONFIG_DCACHE_RAM_BASE + CONFIG_DCACHE_RAM_SIZE) - CONFIG_STACK_SIZE);
+	lower_stack_boundary = (void *)((CONFIG_DCACHE_RAM_BASE + CONFIG_DCACHE_RAM_SIZE) - CONFIG_DCACHE_BSP_STACK_SIZE);
 	if ((*lower_stack_boundary) != 0xdeadbeef)
 		printk(BIOS_WARNING, "BSP overran lower stack boundary.  Undefined behaviour may result!\n");
 
-- 
1.7.9.5

