From 4dfbaf7e6fd49d46c58f8f5e58d0ce4e7e97fa04 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Tue, 2 Jun 2015 20:18:44 -0500
Subject: [PATCH 040/143] cpu/amd/car: Move AP stacks below the BSP stack to
 free up space

Caching SPD data during startup requires additional CAR space.
There was a large chunk of free space between the AP stack top and
the BSP stack bottom; moving the AP stacks below the BSP stack
allows this space to be utilized.

Change-Id: I51af31442f2b77cb64a4b788751ccc7186acb283
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/cpu/amd/family_10h-family_15h/Kconfig |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/cpu/amd/family_10h-family_15h/Kconfig b/src/cpu/amd/family_10h-family_15h/Kconfig
index 7c47e27..81b1d1e 100644
--- a/src/cpu/amd/family_10h-family_15h/Kconfig
+++ b/src/cpu/amd/family_10h-family_15h/Kconfig
@@ -33,7 +33,7 @@ config DCACHE_RAM_SIZE
 
 config DCACHE_BSP_STACK_SIZE
 	hex
-	default 0x2000
+	default 0x4000
 
 config DCACHE_BSP_STACK_SLUSH
 	hex
-- 
1.7.9.5

