From 77935659fbe9426e7a65ecc5506beb4491171e7f Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Fri, 26 Jun 2015 17:49:25 -0500
Subject: [PATCH 079/143] northbridge/amd/amdmct/mct_ddr3: Set SkewMemClk when
 both DCTs are in use

Change-Id: Ibcce54fc53b79beba2f790994bcf87cc0354213a
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/northbridge/amd/amdmct/mct_ddr3/mct_d.c |   41 +++++++++++++++++++++------
 src/northbridge/amd/amdmct/mct_ddr3/mct_d.h |    2 +-
 2 files changed, 34 insertions(+), 9 deletions(-)

diff --git a/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c b/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c
index bb5593d..f3d5cb8 100644
--- a/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c
+++ b/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c
@@ -2645,7 +2645,7 @@ static void DCTPreInit_D(struct MCTStatStruc *pMCTstat, struct DCTStatStruc *pDC
 
 	/* Reset DCT registers */
 	ClearDCT_D(pMCTstat, pDCTstat, dct);
-	pDCTstat->stopDCT = 1;		/*preload flag with 'disable' */
+	pDCTstat->stopDCT[dct] = 1;	/* preload flag with 'disable' */
 
 	if (!is_fam15h()) {
 		/* Enable DDR3 support */
@@ -2656,7 +2656,7 @@ static void DCTPreInit_D(struct MCTStatStruc *pMCTstat, struct DCTStatStruc *pDC
 
 	/* Read the SPD information into the data structures */
 	if (mct_DIMMPresence(pMCTstat, pDCTstat, dct) < SC_StopError) {
-		printk(BIOS_DEBUG, "\t\tDCTInit_D: mct_DIMMPresence Done\n");
+		printk(BIOS_DEBUG, "\t\tDCTPreInit_D: mct_DIMMPresence Done\n");
 	}
 }
 
@@ -2682,17 +2682,40 @@ static void DCTInit_D(struct MCTStatStruc *pMCTstat, struct DCTStatStruc *pDCTst
 				printk(BIOS_DEBUG, "\t\tDCTInit_D: AutoConfig_D Done\n");
 				if (PlatformSpec_D(pMCTstat, pDCTstat, dct) < SC_StopError) {
 					printk(BIOS_DEBUG, "\t\tDCTInit_D: PlatformSpec_D Done\n");
-					pDCTstat->stopDCT = 0;
-					if (!(pMCTstat->GStatus & (1 << GSB_EnDIMMSpareNW))) {
-						printk(BIOS_DEBUG, "\t\tDCTInit_D: StartupDCT_D\n");
-						StartupDCT_D(pMCTstat, pDCTstat, dct);   /*yeaahhh! */
-					}
+					pDCTstat->stopDCT[dct] = 0;
 				}
 			}
 		}
 	}
 
-	if (pDCTstat->stopDCT) {
+
+}
+
+static void DCTFinalInit_D(struct MCTStatStruc *pMCTstat, struct DCTStatStruc *pDCTstat, u8 dct)
+{
+	uint32_t dword;
+
+	/* Finalize DRAM init on a single node */
+	if (is_fam15h()) {
+		/* Set memory clock skew if needed */
+		if (dct == 0) {
+			if (!pDCTstat->stopDCT[0] && !pDCTstat->stopDCT[1]) {
+				dword = Get_NB32_index_wait_DCT(pDCTstat->dev_dct, dct, 0x98, 0x0d0fe00a);
+				dword |= (0x1 << 4);				/* SkewMemClk = 1 */
+				Set_NB32_index_wait_DCT(pDCTstat->dev_dct, dct, 0x98, 0x0d0fe00a, dword);
+			}
+		}
+	}
+
+	if (!pDCTstat->stopDCT[dct]) {
+		if (!(pMCTstat->GStatus & (1 << GSB_EnDIMMSpareNW))) {
+			printk(BIOS_DEBUG, "\t\tDCTFinalInit_D: StartupDCT_D Start\n");
+			StartupDCT_D(pMCTstat, pDCTstat, dct);
+			printk(BIOS_DEBUG, "\t\tDCTFinalInit_D: StartupDCT_D Done\n");
+		}
+	}
+
+	if (pDCTstat->stopDCT[dct]) {
 		dword = 1 << DisDramInterface;
 		Set_NB32_DCT(pDCTstat->dev_dct, dct, 0x94, dword);
 
@@ -4350,6 +4373,7 @@ static void mct_initDCT(struct MCTStatStruc *pMCTstat,
 
 	/* Config. DCT0 for Ganged or unganged mode */
 	DCTInit_D(pMCTstat, pDCTstat, 0);
+	DCTFinalInit_D(pMCTstat, pDCTstat, 0);
 	if (pDCTstat->ErrCode == SC_FatalErr) {
 		/* Do nothing goto exitDCTInit; any fatal errors? */
 	} else {
@@ -4359,6 +4383,7 @@ static void mct_initDCT(struct MCTStatStruc *pMCTstat,
 				err_code = pDCTstat->ErrCode;		/* save DCT0 errors */
 				pDCTstat->ErrCode = 0;
 				DCTInit_D(pMCTstat, pDCTstat, 1);
+				DCTFinalInit_D(pMCTstat, pDCTstat, 1);
 				if (pDCTstat->ErrCode == 2)		/* DCT1 is not Running */
 					pDCTstat->ErrCode = err_code;	/* Using DCT0 Error code to update pDCTstat.ErrCode */
 			} else {
diff --git a/src/northbridge/amd/amdmct/mct_ddr3/mct_d.h b/src/northbridge/amd/amdmct/mct_ddr3/mct_d.h
index 8c9da47..7bc392b 100644
--- a/src/northbridge/amd/amdmct/mct_ddr3/mct_d.h
+++ b/src/northbridge/amd/amdmct/mct_ddr3/mct_d.h
@@ -338,7 +338,7 @@ struct DCTStatStruc {		/* A per Node structure*/
 	u8 Node_ID;			/* Node ID of current controller */
 	uint8_t Internal_Node_ID;	/* Internal Node ID of the current controller */
 	uint8_t Dual_Node_Package;	/* 1=Dual node package (G34) */
-	uint8_t stopDCT;		/* Set if the DCT will be stopped */
+	uint8_t stopDCT[2];		/* Set if the DCT will be stopped */
 	u8 ErrCode;			/* Current error condition of Node
 		0= no error
 		1= Variance Error, DCT is running but not in an optimal configuration.
-- 
1.7.9.5

