From 4d83ab44b211bd6c7e0c96e23de9f413f0927875 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Fri, 7 Aug 2015 23:58:28 -0500
Subject: [PATCH 101/143] cpu/amd/family_10h-family_15h: Configure NB register
 2

Change-Id: I55cfc96a197514212b2a4c344d3513396ebc2ad4
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/cpu/amd/family_10h-family_15h/defaults.h |    8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/src/cpu/amd/family_10h-family_15h/defaults.h b/src/cpu/amd/family_10h-family_15h/defaults.h
index 4868c5c..5ab4335 100644
--- a/src/cpu/amd/family_10h-family_15h/defaults.h
+++ b/src/cpu/amd/family_10h-family_15h/defaults.h
@@ -621,6 +621,14 @@ static const struct {
 					   [5] DisPciCfgCpuMstAbtRsp = 1,
 					   [1] SyncFloodOnUsPwDataErr = 1 */
 
+	/* NB Configuration 2 */
+	{ 3, 0x188, AMD_DR_GT_B0, AMD_PTYPE_ALL,
+	  0x00000010, 0x00000010 },	/* EnStpGntOnFlushMaskWakeup = 0x1 */
+
+	/* NB Configuration 2 */
+	{ 3, 0x188, AMD_FAM15_ALL, AMD_PTYPE_ALL,
+	  0x00000200, 0x00000200 },	/* DisL3HiPriFreeListAlloc = 0x1 */
+
 	/* errata 346 - Fam10 C2, C3
 	 *  System software should set F3x188[22] to 1b. */
 	{ 3, 0x188, AMD_DR_Cx, AMD_PTYPE_ALL,
-- 
1.7.9.5

