
1999 10 21 11:02:21 daniel NMMTL_2DLF

Node = TestMagicad:trap_test
Number of Signal Lines =   2
Number of Ground Lines, including top ground plane =   1
Coupling Length =   0.02540 meters
Rise Time =    25.0000 picoseconds
Contour (conductor) segments [cseg] = 45
Ground Plane/Dielectric segments [dseg] = 45
Note: minimum frequency for surface current assumptions is 1309 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal1 , signal1 )=   1.1523595e-10
B( signal1 , signal2 )=  -3.8479849e-12
B( signal2 , signal1 )=  -3.8482377e-12
B( signal2 , signal2 )=   1.1523599e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal1 , signal1 )=   3.8611270e-07
L( signal1 , signal2 )=   1.2893159e-08
L( signal2 , signal1 )=   1.2894004e-08
L( signal2 , signal2 )=   3.8611253e-07

Asymmetry Ratios:

  Asymmetry ratio for inductance matrix:
     0.006558% (max), 0.006558% (average)

  Asymmetry ratio for electrostatic induction matrix:
     0.006571% (max), 0.006571% (average).


Characteristic Impedance (Ohms):
For Signal Line signal1= 57.8846
For Signal Line signal2= 57.8846

Characteristic Impedance Odd/Even (Ohms):
  odd= 55.9829
 even= 59.8509

Effective Dielectric Constant:
For Signal Line signal1= 4
For Signal Line signal2= 4

Propagation Velocity (meters/second):
For Signal Line signal1=   1.4989626e+08
For Signal Line signal2=   1.4989626e+08

Propagation Velocity Odd/Even (meters/second):
  odd= 1.5e+08
 even= 1.5e+08

Propagation Delay (seconds/meter):
For Signal Line signal1=   6.6712807e-09
For Signal Line signal2=   6.6712807e-09

Propagation Delay Odd/Even (seconds/meter):
  odd= 6.66667e-09
 even= 6.66667e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal1 , signal1 )=   1.0763943e+01
Rdc( signal1 , signal2 )=   0.0000000e+00
Rdc( signal2 , signal1 )=   0.0000000e+00
Rdc( signal2 , signal2 )=   1.0763968e+01

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)
FXT( signal1 , signal2 )= 0.00000e+00 = infinite dB

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)
BXT( signal1 , signal2 )= 1.66972e-02 =   -35.54712 dB

NOTE: Cross talk results assume there are no reflections.
