
1999 04 15 15:01:07 daniel NMMTL_2DLF

Node = TestMagicad:coplanar
Number of Signal Lines =   1
Number of Ground Lines, including top ground plane =   2
Coupling Length =   0.02540 meters
Rise Time =    25.0000 picoseconds
Contour (conductor) segments [cseg] = 45
Ground Plane/Dielectric segments [dseg] = 45
Note: minimum frequency for surface current assumptions is 32719 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal2 , signal2 )=   3.3830971e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal2 , signal2 )=   3.2095753e-07

Characteristic Impedance (Ohms):
For Signal Line signal2= 30.8011

Effective Dielectric Constant:
For Signal Line signal2= 9.77247

Propagation Velocity (meters/second):
For Signal Line signal2=   9.5899976e+07

Propagation Delay (seconds/meter):
For Signal Line signal2=   1.0427531e-08

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal2 , signal2 )=   5.7407524e+01

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)

NOTE: Cross talk results assume there are no reflections.
