

		DUMP OF GEOMETRY

cntr_seg=10, pln_seg=10, coupling=0.0254, risetime=1e-09
conductivity=5.8e+07, frequency=1e+08, half min dim=1.5
1 ground planes, top thickness=1, bottom thickness=1

SIGNAL CONDUCTORS:

R Rect2R1 rectangle
	low left = (12,20), up right = (19,23)

R Rect2R0 rectangle
	low left = (0,20), up right = (7,23)


GROUND CONDUCTORS:


DIELECTRICS:

	low left = (-19,20), up right = (38,40)
	constant=4.26, tangent=0

	low left = (-19,0), up right = (38,20)
	constant=4.26, tangent=0


