#----------------------------------
# File:  /users/zahn/lib/bem/tests/test1.xsctn
# Fri Sep 27 07:51:30 DST 2002
#----------------------------------

package require csdl

set _title "Duplicate of test1.xsctn"
set ::Stackup::couplingLength "0.02540 meters"
set ::Stackup::riseTime "25"
set ::Stackup::frequency "1e9"
set ::Stackup::defaultLengthUnits "mils"
set CSEG 45
set DSEG 45

GroundPlane G9 
DielectricLayer D7  \
	 -thickness 10 \
	 -lossTangent 0.012 \
	 -permittivity 4
RectangleConductors Rect8  \
	 -width 18 \
	 -pitch 50 \
	 -conductivity 3e+07siemens/meter \
	 -height 1.4 \
	 -number 2 \
	 -yOffset 0 \
	 -xOffset 0
