
2002 02 25 18:16:37 harff NMMTL_2DLF

Node = abcs:abcs1
Number of Signal Lines =   1
Number of Ground Lines, including top ground plane =   0
Coupling Length =   0.01000 meters
Rise Time =   400.0000 picoseconds
Contour (conductor) segments [cseg] = 200
Ground Plane/Dielectric segments [dseg] = 400
Note: minimum frequency for surface current assumptions is 23841 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal1 , signal1 )=   1.6849763e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal1 , signal1 )=   4.1248322e-07

Characteristic Impedance (Ohms):
For Signal Line signal1= 49.4773

Effective Dielectric Constant:
For Signal Line signal1= 6.25522

Propagation Velocity (meters/second):
For Signal Line signal1=   1.1986695e+08

Propagation Delay (seconds/meter):
For Signal Line signal1=   8.3425830e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal1 , signal1 )=   1.0457516e+02

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)

NOTE: Cross talk results assume there are no reflections.
