
2000 09 13 12:53:42 sommer NMMTL_2DLF

Node = MRL_TFI_bem:9-7-00
Number of Signal Lines =   3
Number of Ground Lines, including top ground plane =   1
Coupling Length =   0.04000 meters
Rise Time =   400.0000 picoseconds
Contour (conductor) segments [cseg] = 200
Ground Plane/Dielectric segments [dseg] = 400
Note: minimum frequency for surface current assumptions is 23841 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal1 , signal1 )=   1.1508786e-10
B( signal1 , signal2 )=  -4.1967520e-13
B( signal1 , signal3 )=  -2.2046738e-16
B( signal2 , signal1 )=  -4.1965541e-13
B( signal2 , signal2 )=   1.1508984e-10
B( signal2 , signal3 )=  -4.1967683e-13
B( signal3 , signal1 )=  -2.1666831e-16
B( signal3 , signal2 )=  -4.1965783e-13
B( signal3 , signal3 )=   1.1508743e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal1 , signal1 )=   3.0894662e-07
L( signal1 , signal2 )=   1.1265915e-09
L( signal1 , signal3 )=   4.7000351e-12
L( signal2 , signal1 )=   1.1265384e-09
L( signal2 , signal2 )=   3.0894546e-07
L( signal2 , signal3 )=   1.1265960e-09
L( signal3 , signal1 )=   4.6894467e-12
L( signal3 , signal2 )=   1.1265415e-09
L( signal3 , signal3 )=   3.0894708e-07

Asymmetry Ratios:

  Asymmetry ratio for inductance matrix:
     0.225282% (max), 0.078277% (average)

**********
  Asymmetry ratio for electrostatic induction matrix:
     1.723186% (max), 0.577476% (average).
  (Note values greater than 1% are a probable indication of too few elements.
  Try adjusting CSEG and DSEG attributes.)
**********

Characteristic Impedance (Ohms):
For Signal Line signal1= 51.8116
For Signal Line signal2= 51.8111
For Signal Line signal3= 51.8117

Effective Dielectric Constant:
For Signal Line signal1= 3.2
For Signal Line signal2= 3.2
For Signal Line signal3= 3.19999

Propagation Velocity (meters/second):
For Signal Line signal1=   1.6758915e+08
For Signal Line signal2=   1.6758915e+08
For Signal Line signal3=   1.6758934e+08

Propagation Delay (seconds/meter):
For Signal Line signal1=   5.9669733e-09
For Signal Line signal2=   5.9669733e-09
For Signal Line signal3=   5.9669665e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal1 , signal1 )=   2.4767671e+02
Rdc( signal1 , signal2 )=   0.0000000e+00
Rdc( signal1 , signal3 )=   0.0000000e+00
Rdc( signal2 , signal1 )=   0.0000000e+00
Rdc( signal2 , signal2 )=   2.4767580e+02
Rdc( signal2 , signal3 )=   0.0000000e+00
Rdc( signal3 , signal1 )=   0.0000000e+00
Rdc( signal3 , signal2 )=   0.0000000e+00
Rdc( signal3 , signal3 )=   2.4767616e+02

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)
FXT( signal1 , signal2 )= -9.51018e-09 =  -160.43623 dB
FXT( signal1 , signal3 )= -3.96418e-06 =  -108.03694 dB
FXT( signal2 , signal3 )= -3.47087e-09 =  -169.19124 dB

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)
BXT( signal1 , signal2 )= 1.82319e-03 =   -54.78337 dB
BXT( signal1 , signal3 )= 4.26536e-06 =  -107.40088 dB
BXT( signal2 , signal3 )= 1.82320e-03 =   -54.78333 dB

NOTE: Cross talk results assume there are no reflections.
