#----------------------------------
# File:  /users/zahn/lib/bem/tests/generic.xsctn
# Fri Sep 27 07:56:54 DST 2002
#----------------------------------

package require csdl

set _title "Duplicate of generic.xsctn"
set ::Stackup::couplingLength "10000"
set ::Stackup::riseTime "20"
set ::Stackup::frequency "1000MHz"
set ::Stackup::defaultLengthUnits "microns"
set CSEG 90
set DSEG 90

GroundPlane G15 
DielectricLayer D13  \
	 -thickness 10.57 \
	 -lossTangent 0.001 \
	 -permittivity 4.1
RectangleConductors grWires  \
	 -width 40 \
	 -pitch 70 \
	 -conductivity 3e+07siemens/meter \
	 -height 4 \
	 -number 2 \
	 -yOffset 0 \
	 -xOffset 0
RectangleConductors Rect15  \
	 -width 10 \
	 -pitch 70 \
	 -conductivity 3e+07siemens/meter \
	 -height 4 \
	 -yOffset 0 \
	 -xOffset 50
DielectricLayer D15  \
	 -thickness 8.3 \
	 -lossTangent 0.001 \
	 -permittivity 4
