#----------------------------------
# File:  /users/zahn/lib/bem/tests/abcs1.xsctn
# Fri Sep 27 08:05:45 DST 2002
#----------------------------------

package require csdl

set _title "Duplicate of abcs1.xsctn"
set ::Stackup::couplingLength "10000um"
set ::Stackup::riseTime "400"
set ::Stackup::frequency "1000MHz"
set ::Stackup::defaultLengthUnits "microns"
set CSEG 20
set DSEG 40

GroundPlane G7 
DielectricLayer D7  \
	 -thickness 50 \
	 -lossTangent 0.1 \
	 -permittivity 10
RectangleConductors Rect4  \
	 -width 45 \
	 -pitch 0 \
	 -conductivity 4.25e7siemens/meter \
	 -height 5 \
	 -yOffset 0 \
	 -xOffset 0
