#----------------------------------
# File:  /sppdg/software/src/tnt/calcCAP/tests/dmy.xsctn
# Thu Oct 10 10:33:28 DST 2002
#----------------------------------

package require csdl

set _title ""
set ::Stackup::couplingLength "0.0"
set ::Stackup::riseTime "0.0"
set ::Stackup::frequency "1e9"
set ::Stackup::defaultLengthUnits "meters"
set CSEG 10
set DSEG 10

GroundPlane GG2 
DielectricLayer D2  \
	 -thickness 20 \
	 -lossTangent 0.014 \
	 -permittivity 4.26
RectangleConductors Rect2  \
	 -width 7 \
	 -pitch 12 \
	 -conductivity 3.0siemens/meter \
	 -height 3 \
	 -number 2 \
	 -yOffset 0 \
	 -xOffset 0
DielectricLayer D4  \
	 -thickness 20 \
	 -lossTangent 0.014 \
	 -permittivity 4.26
