#----------------------------------
# File:  trap_test.xsctn
# $Id: trap_test.xsctn,v 1.2 2004/07/20 17:02:41 techenti Exp $
#----------------------------------

package require csdl

set _title "Trapzoid Conductor Stripline Example"
set ::Stackup::couplingLength "0.02540"
set ::Stackup::riseTime "25"
set ::Stackup::frequency "1e9"
set ::Stackup::defaultLengthUnits "mils"
set CSEG 10
set DSEG 10

GroundPlane G5 
DielectricLayer D3  \
	 -thickness 7.6 \
	 -lossTangent 0.012 \
	 -permittivity 4
TrapezoidConductors Trap6  \
	 -pitch 20 \
	 -conductivity 3.0e+07siemens/meter \
	 -bottomWidth 5.3 \
	 -height 1 \
	 -number 2 \
	 -topWidth 4.3 \
	 -yOffset 0 \
	 -xOffset 0
DielectricLayer D5  \
	 -thickness 10.3 \
	 -lossTangent 0.012 \
	 -permittivity 4
GroundPlane G7 
