#----------------------------------
# File:  /users/zahn/lib/bem/tests/coplanar.xsctn
# Fri Sep 27 07:47:37 DST 2002
#----------------------------------

package require csdl

set _title "Duplicate of coplanar.xsctn"
set ::Stackup::couplingLength "1000mils"
set ::Stackup::riseTime "25"
set ::Stackup::frequency "1000MHz"
set ::Stackup::defaultLengthUnits "mils"
set CSEG 45
set DSEG 45

GroundPlane G3 
DielectricLayer D1  \
	 -thickness 9.8 \
	 -lossTangent 0.0002 \
	 -permittivity 20
RectangleConductors grWires  \
	 -width 4.5 \
	 -pitch 12 \
	 -conductivity 3e+07siemens/meter \
	 -height 0.2 \
	 -number 2 \
	 -yOffset 0 \
	 -xOffset 0
RectangleConductors Rect4  \
	 -width 4.5 \
	 -pitch 12 \
	 -conductivity 3e+07siemens/meter \
	 -height 0.2 \
	 -yOffset 0 \
	 -xOffset 6
