
2002 09 17 09:04:27 zahn NMMTL_2DLF

Node = /users/zahn/em/tests/opal_mediumline:/users/zahn/em/tests/opal_mediumline
Number of Signal Lines  =   1
Number of Ground Planes =   1
Number of Ground Wires  =   0
Coupling Length =   0.04201 meters
Rise Time =    60.0000 picoseconds
Contour (conductor) segments [cseg] = 10
Ground Plane/Dielectric segments [dseg] = 10
Conductivity ::Rect1R0 = 5.9596e+07 siemens/meter
Note: minimum frequency for surface current assumptions is 2636 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( ::Rect1R0 , ::Rect1R0 )=   1.1298402e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( ::Rect1R0 , ::Rect1R0 )=   2.7763409e-07

Characteristic Impedance (Ohms):
For Signal Line ::Rect1R0= 49.571

Effective Dielectric Constant:
For Signal Line ::Rect1R0= 2.82314

Propagation Velocity (meters/second):
For Signal Line ::Rect1R0=   1.7842454e+08

Propagation Delay (seconds/meter):
For Signal Line ::Rect1R0=   5.6046101e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( ::Rect1R0 , ::Rect1R0 )=   3.0598247e+00

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)

NOTE: Cross talk results assume there are no reflections.
