
2002 06 11 14:45:51 daniel NMMTL_2DLF

Node = TestMagicad:generic
Number of Signal Lines =   1
Number of Ground Lines, including top ground plane =   2
Coupling Length =   0.01000 meters
Rise Time =    20.0000 picoseconds
Contour (conductor) segments [cseg] = 90
Ground Plane/Dielectric segments [dseg] = 90
Note: minimum frequency for surface current assumptions is 52772 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal2 , signal2 )=   1.3125821e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal2 , signal2 )=   3.0472359e-07

Characteristic Impedance (Ohms):
For Signal Line signal2= 48.1826

Effective Dielectric Constant:
For Signal Line signal2= 3.59977

Propagation Velocity (meters/second):
For Signal Line signal2=   1.5800952e+08

Propagation Delay (seconds/meter):
For Signal Line signal2=   6.3287326e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal2 , signal2 )=   8.3333337e+02

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)

NOTE: Cross talk results assume there are no reflections.
