
2001 03 12 14:40:01 zahn NMMTL_2DLF

Node = test:opal2_mediumline
Number of Signal Lines =   1
Number of Ground Lines, including top ground plane =   0
Coupling Length =   0.04201 meters
Rise Time =    60.0000 picoseconds
Contour (conductor) segments [cseg] = 10
Ground Plane/Dielectric segments [dseg] = 15
Note: minimum frequency for surface current assumptions is 2636 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal1 , signal1 )=   1.0285617e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal1 , signal1 )=   2.7763409e-07

Characteristic Impedance (Ohms):
For Signal Line signal1= 51.9543

Effective Dielectric Constant:
For Signal Line signal1= 2.57007

Propagation Velocity (meters/second):
For Signal Line signal1=   1.8700272e+08

Propagation Delay (seconds/meter):
For Signal Line signal1=   5.3475158e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal1 , signal1 )=   3.0601327e+00

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)

NOTE: Cross talk results assume there are no reflections.
