#----------------------------------
# File:  /users/zahn/lib/bem/tests/opal2_mediumline.xsctn
# Wed Sep 25 13:20:05 DST 2002
#----------------------------------

package require csdl

set _title ""
set ::Stackup::couplingLength "1654mils"
set ::Stackup::riseTime "60"
set ::Stackup::frequency "9000MHz"
set ::Stackup::defaultLengthUnits "mils"
set CSEG 10
set DSEG 15

GroundPlane G14 
DielectricLayer D16  \
	 -thickness 8 \
	 -lossTangent 0.003 \
	 -permittivity 3.38
RectangleConductors Rect11  \
	 -width 17 \
	 -pitch 0 \
	 -conductivity 5.959e7siemens/meter \
	 -height 0.5 \
	 -yOffset 0 \
	 -xOffset 17
