
1999 03 25 10:35:44 daniel NMMTL_2DLF

Node = TestMagicad:test1
Number of Signal Lines =   2
Number of Ground Lines, including top ground plane =   0
Coupling Length =   0.02540 meters
Rise Time =    25.0000 picoseconds
Contour (conductor) segments [cseg] = 45
Ground Plane/Dielectric segments [dseg] = 45
Note: minimum frequency for surface current assumptions is 668 MHz.
Mutual and Self Electrostatic Induction:
B(Active Signal , Passive Signal) Farads/Meter
B( signal1 , signal1 )=   1.1014983e-10
B( signal1 , signal2 )=  -1.8015087e-12
B( signal2 , signal1 )=  -1.8149999e-12
B( signal2 , signal2 )=   1.1015717e-10

Mutual and Self Inductance:
L(Active Signal , Passive Signal) Henrys/Meter
L( signal1 , signal1 )=   2.9683324e-07
L( signal1 , signal2 )=   1.7756125e-08
L( signal2 , signal1 )=   1.7754976e-08
L( signal2 , signal2 )=   2.9683378e-07

Asymmetry Ratios:

  Asymmetry ratio for inductance matrix:
     0.006473% (max), 0.006473% (average)

  Asymmetry ratio for electrostatic induction matrix:
     0.748881% (max), 0.748881% (average).


Characteristic Impedance (Ohms):
For Signal Line signal1= 51.9116
For Signal Line signal2= 51.9099

Characteristic Impedance Odd/Even (Ohms):
  odd= 49.9284
 even= 53.8841

Effective Dielectric Constant:
For Signal Line signal1= 2.93212
For Signal Line signal2= 2.93232

Propagation Velocity (meters/second):
For Signal Line signal1=   1.7507725e+08
For Signal Line signal2=   1.7507125e+08

Propagation Velocity Odd/Even (meters/second):
  odd= 1.78905e+08
 even= 1.71284e+08

Propagation Delay (seconds/meter):
For Signal Line signal1=   5.7117644e-09
For Signal Line signal2=   5.7119602e-09

Propagation Delay Odd/Even (seconds/meter):
  odd= 5.58955e-09
 even= 5.83826e-09

Rdc:
Rdc(Active Signal , Passive Signal) Ohms/Meter
Rdc( signal1 , signal1 )=   2.0502687e+00
Rdc( signal1 , signal2 )=   0.0000000e+00
Rdc( signal2 , signal1 )=   0.0000000e+00
Rdc( signal2 , signal2 )=   2.0502687e+00

Far-End (Forward) Cross Talk:
FXT(Active Signal, Passive Signal)
FXT( signal1 , signal2 )= -1.25888e-01 =   -18.00032 dB

Near-End (Backward) Cross Talk:
BXT(Active Signal, Passive Signal)
BXT( signal1 , signal2 )= 1.90729e-02 =   -34.39167 dB

NOTE: Cross talk results assume there are no reflections.
