#----------------------------------
# File:  example-microstrip-2.xsctn
# Thu Jul 29 8:06:45 AM Central Daylight Time 2004
#----------------------------------

package require csdl

set _title "Example Two Conductor Microstrip"
set ::Stackup::couplingLength "2.54e-006"
set ::Stackup::riseTime "250"
set ::Stackup::frequency "1e9"
set ::Stackup::defaultLengthUnits "mils"
set CSEG 10
set DSEG 10

GroundPlane ground  \
	 -thickness 3 \
	 -yOffset 0.0 \
	 -xOffset 0.0
DielectricLayer fr4  \
	 -thickness 50 \
	 -lossTangent 0.0 \
	 -permittivity 4.7 \
	 -permeability 1.0 \
	 -yOffset 0.0 \
	 -xOffset 0.0
RectangleConductors c1  \
	 -width 12 \
	 -pitch 20 \
	 -conductivity 5.0e7S/m \
	 -height 3 \
	 -number 2 \
	 -yOffset 0 \
	 -xOffset 0
