#----------------------------------
# File:  /users/zahn/em/tests/opal_mediumline.xsctn
# Wed Feb 13 14:45:48 CST 2002
#----------------------------------

package require csdl

set _title ""
set ::Stackup::couplingLength "1.65400inches"
set ::Stackup::riseTime "60"
set ::Stackup::frequency "1e9"
set ::Stackup::defaultLengthUnits "mils"
set CSEG 10
set DSEG 10

GroundPlane G1 
DielectricLayer D1  \
	 -thickness 8 \
	 -lossTangent 0.003 \
	 -permittivity 3.8
RectangleConductors Rect1  \
	 -width 17 \
	 -pitch 0 \
	 -conductivity "5.9596e7siemens/meter" \
	 -height 0.5 \
	 -yOffset 0 \
	 -xOffset 0
DielectricLayer Air  \
	 -thickness 8 \
	 -lossTangent 0 \
	 -permittivity 1
