onerror {resume}
quietly WaveActivateNextPane {} 0
add wave -radix hex -position insertpoint  \
sim:/dac_tb/tpg_inst/clk \
sim:/dac_tb/tpg_inst/res_n \
sim:/dac_tb/tpg_inst/pix_rd \
sim:/dac_tb/tpg_inst/pix_data \
sim:/dac_tb/tpg_inst/x \
sim:/dac_tb/tpg_inst/y
add wave -radix hex -position insertpoint  \
sim:/dac_tb/dac_inst/vga_r \
sim:/dac_tb/dac_inst/vga_g \
sim:/dac_tb/dac_inst/vga_b \
sim:/dac_tb/dac_inst/vga_clk \
sim:/dac_tb/dac_inst/vga_sync_n \
sim:/dac_tb/dac_inst/vga_blank_n \
sim:/dac_tb/dac_inst/state \
sim:/dac_tb/dac_inst/state_next \
sim:/dac_tb/dac_inst/fsm_data \
sim:/dac_tb/dac_inst/fsm_data_next \
sim:/dac_tb/dac_inst/TIME_SCANLINE_US \
sim:/dac_tb/dac_inst/TIME_BROAD_SYNC_START_US \
sim:/dac_tb/dac_inst/TIME_BROAD_SYNC_END_US \
sim:/dac_tb/dac_inst/TIME_SHORT_SYNC_START_US \
sim:/dac_tb/dac_inst/TIME_SHORT_SYNC_END_US \
sim:/dac_tb/dac_inst/TIME_H_SYNC_US \
sim:/dac_tb/dac_inst/TIME_BACK_PORCH_US \
sim:/dac_tb/dac_inst/TIME_FRONT_PORCH_US \
sim:/dac_tb/dac_inst/TIME_DISPLAY_AREA_US \
sim:/dac_tb/dac_inst/CYCLES_BROAD_SYNC_START \
sim:/dac_tb/dac_inst/CYCLES_BROAD_SYNC_END \
sim:/dac_tb/dac_inst/CYCLES_SHORT_SYNC_START \
sim:/dac_tb/dac_inst/CYCLES_SHORT_SYNC_END \
sim:/dac_tb/dac_inst/CYCLES_H_SYNC \
sim:/dac_tb/dac_inst/CYCLES_BACK_PORCH \
sim:/dac_tb/dac_inst/CYCLES_DISPLAY_AREA \
sim:/dac_tb/dac_inst/CYCLES_FRONT_PORCH \
sim:/dac_tb/dac_inst/LINES_BROAD_SYNC \
sim:/dac_tb/dac_inst/LINES_SHORT_SYNC \
sim:/dac_tb/dac_inst/LINES_DISPLAY_INACTIVE_START \
sim:/dac_tb/dac_inst/LINES_DISPLAY_ACTIVE \
sim:/dac_tb/dac_inst/LINES_DISPLAY_INACTIVE_END \
sim:/dac_tb/dac_inst/LINES_DISPLAY_TOTAL \
sim:/dac_tb/dac_inst/MAX_CYCLES \
sim:/dac_tb/dac_inst/MAX_LINES \
sim:/dac_tb/dac_inst/INITIAL_STATE \
sim:/dac_tb/dac_inst/INITIAL_FSM_DATA
update
