From 3003a569ad63a35922984a8c7d1f079cc5cbd960 Mon Sep 17 00:00:00 2001
From: Paul Kocialkowski <contact@paulk.fr>
Date: Mon, 10 Aug 2015 20:30:14 +0200
Subject: [PATCH 1/4] fdt: nonvolatile-context-storage report to mkbp for EC NV
 storage

This allows old versions of crossystem to detect that it should use mosys to
access NV storage in case it is stored on the EC.

Change-Id: I78ed64c2002727432def0e132f572a1c5173fa5e
Signed-off-by: Paul Kocialkowski <contact@paulk.fr>
---
 src/vboot/crossystem/fdt.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/src/vboot/crossystem/fdt.c b/src/vboot/crossystem/fdt.c
index c0b10c0..5cba178 100644
--- a/src/vboot/crossystem/fdt.c
+++ b/src/vboot/crossystem/fdt.c
@@ -51,7 +51,7 @@ static int install_crossystem_data(DeviceTreeFixup *fixup, DeviceTree *tree)
 		dt_add_string_prop(node, "nonvolatile-context-storage","nvram");
 	} else if (CONFIG_NV_STORAGE_CROS_EC) {
 		dt_add_string_prop(node,
-				"nonvolatile-context-storage", "cros-ec");
+				"nonvolatile-context-storage", "mkbp");
 	} else if (CONFIG_NV_STORAGE_DISK) {
 		dt_add_string_prop(node, "nonvolatile-context-storage", "disk");
 		dt_add_u32_prop(node, "nonvolatile-context-lba",
-- 
2.10.2

