Fix build against xorg-server >= 1.20.

Patch taken from upstream:
https://cgit.freedesktop.org/xorg/driver/xf86-video-savage/commit/?id=0ece556daa8a88771b669d8104396abd9166d2d0

diff --git a/src/savage_driver.c b/src/savage_driver.c
index 58a294d..3cda923 100644
--- a/src/savage_driver.c
+++ b/src/savage_driver.c
@@ -2034,8 +2034,6 @@ static Bool SavagePreInit(ScrnInfoPtr pScrn, int flags)
     xf86DrvMsg(pScrn->scrnIndex, X_PROBED, "Detected current MCLK value of %1.3f MHz\n",
 	       mclk / 1000.0);
 
-    pScrn->maxHValue = 2048 << 3;	/* 11 bits of h_total 8-pixel units */
-    pScrn->maxVValue = 2048;		/* 11 bits of v_total */
     pScrn->virtualX = pScrn->display->virtualX;
     pScrn->virtualY = pScrn->display->virtualY;
 
@@ -3637,6 +3635,14 @@ static ModeStatus SavageValidMode(SCRN_ARG_TYPE arg, DisplayModePtr pMode,
        (pMode->VDisplay > psav->PanelY)))
 	    return MODE_PANEL;
 
+    /* 11 bits of h_total 8-pixel units */
+    if (pMode->HTotal > (2048 << 3))
+	return MODE_BAD_HVALUE;
+
+    /* 11 bits of v_total */
+    if (pMode->VTotal > 2048)
+	return MODE_BAD_VVALUE;
+
     if (psav->UseBIOS) {
 	refresh = SavageGetRefresh(pMode);
         return (SavageMatchBiosMode(pScrn,pMode->HDisplay,
