[options]

version: 1.343
file_version: 1.332
project_name: "test"
full_library_folder: "c:\program files\freepcb\lib"
CAM_folder: ""
ses_file_path: ""
SMT_connect_copper: "0"
dsn_flags: "0"
dsn_bounds_poly: "0"
dsn_signals_poly: "0"
autosave_interval: 0
netlist_import_flags: 451
units: MIL

visible_grid_spacing: 5080000.000000
  visible_grid_item: 100MIL
  visible_grid_item: 125MIL
  visible_grid_item: 200MIL
  visible_grid_item: 250MIL
  visible_grid_item: 400MIL
  visible_grid_item: 500MIL
  visible_grid_item: 1000MIL
  visible_grid_item: 1MM
  visible_grid_item: 2MM
  visible_grid_item: 2.5MM
  visible_grid_item: 4MM
  visible_grid_item: 5MM
  visible_grid_item: 10MM
  visible_grid_item: 20MM
  visible_grid_item: 25MM
  visible_grid_item: 40MM
  visible_grid_item: 50MM
  visible_grid_item: 100MM

placement_grid_spacing: 2540000.000000
  placement_grid_item: 10MIL
  placement_grid_item: 20MIL
  placement_grid_item: 25MIL
  placement_grid_item: 40MIL
  placement_grid_item: 50MIL
  placement_grid_item: 100MIL
  placement_grid_item: 200MIL
  placement_grid_item: 250MIL
  placement_grid_item: 400MIL
  placement_grid_item: 500MIL
  placement_grid_item: 1000MIL
  placement_grid_item: 0.1MM
  placement_grid_item: 0.2MM
  placement_grid_item: 0.25MM
  placement_grid_item: 0.4MM
  placement_grid_item: 0.5MM
  placement_grid_item: 1MM
  placement_grid_item: 2MM
  placement_grid_item: 2.5MM
  placement_grid_item: 4MM
  placement_grid_item: 5MM
  placement_grid_item: 10MM

routing_grid_spacing: 508000.000000
  routing_grid_item: 1MIL
  routing_grid_item: 2MIL
  routing_grid_item: 2.5MIL
  routing_grid_item: 3.33330709MIL
  routing_grid_item: 4MIL
  routing_grid_item: 5MIL
  routing_grid_item: 6.66665354MIL
  routing_grid_item: 10MIL
  routing_grid_item: 12.5MIL
  routing_grid_item: 16.66665354MIL
  routing_grid_item: 20MIL
  routing_grid_item: 25MIL
  routing_grid_item: 40MIL
  routing_grid_item: 50MIL
  routing_grid_item: 0.01MM
  routing_grid_item: 0.02MM
  routing_grid_item: 0.04MM
  routing_grid_item: 0.05MM
  routing_grid_item: 0.1MM
  routing_grid_item: 0.2MM
  routing_grid_item: 0.25MM
  routing_grid_item: 0.4MM
  routing_grid_item: 0.5MM
  routing_grid_item: 1MM
  routing_grid_item: 2MM
  routing_grid_item: 2.5MM
  routing_grid_item: 4MM
  routing_grid_item: 5MM
  routing_grid_item: 10MM

snap_angle: 45

fp_visible_grid_spacing: 5080000.000000
  fp_visible_grid_item: 100MIL
  fp_visible_grid_item: 125MIL
  fp_visible_grid_item: 200MIL
  fp_visible_grid_item: 250MIL
  fp_visible_grid_item: 400MIL
  fp_visible_grid_item: 500MIL
  fp_visible_grid_item: 1000MIL
  fp_visible_grid_item: 1MM
  fp_visible_grid_item: 2MM
  fp_visible_grid_item: 2.5MM
  fp_visible_grid_item: 4MM
  fp_visible_grid_item: 5MM
  fp_visible_grid_item: 10MM
  fp_visible_grid_item: 20MM
  fp_visible_grid_item: 25MM
  fp_visible_grid_item: 40MM
  fp_visible_grid_item: 50MM
  fp_visible_grid_item: 100MM

fp_placement_grid_spacing: 2540000.000000
  fp_placement_grid_item: 10MIL
  fp_placement_grid_item: 20MIL
  fp_placement_grid_item: 25MIL
  fp_placement_grid_item: 40MIL
  fp_placement_grid_item: 50MIL
  fp_placement_grid_item: 100MIL
  fp_placement_grid_item: 200MIL
  fp_placement_grid_item: 250MIL
  fp_placement_grid_item: 400MIL
  fp_placement_grid_item: 500MIL
  fp_placement_grid_item: 1000MIL
  fp_placement_grid_item: 0.1MM
  fp_placement_grid_item: 0.2MM
  fp_placement_grid_item: 0.25MM
  fp_placement_grid_item: 0.4MM
  fp_placement_grid_item: 0.5MM
  fp_placement_grid_item: 1MM
  fp_placement_grid_item: 2MM
  fp_placement_grid_item: 2.5MM
  fp_placement_grid_item: 4MM
  fp_placement_grid_item: 5MM
  fp_placement_grid_item: 10MM

fp_snap_angle: 45

fill_clearance: 254000
mask_clearance: 203200
thermal_width: 254000
min_silkscreen_width: 127000
board_outline_width: 127000
hole_clearance: 381000
pilot_diameter: 254000
annular_ring_for_pins: 177800
annular_ring_for_vias: 127000
shrink_paste_mask: 0
cam_flags: 1
cam_layers: 15732735
cam_drill_file: 1
cam_units: 2
cam_n_x: 1
cam_n_y: 1
cam_space_x: 0
cam_space_y: 0

report_options: 0
drc_check_unrouted: 0
drc_trace_width: 254000
drc_pad_pad: 254000
drc_pad_trace: 254000
drc_trace_trace: 254000
drc_hole_copper: 381000
drc_annular_ring_pins: 177800
drc_annular_ring_vias: 127000
drc_board_edge_copper: 635000
drc_board_edge_hole: 635000
drc_hole_hole: 635000
drc_copper_copper: 254000

default_trace_width: 254000
default_via_pad_width: 711200
default_via_hole_width: 355600
n_width_menu: 7
  width_menu_item: 1 152400 711200 355600
  width_menu_item: 2 203200 711200 355600
  width_menu_item: 3 254000 711200 355600
  width_menu_item: 4 304800 711200 355600
  width_menu_item: 5 381000 711200 355600
  width_menu_item: 6 508000 711200 355600
  width_menu_item: 7 635000 711200 355600

n_copper_layers: 2
  layer_info: "selection" 0 255 255 255 1
  layer_info: "background" 1 0 0 0 1
  layer_info: "visible grid" 2 255 255 255 1
  layer_info: "highlight" 3 255 255 255 1
  layer_info: "DRC error" 4 255 128 64 1
  layer_info: "board outline" 5 0 0 255 1
  layer_info: "rat line" 6 255 0 255 1
  layer_info: "top silk" 7 255 255 0 1
  layer_info: "bottom silk" 8 255 192 192 1
  layer_info: "top sm cutout" 9 160 160 160 1
  layer_info: "bot sm cutout" 10 95 95 95 1
  layer_info: "thru pad" 11 0 0 255 1
  layer_info: "top copper" 12 0 255 0 1
  layer_info: "bottom copper" 13 255 0 0 1

[footprints]

name: "1X2HDR-100"
author: "Ivex"
source: "PRINTED CIRCUIT DESIGN METHODS PAGE 411"
  units: MIL
  sel_rect: -33 -33 33 133
  ref_text: 50 0 160 0 7
  centroid: 0 0 50
  n_pins: 2
    pin: "1" 28 0 0 0
      top_pad: 2 50 25 25 0
      inner_pad: 1 50 25 25 0
      bottom_pad: 2 50 25 25 0
    pin: "2" 28 0 100 0
      top_pad: 1 50 25 25 0
      inner_pad: 1 50 25 25 0
      bottom_pad: 1 50 25 25 0

name: "SS14MDP2"
author: "Jeff Connelly"
source: "http://www.nkkswitches.com/pdf/SSnonilluminated.pdf"
description: "NKK SP3T Switch"
  units: MIL
  sel_rect: -15 -15 215 715
  ref_text: 100 0 800 0 10
  centroid: -842150451 -33155.529528 -33155.529528
  outline_polyline: 10 0 0
    next_corner: 200 0 0
    next_corner: 200 700 0
    next_corner: 0 700 0
    close_polyline: 0
  n_pins: 4
    pin: "1" 45 100 100 0
      top_pad: 1 75 0 0 0
      inner_pad: 0 75 0 0 0
      bottom_pad: 1 75 0 0 0
    pin: "2" 45 100 200 0
      top_pad: 1 75 0 0 0
      inner_pad: 0 75 0 0 0
      bottom_pad: 1 75 0 0 0
    pin: "3" 45 100 300 0
      top_pad: 1 75 0 0 0
      inner_pad: 0 75 0 0 0
      bottom_pad: 1 75 0 0 0
    pin: "4" 45 100 500 0
      top_pad: 1 75 0 0 0
      inner_pad: 0 75 0 0 0
      bottom_pad: 1 75 0 0 0

[board]

[solder_mask_cutouts]


[parts]

part: X$Xtrit_i$XX1
  ref_text: 2540000 254000 0 0 20320000
  package: "SS14MDP2"
  shape: "SS14MDP2"
  pos: 55880000 38100000 0 0 0

part: V$Xpower$Vdd
  ref_text: 1270000 177800 0 0 4064000
  package: "1X2HDR-100"
  shape: "1X2HDR-100"
  pos: 78740000 48260000 0 180 0

part: V$Xpower$Vss
  ref_text: 1270000 177800 0 0 4064000
  package: "1X2HDR-100"
  shape: "1X2HDR-100"
  pos: 78740000 40640000 0 180 0

part: X$Xtrit_0$XX1
  ref_text: 2540000 254000 0 0 20320000
  package: "SS14MDP2"
  shape: "SS14MDP2"
  pos: -9779000 37973000 0 0 0

part: X$Xtrit_1$XX1
  ref_text: 2540000 254000 0 0 20320000
  package: "SS14MDP2"
  shape: "SS14MDP2"
  pos: 22860000 38100000 0 0 0

[nets]

net: "TRIT_i" 1 0 0 0 0 0 1
  pin: 1 X$Xtrit_i$XX1.4

net: "$G_Vss" 4 3 0 0 0 0 1
  pin: 1 X$Xtrit_i$XX1.1
  pin: 2 V$Xpower$Vss.2
  pin: 3 X$Xtrit_0$XX1.1
  pin: 4 X$Xtrit_1$XX1.1
  connect: 1 1 0 2 0
    vtx: 1 78740000 38100000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 60960000 38100000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 58420000 40640000 11 0 0 0 0
  connect: 2 3 2 3 0
    vtx: 1 25400000 40640000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 25400000 40640000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 -7112000 40640000 0 0 0 0 0
    seg: 3 12 254000 0 0
    vtx: 4 -7239000 40513000 11 0 0 0 0
  connect: 3 3 0 2 0
    vtx: 1 25400000 40640000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 57912000 40640000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 58420000 40640000 11 0 0 0 0

net: "$G_Vdd" 4 3 0 0 0 0 1
  pin: 1 X$Xtrit_i$XX1.3
  pin: 2 V$Xpower$Vdd.1
  pin: 3 X$Xtrit_0$XX1.3
  pin: 4 X$Xtrit_1$XX1.3
  connect: 1 1 0 3 0
    vtx: 1 78740000 48260000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 78232000 48260000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 60960000 48260000 0 0 0 0 0
    seg: 3 12 254000 0 0
    vtx: 4 58420000 45720000 11 0 0 0 0
  connect: 2 3 2 3 0
    vtx: 1 25400000 45720000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 25908000 45720000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 25781000 45593000 0 0 0 0 0
    seg: 3 12 254000 0 0
    vtx: 4 -7239000 45593000 11 0 0 0 0
  connect: 3 3 0 2 0
    vtx: 1 25400000 45720000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 58928000 45720000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 58420000 45720000 11 0 0 0 0

net: "TRIT_0" 1 0 0 0 0 0 1
  pin: 1 X$Xtrit_0$XX1.4

net: "0" 5 4 0 0 0 0 1
  pin: 1 X$Xtrit_i$XX1.2
  pin: 2 V$Xpower$Vdd.2
  pin: 3 V$Xpower$Vss.1
  pin: 4 X$Xtrit_0$XX1.2
  pin: 5 X$Xtrit_1$XX1.2
  connect: 1 2 1 3 0
    vtx: 1 78740000 40640000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 81280000 40640000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 81280000 45720000 0 0 0 0 0
    seg: 3 12 254000 0 0
    vtx: 4 78740000 45720000 11 0 0 0 0
  connect: 2 2 0 4 0
    vtx: 1 78740000 40640000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 64008000 40640000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 61976000 40640000 0 0 0 0 0
    seg: 3 12 254000 0 0
    vtx: 4 58928000 43688000 0 0 0 0 0
    seg: 4 12 254000 0 0
    vtx: 5 58420000 43180000 11 0 0 0 0
  connect: 3 4 3 3 0
    vtx: 1 25400000 43180000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 25908000 43688000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 25273000 43053000 0 0 0 0 0
    seg: 3 12 254000 0 0
    vtx: 4 -7239000 43053000 11 0 0 0 0
  connect: 4 4 0 2 0
    vtx: 1 25400000 43180000 11 0 0 0 0
    seg: 1 12 254000 0 0
    vtx: 2 57912000 43180000 0 0 0 0 0
    seg: 2 12 254000 0 0
    vtx: 3 58420000 43180000 11 0 0 0 0

net: "TRIT_1" 1 0 0 0 0 0 1
  pin: 1 X$Xtrit_1$XX1.4

[texts]

[end]
