From 99b8fb271fd244d8e349ca956819c7e1b3420d80 Mon Sep 17 00:00:00 2001
From: Arthur Heymans <arthur@aheymans.xyz>
Date: Mon, 8 Aug 2016 21:51:34 +0200
Subject: [PATCH] hardcode use on intel integrated graphic device on t400

Change-Id: I2ff2d93b024866063715d26aedf510a9753a5445
---
 src/mainboard/lenovo/t400/romstage.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/src/mainboard/lenovo/t400/romstage.c b/src/mainboard/lenovo/t400/romstage.c
index 147131f..1316d69 100644
--- a/src/mainboard/lenovo/t400/romstage.c
+++ b/src/mainboard/lenovo/t400/romstage.c
@@ -208,7 +208,8 @@ void main(unsigned long bist)
 	default_southbridge_gpio_setup();
 
 	uint8_t hybrid_graphics_mode = HYBRID_GRAPHICS_INTEGRATED_ONLY;
-	get_option(&hybrid_graphics_mode, "hybrid_graphics_mode");
+	/* hardcode use of integrated graphic device for libreboot */
+	/* get_option(&hybrid_graphics_mode, "hybrid_graphics_mode"); */
 
 	/* Set up hybrid graphics */
 	hybrid_graphics_set_up_gpio();
-- 
2.9.2

