From f7c7c25e274b79a7c8e62250fa9bc49f81bd4456 Mon Sep 17 00:00:00 2001
From: Patrick Rudolph <patrick.rudolph@9elements.com>
Date: Mon, 7 Dec 2020 08:41:23 +0100
Subject: [PATCH 16/26] usbtrans: Set default maximum packet size

Set the maximum packet size to 512 for SuperSpeed devices.

Signed-off-by: Patrick Rudolph <patrick.rudolph@9elements.com>
---
 grub-core/bus/usb/usbtrans.c | 6 +++++-
 1 file changed, 5 insertions(+), 1 deletion(-)

diff --git a/grub-core/bus/usb/usbtrans.c b/grub-core/bus/usb/usbtrans.c
index c5680b33a..c1080bb33 100644
--- a/grub-core/bus/usb/usbtrans.c
+++ b/grub-core/bus/usb/usbtrans.c
@@ -128,8 +128,12 @@ grub_usb_control_msg (grub_usb_device_t dev,
   setupdata_addr = grub_dma_get_phys (setupdata_chunk);
 
   /* Determine the maximum packet size.  */
-  if (dev->descdev.maxsize0)
+  if (dev->descdev.maxsize0 && dev->speed != GRUB_USB_SPEED_SUPER)
     max = dev->descdev.maxsize0;
+  else if (dev->descdev.maxsize0 && dev->speed == GRUB_USB_SPEED_SUPER)
+    max = 1UL << dev->descdev.maxsize0;
+  else if (dev->speed == GRUB_USB_SPEED_SUPER)
+    max = 512;
   else
     max = 64;
 
-- 
2.39.5

